; /*****************************************************************************
; ** COPYRIGHT (C) 2008-2009 Mellanox                                        **
; ****************************************************************************/

[version]
;Layoutfile parameter is reserved for internal Microsoft use only
;LayoutFile = layout.inf
Signature   = "$Chicago$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Mellanox%
Compatible  = 1
DriverVer = 04/25/2018,5.50.14643.0
CatalogFile=mlx4eth63.cat

[Manufacturer]
%Mellanox%     = Mellanox,ntamd64.6.3

; Mellanox CX Based PCI VPI Adapter

[Mellanox.ntamd64.6.3]
; DisplayName           Section       DeviceID
; -----------           -------       --------
%mlx4eth63_CX.DeviceDesc%   = mlx4eth63_CX2.ndi,   MLX4\ConnectX_Eth 	 ; Mellanox ConnectX Ethernet Adapter
%mlx4eth63_CX2.DeviceDesc%  = mlx4eth63_CX2.ndi,   MLX4\ConnectX-2_Eth   ; Mellanox ConnectX Ethernet Adapter
%mlx4eth63_CX3.DeviceDesc%  = mlx4eth63_CX3.ndi,   MLX4\ConnectX-3_Eth   								; Mellanox ConnectX-3 Ethernet Adapter
%mlx4eth63_CX3Pro.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,   MLX4\ConnectX-3Pro_Eth   						; Mellanox ConnectX-3 Pro Ethernet Adapter
%mlx4eth63_vCX3.DeviceDesc%  = mlx4eth63_vCX3.ndi,   MLX4\ConnectX-3_vEth   								; Mellanox ConnectX-3 Virtual Function Ethernet Adapter
%mlx4eth63_vCX3.DeviceDesc%  = mlx4eth63_vCX3_NW.ndi,   MLX4\ConnectX-3_vEth_NW   						; Mellanox ConnectX-3 Virtual Function Ethernet Adapter

;;;;; cards of other companies

; HP Maze
%mlx4eth63_CX3Pro.801f.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&801f103c	                     ; Ethernet name for CX3 Pro
%mlx4eth63_vCX3.801f.DeviceDesc%  = mlx4eth63_vCX3.ndi,  MLX4\ConnectX-3_vEth&801f103c	                     	; Ethernet name for CX3 in VM
%mlx4eth63_vCX3.801f.DeviceDesc%  = mlx4eth63_vCX3_NW.ndi,  MLX4\ConnectX-3_vEth_NW&801f103c	               	; Ethernet name for CX3 in VM over non Windows

; HP Mesa
%mlx4eth63_CX3Pro.8020.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&8020103c	                     ; Ethernet name for CX3 Pro
%mlx4eth63_vCX3.8020.DeviceDesc%  = mlx4eth63_vCX3.ndi,  MLX4\ConnectX-3_vEth&8020103c					; Ethernet name for CX3 in VM
%mlx4eth63_vCX3.8020.DeviceDesc%  = mlx4eth63_vCX3_NW.ndi,  MLX4\ConnectX-3_vEth_NW&8020103c			; Ethernet name for CX3 in VM over non Windows

; HP Attitash CX3
%mlx4eth63_CX3.18cd.DeviceDesc%  = mlx4eth63_CX3.ndi,  MLX4\ConnectX-3_Eth&18cd103c	                     		; Ethernet name for CX3
%mlx4eth63_vCX3.18cd.DeviceDesc%  = mlx4eth63_CX3.ndi,  MLX4\ConnectX-3_vEth&18cd103c	                     	; Ethernet name for CX3 in VM
%mlx4eth63_vCX3.18cd.DeviceDesc%  = mlx4eth63_CX3.ndi,  MLX4\ConnectX-3_vEth_NW&18cd103c	                 	; Ethernet name for CX3 in VM over non Windows

; HP Attitash CX3 PRO
%mlx4eth63_CX3Pro.22f1.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&22f1103c	                     ; Ethernet name for CX3 Pro
%mlx4eth63_vCX3Pro.22f1.DeviceDesc%  = mlx4eth63_vCX3Pro.ndi,  MLX4\ConnectX-3_vEth&22f1103c	              	; Ethernet name for CX3 in VM
%mlx4eth63_vCX3Pro.22f1.DeviceDesc%  = mlx4eth63_vCX3Pro_NW.ndi,  MLX4\ConnectX-3_vEth_NW&22f1103c	            ; Ethernet name for CX3 in VM over non Windows

; HP Attitash CX3 PRO
%mlx4eth63_CX3Pro.22f2.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&22f2103c	                     ; Ethernet name for CX3 Pro
%mlx4eth63_vCX3Pro.22f2.DeviceDesc%  = mlx4eth63_vCX3Pro.ndi,  MLX4\ConnectX-3_vEth&22f2103c	              	; Ethernet name for CX3 in VM
%mlx4eth63_vCX3Pro.22f2.DeviceDesc%  = mlx4eth63_vCX3Pro_NW.ndi,  MLX4\ConnectX-3_vEth_NW&22f2103c	            ; Ethernet name for CX3 in VM over non Windows

; HP Attitash CX3 PRO
%mlx4eth63_CX3Pro.22f3.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&22f3103c	                     ; Ethernet name for CX3 Pro
%mlx4eth63_vCX3Pro.22f3.DeviceDesc%  = mlx4eth63_vCX3Pro.ndi,  MLX4\ConnectX-3_vEth&22f3103c	              	; Ethernet name for CX3 in VM
%mlx4eth63_vCX3Pro.22f3.DeviceDesc%  = mlx4eth63_vCX3Pro_NW.ndi,  MLX4\ConnectX-3_vEth_NW&22f3103c	            ; Ethernet name for CX3 in VM over non Windows

; HP Attitash CX3 PRO
%mlx4eth63_CX3Pro.22f4.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&22f4103c	                     ; Ethernet name for CX3 Pro
%mlx4eth63_vCX3Pro.22f4.DeviceDesc%  = mlx4eth63_vCX3Pro.ndi,  MLX4\ConnectX-3_vEth&22f4103c	              	; Ethernet name for CX3 in VM
%mlx4eth63_vCX3Pro.22f4.DeviceDesc%  = mlx4eth63_vCX3Pro_NW.ndi,  MLX4\ConnectX-3_vEth_NW&22f4103c	              	; Ethernet name for CX3 in VM over non Windows

; HP Attitash CX3 PRO
%mlx4eth63_CX3Pro.22f5.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&22f5103c	                     ; Ethernet name for CX3 Pro
%mlx4eth63_vCX3Pro.22f5.DeviceDesc%  = mlx4eth63_vCX3Pro.ndi,  MLX4\ConnectX-3_vEth&22f5103c	              	; Ethernet name for CX3 in VM
%mlx4eth63_vCX3Pro.22f5.DeviceDesc%  = mlx4eth63_vCX3Pro_NW.ndi,  MLX4\ConnectX-3_vEth_NW&22f5103c	           	; Ethernet name for CX3 in VM over non Windows

; VEA HWIDs
%mlx4eth63_CX3Pro_VEA.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi, MLX4\ConnectX-3Pro_Eth_V   				; VEA Ethernet name for CX3 Pro
%mlx4eth63_CX3_VEA.DeviceDesc%	   = mlx4eth63_CX3_VEA.ndi,    MLX4\ConnectX-3_Eth_V	  					; VEA Ethernet name for CX3
%mlx4eth63_CX3_VEA.DeviceDesc%	   = mlx4eth63_CX3_VEA.ndi,    MLX4\ConnectX-3_vEth_V	  				; VEA Ethernet name for CX3
%mlx4eth63_CX3_VEA.DeviceDesc%	   = mlx4eth63_CX3_VEA.ndi,    MLX4\ConnectX-3_vEth_NW_V	  		    ; VEA Ethernet name for CX3 over non Windows

;;;;; cards of other companies

; HP Maze
%mlx4eth63_CX3Pro_VEA.801f.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&801f103c	 ; HP Maze ConnectX-3 Pro virtual Ethernet Adapter for VEA CX3 in Host
%mlx4eth63_CX3Pro_VEA.801f.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_V&801f103c	 	 ; HP Maze ConnectX-3 Pro virtual Ethernet Adapter for VEA CX3 in VM
%mlx4eth63_CX3Pro_VEA.801f.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_NW_V&801f103c	 ; HP Maze ConnectX-3 Pro virtual Ethernet Adapter for VEA CX3 in VM over non Windows

; HP Mesa
%mlx4eth63_CX3Pro_VEA.8020.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&8020103c	 ; HP Mesa ConnectX-3 Pro virtual Ethernet Adapter for VEA CX3 in Host
%mlx4eth63_CX3Pro_VEA.8020.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_V&8020103c	 ; HP Mesa ConnectX-3 Pro virtual Ethernet Adapter for VEA CX3 in VM
%mlx4eth63_CX3Pro_VEA.8020.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_NW_V&8020103c	 ; HP Mesa ConnectX-3 Pro virtual Ethernet Adapter for VEA CX3 in VM over non Windows

; HP Attitash CX3
%mlx4eth63_CX3_VEA.18cd.DeviceDesc%  = mlx4eth63_CX3_VEA.ndi,  MLX4\ConnectX-3_Eth_V&18cd103c	               ; HP Attitash QDR ConnectX-3 Ethernet Adapter for VEA CX3 in Host
%mlx4eth63_CX3_VEA.18cd.DeviceDesc%  = mlx4eth63_CX3_VEA.ndi,  MLX4\ConnectX-3_vEth_V&18cd103c	               ; HP Attitash QDR ConnectX-3 Ethernet Adapter for VEA CX3 in VM
%mlx4eth63_CX3_VEA.18cd.DeviceDesc%  = mlx4eth63_CX3_VEA.ndi,  MLX4\ConnectX-3_vEth_NW_V&18cd103c	       ; HP Attitash QDR ConnectX-3 Ethernet Adapter for VEA CX3 in VM over non Windows

; HP Attitash CX3 PRO
%mlx4eth63_CX3_VEA.22f1.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&22f1103c	               ; Ethernet name for VEA CX3 in Host
%mlx4eth63_CX3_VEA.22f2.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&22f2103c	               ; Ethernet name for VEA CX3 in Host
%mlx4eth63_CX3_VEA.22f3.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&22f3103c	               ; Ethernet name for VEA CX3 in Host
%mlx4eth63_CX3_VEA.22f4.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&22f4103c	               ; Ethernet name for VEA CX3 in Host
%mlx4eth63_CX3_VEA.22f5.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&22f5103c	               ; Ethernet name for VEA CX3 in Host
%mlx4eth63_CX3_VEA.22f1.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_V&22f1103c	               ; Ethernet name for VEA CX3 in VM
%mlx4eth63_CX3_VEA.22f2.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_V&22f2103c	               ; Ethernet name for VEA CX3 in VM
%mlx4eth63_CX3_VEA.22f3.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_V&22f3103c	               ; Ethernet name for VEA CX3 in VM
%mlx4eth63_CX3_VEA.22f4.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_V&22f4103c	               ; Ethernet name for VEA CX3 in VM
%mlx4eth63_CX3_VEA.22f5.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_V&22f5103c	               ; Ethernet name for VEA CX3 in VM
%mlx4eth63_CX3_VEA.22f5.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3_vEth_NW_V&22f5103c	           ; Ethernet name for VEA CX3 in VM over non Windows


; ATTO CX3 PRO Single Port 10GbE
%mlx4eth63_CX3Pro.0092.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&0092117c	                    ; Ethernet name for CX3 Pro
%mlx4eth63_CX3Pro_VEA.0092.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&0092117c	            ; ATTO Virtual Ethernet Adapter for CX3 Pro

; ATTO CX3 PRO Dual Port 10GbE
%mlx4eth63_CX3Pro.0093.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&0093117c	                    ; Ethernet name for CX3 Pro
%mlx4eth63_CX3Pro_VEA.0093.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&0093117c	            ; ATTO Virtual Ethernet Adapter for CX3 Pro

; ATTO CX3 PRO Single Port 40GbE
%mlx4eth63_CX3Pro.0090.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&0090117c	                    ; Ethernet name for CX3 Pro
%mlx4eth63_CX3Pro_VEA.0090.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&0090117c	            ; ATTO Virtual Ethernet Adapter for CX3 Pro

; ATTO CX3 PRO Dual Port 40GbE
%mlx4eth63_CX3Pro.0091.DeviceDesc%  = mlx4eth63_CX3Pro.ndi,  MLX4\ConnectX-3Pro_Eth&0091117c	                    ; Ethernet name for CX3 Pro
%mlx4eth63_CX3Pro_VEA.0091.DeviceDesc%  = mlx4eth63_CX3Pro_VEA.ndi,  MLX4\ConnectX-3Pro_Eth_V&0091117c	            ; ATTO Virtual Ethernet Adapter for CX3 Pro

;
; Windows NT specific entry
;
;-----------------------------------------------------------------------------
; ConnectX-2 and ConnectX
;
[mlx4eth63_CX2.ndi.NT]
Characteristics = 0x81
AddReg          = cx.reg, cx_pf.reg, mlx4eth63.reg, bindings.reg, virt.reg, WinCtxTune_reg, rx_int_mod_pf.reg , int_mod_pf.reg
DelReg          = cx_del.reg
CopyFiles       = mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[mlx4eth63_CX2.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog



;-----------------------------------------------------------------------------
; ConnectX-3
;
[mlx4eth63_CX3.ndi.NT]
Characteristics = 0x81
AddReg          = cx.reg, cx_pf.reg, mlx4eth63.reg, bindings.reg, virt.reg, WinCtxTune_reg, cx3_pf.reg, rx_int_mod_pf.reg, int_mod_pf.reg
DelReg          = cx_del.reg
CopyFiles       = mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[mlx4eth63_CX3.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog



;-----------------------------------------------------------------------------
; ConnectX-3Pro
;
[mlx4eth63_CX3Pro.ndi.NT]
Characteristics = 0x81
AddReg          = cx.reg, cx_pf.reg, mlx4eth63.reg, bindings.reg, virt.reg, WinCtxTune_reg, cx3_pf.reg, cx3Pro.reg, rx_int_mod_pf.reg, int_mod_pf.reg
DelReg          = cx_del.reg
CopyFiles       = mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[mlx4eth63_CX3Pro.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog



;-----------------------------------------------------------------------------
; ConnectX-3 VF
;
[mlx4eth63_vCX3.ndi.NT]
Characteristics = 0x81
AddReg          = cx.reg, cx_vf.reg, mlx4eth63.reg, vf_bindings.reg, WinCtxTune_reg, cx3_vf.reg, rx_int_mod_vf.reg, int_mod_vf.reg
DelReg          = cx_del.reg, cx_vf_del.reg
CopyFiles       = mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[mlx4eth63_vCX3.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog

;-----------------------------------------------------------------------------
; ConnectX-3 VF over non-windows
;
[mlx4eth63_vCX3_NW.ndi.NT]
Characteristics = 0x81
AddReg          = cx.reg, cx_vf.reg, mlx4eth63.reg, bindings.reg, WinCtxTune_reg, cx3_vf.reg, rx_int_mod_vf.reg, int_mod_vf.reg
DelReg          = cx_del.reg, cx_vf_del.reg
CopyFiles       = mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[mlx4eth63_vCX3_NW.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog

;-----------------------------------------------------------------------------
; ConnectX-3 Pro VF
;
[mlx4eth63_vCX3Pro.ndi.NT]
Characteristics = 0x81
AddReg          = cx.reg, cx_vf.reg, mlx4eth63.reg, vf_bindings.reg, WinCtxTune_reg, cx3_vf.reg, cx3Pro.reg, rx_int_mod_vf.reg, int_mod_vf.reg
DelReg          = cx_del.reg, cx_vf_del.reg
CopyFiles       = mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[mlx4eth63_vCX3Pro.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog

;-----------------------------------------------------------------------------
; ConnectX-3 Pro VF over non-windows
;
[mlx4eth63_vCX3Pro_NW.ndi.NT]
Characteristics = 0x81
AddReg          = cx.reg, cx_vf.reg, mlx4eth63.reg, bindings.reg, WinCtxTune_reg, cx3_vf.reg, cx3Pro.reg, rx_int_mod_vf.reg, int_mod_vf.reg
DelReg          = cx_del.reg, cx_vf_del.reg
CopyFiles       = mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[mlx4eth63_vCX3Pro_NW.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog


;-----------------------------------------------------------------------------

; ConnectX-3 VEA (Virtual Ethernet Adapter)
;
[mlx4eth63_CX3_VEA.ndi.NT]
Characteristics = 0x81
AddReg			= cx.reg, cx_vea.reg, mlx4eth63.reg, bindings.reg, virt.reg, WinCtxTune_reg, rx_int_mod_pf.reg, int_mod_pf.reg
CopyFiles		= mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType 		= 6 	; IF_TYPE_ETHERNET_CSMACD
*MediaType		= 0 	; NdisMedium802_3
*PhysicalMediaType = 14 	; NdisPhysicalMedium802_3

[mlx4eth63_CX3_VEA.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog


;-----------------------------------------------------------------------------
; ConnectX-3Pro VEA (Virtual Ethernet Adapter)
;
[mlx4eth63_CX3Pro_VEA.ndi.NT]
Characteristics = 0x81
AddReg			= cx.reg, cx_vea.reg, mlx4eth63.reg, bindings.reg, virt.reg, WinCtxTune_reg, cx3Pro.reg, rx_int_mod_pf.reg, int_mod_pf.reg
CopyFiles		= mlx4eth63.CopyFiles, Wctxtune.CopyFiles
*IfType 		= 6 	; IF_TYPE_ETHERNET_CSMACD
*MediaType		= 0 	; NdisMedium802_3
*PhysicalMediaType = 14 	; NdisPhysicalMedium802_3

[mlx4eth63_CX3Pro_VEA.ndi.NT.Services]
AddService = mlx4eth63, 2, mlx4eth63.Service, common.EventLog


;-----------------------------------------------------------------------------

; cx.reg - parameters, HW-agnostic and common for PF and VF
;
[cx.reg]
HKR, NDI\Params\NumTcb,         ParamDesc,  0, "%TransmitControlBlocks%"
HKR, NDI\Params\NumTcb,         default,    0, "16"
HKR, NDI\Params\NumTcb,         min,        0, "1"
HKR, NDI\Params\NumTcb,         max,        0, "00000064"
HKR, NDI\Params\NumTcb,         step,       0, "1"
HKR, NDI\Params\NumTcb,         Base,       0, "10"
HKR, NDI\Params\NumTcb,         type,       0, "int"
HKR, "",                        NumTcb,     %FLG_ADDREG_NOCLOBBER%, "16"

;RSS
HKR, NDI\Params\*RSS,  ParamDesc, 0, "%RssMode%"
HKR, NDI\Params\*RSS,  Type,  0, "enum"
HKR, NDI\Params\*RSS,  Default, 0, "1"
HKR, NDI\Params\*RSS,  Optional, 0, "0"
HKR, NDI\Params\*RSS\enum,  "0", 0, "%No_rebalnce%"
HKR, NDI\Params\*RSS\enum,  "1", 0, "%NDIS_RSS%"
HKR, "", *RSS,  %FLG_ADDREG_NOCLOBBER%, "1"

; *NumaNodeId
HKR, Ndi\params\*NumaNodeId, ParamDesc, 0, %NumaNodeId%
HKR, Ndi\params\*NumaNodeId, default, 0, "65535"
HKR, Ndi\params\*NumaNodeId, type, 0, "enum"
HKR, Ndi\params\*NumaNodeId\Enum, "65535", 0, %NumaNodeId_default%
HKR, Ndi\params\*NumaNodeId\Enum, "0", 0, %node0%
HKR, Ndi\params\*NumaNodeId\Enum, "1", 0, %node1%
HKR, Ndi\params\*NumaNodeId\Enum, "2", 0, %node2%
HKR, Ndi\params\*NumaNodeId\Enum, "3", 0, %node3%
HKR, Ndi\params\*NumaNodeId\Enum, "4", 0, %node4%
HKR, Ndi\params\*NumaNodeId\Enum, "5", 0, %node5%
HKR, Ndi\params\*NumaNodeId\Enum, "6", 0, %node6%
HKR, Ndi\params\*NumaNodeId\Enum, "7", 0, %node7%
HKR, "", *NumaNodeId,  0, "65535"

; *RssBaseProcNumber
HKR, Ndi\params\*RssBaseProcNumber, ParamDesc, 0, %RssBaseProcNumber%
HKR, Ndi\params\*RssBaseProcNumber, default, 0, "0"
HKR, Ndi\params\*RssBaseProcNumber, min, 0, "0"
HKR, Ndi\params\*RssBaseProcNumber, max, 0, "63"
HKR, Ndi\params\*RssBaseProcNumber, step, 0, "1"
HKR, Ndi\params\*RssBaseProcNumber, Optional, 0, "0"
HKR, Ndi\params\*RssBaseProcNumber, type, 0, "int"
HKR, "", *RssBaseProcNumber,  %FLG_ADDREG_NOCLOBBER%, "0"

; *MaxRssProcessors
HKR, Ndi\Params\*MaxRssProcessors,	ParamDesc, 0, %MaxRssProcessors%
HKR, Ndi\Params\*MaxRssProcessors,  default, 0, "8"
HKR, Ndi\Params\*MaxRssProcessors,  type,    0, "int"
HKR, NDI\Params\*MaxRssProcessors,  min,     0, "1"
HKR, NDI\Params\*MaxRssProcessors,  max,     0, "64"
HKR, NDI\Params\*MaxRssProcessors,  step,        0, "1"
HKR, NDI\Params\*MaxRssProcessors,  Base,        0, "10"
HKR, "", *MaxRssProcessors,  %FLG_ADDREG_NOCLOBBER%, "8"

;*NumRSSQueues
HKR, NDI\Params\*NumRSSQueues,  ParamDesc, 0, "%NumRSSQueues%"
HKR, NDI\Params\*NumRSSQueues,  Type,      0, "int"
HKR, NDI\Params\*NumRSSQueues,  Default,   0, "8"
HKR, NDI\Params\*NumRSSQueues,  min,       0, "1"
HKR, NDI\Params\*NumRSSQueues,  max,       0, "512"
HKR, NDI\Params\*NumRSSQueues,  step,      0, "1"
HKR, NDI\Params\*NumRSSQueues,  Base,      0, "10"
HKR, "", *NumRSSQueues,%FLG_ADDREG_NOCLOBBER%, "8"

;*RscIPv4
HKR, NDI\Params\*RscIPv4,  ParamDesc, 0, "%RscIPv4%"
HKR, NDI\Params\*RscIPv4,  Type,      0, "enum"
HKR, NDI\Params\*RscIPv4,  Default,   0, "1"
HKR, NDI\Params\*RscIPv4,  Optional,  0, "0"
HKR, NDI\Params\*RscIPv4\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*RscIPv4\enum,  "1",  0, "%Enabled%"
HKR, "", *RscIPv4, 0, "1"

;*RscIPv6
HKR, NDI\Params\*RscIPv6,  ParamDesc, 0, "%RscIPv6%"
HKR, NDI\Params\*RscIPv6,  Type,      0, "enum"
HKR, NDI\Params\*RscIPv6,  Default,   0, "1"
HKR, NDI\Params\*RscIPv6,  Optional,  0, "0"
HKR, NDI\Params\*RscIPv6\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*RscIPv6\enum,  "1",  0, "%Enabled%"
HKR, "", *RscIPv6, 0, "1"

; *RSSProfile
HKR, NDI\Params\*RSSProfile,  ParamDesc, 0, "%RssProfile%"
HKR, NDI\Params\*RSSProfile,  Type,  0, "enum"
HKR, NDI\Params\*RSSProfile,  Default, 0, "1"
HKR, NDI\Params\*RSSProfile\enum,  "1", 0, "%Closest_Processor%"
HKR, NDI\Params\*RSSProfile\enum,  "2", 0, "%Closest_Processor_Static%"
HKR, NDI\Params\*RSSProfile\enum,  "3", 0, "%Numa_Scaling%"
HKR, NDI\Params\*RSSProfile\enum,  "4", 0, "%Numa_Scaling_Static%"
HKR, NDI\Params\*RSSProfile\enum,  "5", 0, "%Conservative_Scaling%"
HKR, "", *RSSProfile,  0, "1"

HKR, NDI\Params\*IPChecksumOffloadIPv4,  ParamDesc, 0, "%IPChecksumOffloadIPv4%"
HKR, NDI\Params\*IPChecksumOffloadIPv4,  Type,      0, "enum"
HKR, NDI\Params\*IPChecksumOffloadIPv4,  Default,   0, "3"
HKR, NDI\Params\*IPChecksumOffloadIPv4,  Optional,  0, "0"
HKR, NDI\Params\*IPChecksumOffloadIPv4\enum,	"0",  0, "%Disabled%"
HKR, NDI\Params\*IPChecksumOffloadIPv4\enum,	"1",  0, "%TxEnabled%"
HKR, NDI\Params\*IPChecksumOffloadIPv4\enum,	"2",  0, "%RxEnabled%"
HKR, NDI\Params\*IPChecksumOffloadIPv4\enum,	"3",  0, "%TxRxEnabled%"
HKR, "", *IPChecksumOffloadIPv4, %FLG_ADDREG_NOCLOBBER%, "3"

HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4,  ParamDesc, 0, "%TCPUDPChecksumOffloadIPv4%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4,  Type,      0, "enum"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4,  Default,   0, "3"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4,  Optional,  0, "0"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4\enum,	"0",  0, "%Disabled%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4\enum,	"1",  0, "%TxEnabled%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4\enum,	"2",  0, "%RxEnabled%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv4\enum,	"3",  0, "%TxRxEnabled%"
HKR, "", *TCPUDPChecksumOffloadIPv4, %FLG_ADDREG_NOCLOBBER%, "3"

HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6,  ParamDesc, 0, "%TCPUDPChecksumOffloadIPv6%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6,  Type,      0, "enum"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6,  Default,   0, "3"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6,  Optional,  0, "0"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6\enum,	"0",  0, "%Disabled%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6\enum,	"1",  0, "%TxEnabled%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6\enum,	"2",  0, "%RxEnabled%"
HKR, NDI\Params\*TCPUDPChecksumOffloadIPv6\enum,	"3",  0, "%TxRxEnabled%"
HKR, "", *TCPUDPChecksumOffloadIPv6, %FLG_ADDREG_NOCLOBBER%, "3"

HKR, NDI\Params\*LsoV2IPv4,  ParamDesc, 0, "%LsoV2IPv4%"
HKR, NDI\Params\*LsoV2IPv4,  Type,      0, "enum"
HKR, NDI\Params\*LsoV2IPv4,  Default,   0, "1"
HKR, NDI\Params\*LsoV2IPv4,  Optional,  0, "0"
HKR, NDI\Params\*LsoV2IPv4\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*LsoV2IPv4\enum,  "1",  0, "%Enabled%"
HKR, "", *LsoV2IPv4, %FLG_ADDREG_NOCLOBBER%, "1"

HKR, NDI\Params\*LsoV2IPv6,  ParamDesc, 0, "%LsoV2IPv6%"
HKR, NDI\Params\*LsoV2IPv6,  Type,      0, "enum"
HKR, NDI\Params\*LsoV2IPv6,  Default,   0, "1"
HKR, NDI\Params\*LsoV2IPv6,  Optional,  0, "0"
HKR, NDI\Params\*LsoV2IPv6\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*LsoV2IPv6\enum,  "1",  0, "%Enabled%"
HKR, "", *LsoV2IPv6, %FLG_ADDREG_NOCLOBBER%, "1"

HKR, NDI\Params\TxBwPrecedence,  ParamDesc, 0, "%TxBwPrecedence%"
HKR, NDI\Params\TxBwPrecedence,  Type,      0, "enum"
HKR, NDI\Params\TxBwPrecedence,  Default,	0, "0"
HKR, NDI\Params\TxBwPrecedence,  Optional,  0, "1"
HKR, Ndi\Params\TxBwPrecedence\enum,	"0",  0, "%Default%"
HKR, Ndi\Params\TxBwPrecedence\enum,	"1",  0, "%Precending%"
HKR, "", TxBwPrecedence,  %FLG_ADDREG_NOCLOBBER%,  "0"

HKR, NDI\Params\NetworkAddress,  ParamDesc,  0, "%NetworkAddress%"
HKR, NDI\params\NetworkAddress,  Default,    0, ""
HKR, NDI\params\NetworkAddress,  type,       0, "edit"
HKR, NDI\params\NetworkAddress,  LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,  UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,  optional,   0, "1"

HKR, NDI\Params\RxBufferAlignment ,         ParamDesc,  0, "%RxBufferAlignment%"
HKR, NDI\Params\RxBufferAlignment ,         default,    0, "0"
HKR, NDI\Params\RxBufferAlignment ,         min,        0, "0"
HKR, NDI\Params\RxBufferAlignment ,         max,        0, "63"
HKR, NDI\Params\RxBufferAlignment ,         step,       0, "1"
HKR, NDI\Params\RxBufferAlignment ,         Base,       0, "10"
HKR, NDI\Params\RxBufferAlignment ,         type,       0, "int"
HKR, "", RxBufferAlignment ,  %FLG_ADDREG_NOCLOBBER%, "0"


;-----------------------------------------------------------------------------
; rx_int_mod_pf.reg - RX interrupt moderation parameters for PF
;
[rx_int_mod_pf.reg]
HKR, NDI\Params\RecvCompletionMethod,  ParamDesc, 0, "%RecvCompletionMethod%"
HKR, NDI\Params\RecvCompletionMethod,  Type,  0, "enum"
HKR, NDI\Params\RecvCompletionMethod,  Default, 0, "1"
HKR, NDI\Params\RecvCompletionMethod,  Optional, 0, "0"
HKR, NDI\Params\RecvCompletionMethod\enum,  "0", 0, "%Polling%"
HKR, NDI\Params\RecvCompletionMethod\enum,  "1", 0, "%Adaptive%"
;Fix RM:-443273, delete uncorrect registry value.
HKR, NDI\Params\RecvCompletionMethod\enum,  "2", 0x00000004, ""
HKR, "", RecvCompletionMethod, 0, "1"

HKR, NDI\Params\RxIntModeration,  ParamDesc, 0, "%RxIntModeration%"
HKR, NDI\Params\RxIntModeration,  Type,		0, "enum"
HKR, NDI\Params\RxIntModeration,  Default,	0, "2"
HKR, NDI\Params\RxIntModeration,  Optional,	0, "0"
HKR, NDI\Params\RxIntModeration\enum, "1",	0, "%Static%"
HKR, NDI\Params\RxIntModeration\enum, "2",	0, "%Adaptive%"
HKR, "", RxIntModeration,%FLG_ADDREG_NOCLOBBER%, "2"

HKR, NDI\Params\RxIntModerationProfile,  ParamDesc, 0, "%RxIntModerationProfile%"
HKR, NDI\Params\RxIntModerationProfile,  Type,      0, "enum"
HKR, NDI\Params\RxIntModerationProfile,  Default,   0, "1"
HKR, NDI\Params\RxIntModerationProfile,  Optional,  0, "0"
HKR, NDI\Params\RxIntModerationProfile\enum,  "0",  0, "%LowLatency%"
HKR, NDI\Params\RxIntModerationProfile\enum,  "1",  0, "%Moderate%"
HKR, NDI\Params\RxIntModerationProfile\enum,  "2",  0, "%Aggressive%"
HKR, "", RxIntModerationProfile, 0, "1"


;-----------------------------------------------------------------------------
; int_mod_pf.reg - TX interrupt moderation parameters for PF
;
[int_mod_pf.reg]
HKR, NDI\Params\TxIntModerationProfile,  ParamDesc, 0, "%TxIntModerationProfile%"
HKR, NDI\Params\TxIntModerationProfile,  Type,      0, "enum"
HKR, NDI\Params\TxIntModerationProfile,  Default,   0, "1"
HKR, NDI\Params\TxIntModerationProfile,  Optional,  0, "0"
HKR, NDI\Params\TxIntModerationProfile\enum,  "0",  0, "%LowLatency%"
HKR, NDI\Params\TxIntModerationProfile\enum,  "1",  0, "%Moderate%"
HKR, NDI\Params\TxIntModerationProfile\enum,  "2",  0, "%Aggressive%"
HKR, "", TxIntModerationProfile, 0, "1"

HKR, NDI\Params\ThreadPoll,         ParamDesc,  0, "%ThreadPoll%"
HKR, NDI\Params\ThreadPoll,         Default,    0, "10000"
HKR, NDI\Params\ThreadPoll,         min,        0, "1"
HKR, NDI\Params\ThreadPoll,         max,        0, "200000"
HKR, NDI\Params\ThreadPoll,         step,       0, "1"
HKR, NDI\Params\ThreadPoll,         Base,       0, "10"
HKR, NDI\Params\ThreadPoll,         type,       0, "dword"
HKR, "", ThreadPoll,  %FLG_ADDREG_NOCLOBBER%, "10000"

;-----------------------------------------------------------------------------
; rx_int_mod_vf.reg - RX interrupt moderation parameters for VF
;
[rx_int_mod_vf.reg]
HKR, NDI\Params\RecvCompletionMethod,  ParamDesc, 0, "%RecvCompletionMethod%"
HKR, NDI\Params\RecvCompletionMethod,  Type,  0, "enum"
HKR, NDI\Params\RecvCompletionMethod,  Default, 0, "1"
HKR, NDI\Params\RecvCompletionMethod,  Optional, 0, "0"
HKR, NDI\Params\RecvCompletionMethod\enum,  "0", 0, "%Polling%"
HKR, NDI\Params\RecvCompletionMethod\enum,  "1", 0, "%Adaptive%"
;Fix RM:-443273, delete uncorrect registry value.
HKR, NDI\Params\RecvCompletionMethod\enum,  "2", 0x00000004, ""
HKR, "", RecvCompletionMethod, 0, "1"

HKR, NDI\Params\RxIntModeration,  ParamDesc, 0, "%RxIntModeration%"
HKR, NDI\Params\RxIntModeration,  Type,     0, "enum"
HKR, NDI\Params\RxIntModeration,  Default,  0, "0"
HKR, NDI\Params\RxIntModeration,  Optional, 0, "0"
HKR, NDI\Params\RxIntModeration\enum, "1",  0, "%Static%"
HKR, NDI\Params\RxIntModeration\enum, "2",  0, "%Adaptive%"
HKR, "", RxIntModeration,0, "0"

HKR, NDI\Params\RxIntModerationProfile,  ParamDesc, 0, "%RxIntModerationProfile%"
HKR, NDI\Params\RxIntModerationProfile,  Type,      0, "enum"
HKR, NDI\Params\RxIntModerationProfile,  Default,   0, "0"
HKR, NDI\Params\RxIntModerationProfile,  Optional,  0, "0"
HKR, NDI\Params\RxIntModerationProfile\enum,  "0",  0, "%LowLatency%"
HKR, NDI\Params\RxIntModerationProfile\enum,  "1",  0, "%Moderate%"
HKR, NDI\Params\RxIntModerationProfile\enum,  "2",  0, "%Aggressive%"
HKR, "", RxIntModerationProfile, 0, "0"

;-----------------------------------------------------------------------------
; int_mod_vf.reg - TX interrupt moderation parameters for VF
;
[int_mod_vf.reg]
HKR, NDI\Params\TxIntModerationProfile,  ParamDesc, 0, "%TxIntModerationProfile%"
HKR, NDI\Params\TxIntModerationProfile,  Type,      0, "enum"
HKR, NDI\Params\TxIntModerationProfile,  Default,   0, "0"
HKR, NDI\Params\TxIntModerationProfile,  Optional,  0, "0"
HKR, NDI\Params\TxIntModerationProfile\enum,  "0",  0, "%LowLatency%"
HKR, NDI\Params\TxIntModerationProfile\enum,  "1",  0, "%Moderate%"
HKR, NDI\Params\TxIntModerationProfile\enum,  "2",  0, "%Aggressive%"
HKR, "", TxIntModerationProfile, 0, "0"

HKR, NDI\Params\ThreadPoll,         ParamDesc,  0, "%ThreadPoll%"
HKR, NDI\Params\ThreadPoll,         Default,    0, "10000"
HKR, NDI\Params\ThreadPoll,         min,        0, "1"
HKR, NDI\Params\ThreadPoll,         max,        0, "200000"
HKR, NDI\Params\ThreadPoll,         step,       0, "1"
HKR, NDI\Params\ThreadPoll,         Base,       0, "10"
HKR, NDI\Params\ThreadPoll,         type,       0, "dword"
HKR, "", ThreadPoll,  %FLG_ADDREG_NOCLOBBER%, "10000"


;-----------------------------------------------------------------------------
; cx_pf.reg - parameters, HW agnostic and specific for PF
;
[cx_pf.reg]
HKR, NDI\Params\IgnoreFCS,  ParamDesc, 0, "%IgnoreFCS%"
HKR, NDI\Params\IgnoreFCS,  Type,      0, "enum"
HKR, NDI\Params\IgnoreFCS,  Default,   0, "0"
HKR, NDI\Params\IgnoreFCS,  Optional,  0, "0"
HKR, NDI\Params\IgnoreFCS\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\IgnoreFCS\enum,  "1",  0, "%Enabled%"
HKR, "", IgnoreFCS, 0, "0"

HKR, NDI\Params\*ReceiveBuffers,  ParamDesc, 0, "%RecvRingSize%"
HKR, NDI\Params\*ReceiveBuffers,  default,    0, "4096"
HKR, NDI\Params\*ReceiveBuffers,  min, 	   0, "256"
HKR, NDI\Params\*ReceiveBuffers,  max, 	   0, "4096"
HKR, NDI\Params\*ReceiveBuffers,  step,	   0, "1"
HKR, NDI\Params\*ReceiveBuffers,  Base,	   0, "10"
HKR, NDI\Params\*ReceiveBuffers,  type,	   0, "int"
HKR, "", *ReceiveBuffers, %FLG_ADDREG_NOCLOBBER%, "4096"

HKR, NDI\Params\*TransmitBuffers,  ParamDesc, 0, "%SendRingSize%"
HKR, NDI\Params\*TransmitBuffers,  default,	  0, "2048"
HKR, NDI\Params\*TransmitBuffers,  min,	   0, "256"
HKR, NDI\Params\*TransmitBuffers,  max,	   0, "4096"
HKR, NDI\Params\*TransmitBuffers,  step,    0, "1"
HKR, NDI\Params\*TransmitBuffers,  Base,    0, "10"
HKR, NDI\Params\*TransmitBuffers,  type,    0, "int"
HKR, "", *TransmitBuffers,  %FLG_ADDREG_NOCLOBBER%, "2048"

HKR, NDI\Params\*JumboPacket ,		   ParamDesc,  0, "%MaxFrameSize%"
HKR, NDI\Params\*JumboPacket ,		   default,    0, "1514"
HKR, NDI\Params\*JumboPacket ,		   min, 	   0, "614"
HKR, NDI\Params\*JumboPacket ,		   max, 	   0, "00009614"
HKR, NDI\Params\*JumboPacket ,		   step,	   0, "1"
HKR, NDI\Params\*JumboPacket ,		   Base,	   0, "10"
HKR, NDI\Params\*JumboPacket ,		   type,	   0, "int"
HKR, "", *JumboPacket ,  %FLG_ADDREG_NOCLOBBER%, "1514"

HKR, NDI\Params\*NetworkDirect,            ParamDesc,  0, %ND_STR%
HKR, NDI\Params\*NetworkDirect,            Type,       0, "enum"
HKR, NDI\Params\*NetworkDirect,            Default,   0, "1"
HKR, NDI\Params\*NetworkDirect\enum,       "0",        0, "%Disabled%"
HKR, NDI\Params\*NetworkDirect\enum,       "1",        0, "%Enabled%"
HKR, "", *NetworkDirect, %FLG_ADDREG_NOCLOBBER%, "1"

HKR, NDI\Params\RoceMaxFrameSize ,         ParamDesc,  0, "%RoceMaxFrameSize%"
HKR, NDI\Params\RoceMaxFrameSize ,		   type,	   0, "enum"
HKR, NDI\Params\RoceMaxFrameSize ,         default,    0, "0"
HKR, NDI\Params\RoceMaxFrameSize\enum,		  "0",		0, "%MaxSizeWithinMaxFramSize%"
HKR, NDI\Params\RoceMaxFrameSize\enum,		  "256",	0, "256"
HKR, NDI\Params\RoceMaxFrameSize\enum,		  "512",	0, "512"
HKR, NDI\Params\RoceMaxFrameSize\enum,		  "1024",	0, "1024"
HKR, NDI\Params\RoceMaxFrameSize\enum,		  "2048",	0, "2048"
HKR, "", RoceMaxFrameSize ,  %FLG_ADDREG_NOCLOBBER%, "0"

HKR, NDI\Params\*FlowControl,  ParamDesc, 0, "%FlowControl%"
HKR, NDI\Params\*FlowControl,  Type,      0, "enum"
HKR, NDI\Params\*FlowControl,  Default,   0, "3"
HKR, NDI\Params\*FlowControl,  Optional,  0, "0"
HKR, NDI\Params\*FlowControl\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*FlowControl\enum,  "1",  0, "%TxEnabled%"
HKR, NDI\Params\*FlowControl\enum,  "2",  0, "%RxEnabled%"
HKR, NDI\Params\*FlowControl\enum,  "3",  0, "%TxRxEnabled%"
HKR, "", *FlowControl, %FLG_ADDREG_NOCLOBBER%, "3"

HKR, NDI\Params\*PriorityVLANTag,  ParamDesc, 0, "%PriorityVLANTag%"
HKR, NDI\Params\*PriorityVLANTag,  Type,      0, "enum"
HKR, NDI\Params\*PriorityVLANTag,  Default,   0, "3"
HKR, NDI\Params\*PriorityVLANTag\enum,        "0",  0, "%PriorityVlanDisabled%"
HKR, NDI\Params\*PriorityVLANTag\enum,        "1",  0, "%PriorityEnabled%"
HKR, NDI\Params\*PriorityVLANTag\enum,        "2",  0, "%VlanEnabled%"
HKR, NDI\Params\*PriorityVLANTag\enum,        "3",  0, "%PriorityVlanEnabled%"
HKR, "", *PriorityVLANTag, %FLG_ADDREG_NOCLOBBER%, "3"

HKR, NDI\Params\*PriorityVLANTag,  ParamDesc, 0, "%PriorityVLANTag%"
HKR, NDI\Params\*PriorityVLANTag,  Type,      0, "enum"
HKR, NDI\Params\*PriorityVLANTag,  Default,   0, "3"
HKR, NDI\Params\*PriorityVLANTag\enum,        "0",  0, "%PriorityVlanDisabled%"
HKR, NDI\Params\*PriorityVLANTag\enum,        "1",  0, "%PriorityEnabled%"
HKR, NDI\Params\*PriorityVLANTag\enum,        "2",  0, "%VlanEnabled%"
HKR, NDI\Params\*PriorityVLANTag\enum,        "3",  0, "%PriorityVlanEnabled%"
HKR, "", *PriorityVLANTag, %FLG_ADDREG_NOCLOBBER%, "3"

HKR, NDI\Params\VlanID,  ParamDesc, 0, "%VlanID%"
HKR, NDI\Params\VlanID,  default,	  0, "0"
HKR, NDI\Params\VlanID,  min,	   0, "0"
HKR, NDI\Params\VlanID,  max,	   0, "4095"
HKR, NDI\Params\VlanID,  step,    0, "1"
HKR, NDI\Params\VlanID,  Base,    0, "10"
HKR, NDI\Params\VlanID,  type,    0, "int"
HKR, "", VlanID,  %FLG_ADDREG_NOCLOBBER%, "0"

HKR, NDI\Params\*InterruptModeration,  ParamDesc, 0, "%InterruptModeration%"
HKR, NDI\Params\*InterruptModeration,  Type,      0, "enum"
HKR, NDI\Params\*InterruptModeration,  Default,   0, "1"
HKR, NDI\Params\*InterruptModeration,  Optional,  0, "0"
HKR, NDI\Params\*InterruptModeration\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*InterruptModeration\enum,  "1",  0, "%Enabled%"
HKR, "", *InterruptModeration, %FLG_ADDREG_NOCLOBBER%, "1"

;-----------------------------------------------------------------------------
; cx_vf.reg - parameters, HW agnostic and specific for VF
;
[cx_vf.reg]
HKR, "", *PriorityVLANTag, 0, "0"

HKR, NDI\Params\*ReceiveBuffers,  ParamDesc, 0, "%RecvRingSize%"
HKR, NDI\Params\*ReceiveBuffers,  default,    0, "3072"
HKR, NDI\Params\*ReceiveBuffers,  min, 	   0, "256"
HKR, NDI\Params\*ReceiveBuffers,  max, 	   0, "4096"
HKR, NDI\Params\*ReceiveBuffers,  step,	   0, "1"
HKR, NDI\Params\*ReceiveBuffers,  Base,	   0, "10"
HKR, NDI\Params\*ReceiveBuffers,  type,	   0, "int"
HKR, "", *ReceiveBuffers, 0, "3072"

HKR, NDI\Params\*TransmitBuffers,  ParamDesc, 0, "%SendRingSize%"
HKR, NDI\Params\*TransmitBuffers,  default,	  0, "2048"
HKR, NDI\Params\*TransmitBuffers,  min,	   0, "256"
HKR, NDI\Params\*TransmitBuffers,  max,	   0, "4096"
HKR, NDI\Params\*TransmitBuffers,  step,    0, "1"
HKR, NDI\Params\*TransmitBuffers,  Base,    0, "10"
HKR, NDI\Params\*TransmitBuffers,  type,    0, "int"
HKR, "", *TransmitBuffers,  %FLG_ADDREG_NOCLOBBER%, "2048"

HKR, NDI\Params\*JumboPacket ,		   ParamDesc,  0, "%MaxFrameSize%"
HKR, NDI\Params\*JumboPacket ,		   default,    0, "1514"
HKR, NDI\Params\*JumboPacket ,		   min, 	   0, "614"
HKR, NDI\Params\*JumboPacket ,		   max, 	   0, "00009614"
HKR, NDI\Params\*JumboPacket ,		   step,	   0, "1"
HKR, NDI\Params\*JumboPacket ,		   Base,	   0, "10"
HKR, NDI\Params\*JumboPacket ,		   type,	   0, "int"
HKR, "", *JumboPacket ,  %FLG_ADDREG_NOCLOBBER%, "1514"

HKR, NDI\Params\*InterruptModeration,  ParamDesc, 0, "%InterruptModeration%"
HKR, NDI\Params\*InterruptModeration,  Type,      0, "enum"
HKR, NDI\Params\*InterruptModeration,  Default,   0, "0"
HKR, NDI\Params\*InterruptModeration,  Optional,  0, "0"
HKR, NDI\Params\*InterruptModeration\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*InterruptModeration\enum,  "1",  0, "%Enabled%"
HKR, "", *InterruptModeration, 0, "0"

;-----------------------------------------------------------------------------
;cx_vea.reg - parameters only for virtual ethernet adapters
;
[cx_vea.reg]
HKR, NDI\Params\*ReceiveBuffers,  ParamDesc, 0, "%RecvRingSize%"
HKR, NDI\Params\*ReceiveBuffers,  default,	  0, "512"
HKR, NDI\Params\*ReceiveBuffers,  min,	   0, "256"
HKR, NDI\Params\*ReceiveBuffers,  max,	   0, "4096"
HKR, NDI\Params\*ReceiveBuffers,  step,    0, "1"
HKR, NDI\Params\*ReceiveBuffers,  Base,    0, "10"
HKR, NDI\Params\*ReceiveBuffers,  type,    0, "int"
HKR, "", *ReceiveBuffers, 0, "512"

HKR, NDI\Params\*TransmitBuffers,  ParamDesc, 0, "%SendRingSize%"
HKR, NDI\Params\*TransmitBuffers,  default,   0, "2048"
HKR, NDI\Params\*TransmitBuffers,  min,    0, "256"
HKR, NDI\Params\*TransmitBuffers,  max,    0, "4096"
HKR, NDI\Params\*TransmitBuffers,  step,	0, "1"
HKR, NDI\Params\*TransmitBuffers,  Base,	0, "10"
HKR, NDI\Params\*TransmitBuffers,  type,	0, "int"
HKR, "", *TransmitBuffers,	%FLG_ADDREG_NOCLOBBER%, "2048"

HKR, NDI\Params\*InterruptModeration,  ParamDesc, 0, "%InterruptModeration%"
HKR, NDI\Params\*InterruptModeration,  Type,      0, "enum"
HKR, NDI\Params\*InterruptModeration,  Default,   0, "1"
HKR, NDI\Params\*InterruptModeration,  Optional,  0, "0"
HKR, NDI\Params\*InterruptModeration\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*InterruptModeration\enum,  "1",  0, "%Enabled%"
HKR, "", *InterruptModeration, %FLG_ADDREG_NOCLOBBER%, "1"

;-----------------------------------------------------------------------------
; ConnectX-3 specific registry keys for PF
;
[cx3_pf.reg]
HKR, NDI\Params\*QOS,  ParamDesc, 0, "%QOS%"
HKR, NDI\Params\*QOS,  Type,      0, "enum"
HKR, NDI\Params\*QOS,  Default,   0, "1"
HKR, NDI\Params\*QOS,  Optional,  0, "0"
HKR, NDI\Params\*QOS\enum,  "0",  0, "%Disabled%"
HKR, NDI\Params\*QOS\enum,  "1",  0, "%Enabled%"
HKR, "", *QOS, %FLG_ADDREG_NOCLOBBER%, "1"


;-----------------------------------------------------------------------------
; ConnectX-3 specific registry keys for VF
;
[cx3_vf.reg]

;------------------------------------------------------------------------------
;ConnectX-3 Pro specific registry keys
;
[cx3Pro.reg]
HKR, Ndi\Params\*EncapsulatedPacketTaskOffload,  ParamDesc, 0, "%EncapsulatedPacketTaskOffload%"
HKR, Ndi\Params\*EncapsulatedPacketTaskOffload,  Type,      0, "enum"
HKR, Ndi\Params\*EncapsulatedPacketTaskOffload,  Default,   0, "1"
HKR, Ndi\Params\*EncapsulatedPacketTaskOffload,  Optional,  0, "0"
HKR, Ndi\Params\*EncapsulatedPacketTaskOffload\enum,  "0",  0, "%Disabled%"
HKR, Ndi\Params\*EncapsulatedPacketTaskOffload\enum,  "1",  0, "%Enabled%"
HKR, "", *EncapsulatedPacketTaskOffload, 0, "1"


[virt.reg]

;-------------------------------
; SRIOV Default switch registry keys.
;
HKR, NicSwitches\0, *SwitchId,   %REG_DWORD_NO_CLOBBER%, 0
HKR, NicSwitches\0, *SwitchName, %FLG_ADDREG_NOCLOBBER%, “%DefaultSwitchName%”
HKR, NicSwitches\0, *SwitchType,   %REG_DWORD_NO_CLOBBER%, 1
HKR, NicSwitches\0, *Flags,   %REG_DWORD_NO_CLOBBER%, 0
HKR, NicSwitches\0, *NumVFs, 0, 128

HKR, Ndi\Params\*Sriov,      paramDesc, , %Sriov%
HKR, Ndi\Params\*Sriov,      type,      , "enum"
HKR, Ndi\Params\*Sriov\enum, 0,         , %Disabled%
HKR, Ndi\Params\*Sriov\enum, 1,         , %Enabled%
HKR, "", *SRIOV, %FLG_ADDREG_NOCLOBBER%, "1"

HKR, Ndi\Params\*VMQ,  ParamDesc, 0, "%VMQ%"
HKR, Ndi\Params\*VMQ,  Type,      0, "enum"
HKR, Ndi\Params\*VMQ,  Default,   0, "1"
HKR, Ndi\Params\*VMQ,  Optional,  0, "0"
HKR, Ndi\Params\*VMQ\enum,  "0",  0, "%Disabled%"
HKR, Ndi\Params\*VMQ\enum,  "1",  0, "%Enabled%"
HKR, "", *VMQ, %FLG_ADDREG_NOCLOBBER%, "1"

HKR, Ndi\Params\*VMQVlanFiltering,  ParamDesc, 0, "%VMQVlanFiltering%"
HKR, Ndi\Params\*VMQVlanFiltering,  Type,	  0, "enum"
HKR, Ndi\Params\*VMQVlanFiltering,  Default,   0, "1"
HKR, Ndi\Params\*VMQVlanFiltering,  Optional,  0, "0"
HKR, Ndi\Params\*VMQVlanFiltering\enum,	"0",  0, "%Disabled%"
HKR, Ndi\Params\*VMQVlanFiltering\enum,	"1",  0, "%Enabled%"
HKR, "", *VMQVlanFiltering, %FLG_ADDREG_NOCLOBBER%, "1"

;-----------------------------------------------------------------------------
; delete unused keys
;

[cx_del.reg]
HKR, Ndi\Params\UseDma
HKR, "", UseDma

HKR, Ndi\Params\TxRingNum
HKR, "", TxRingNum

HKR, NDI\Params\SendIntModCount
HKR, "", SendIntModCount

HKR, NDI\Params\SendIntModTime
HKR, "", SendIntModTime

HKR, NDI\Params\SendCompletionMethod
HKR, "", SendCompletionMethod

HKR, NDI\Params\SendPollingModCount
HKR, "", SendPollingModCount

HKR, NDI\Params\SendPollingModTime
HKR, "", SendPollingModTime

HKR, NDI\Params\RecvIntModCount
HKR, "", RecvIntModCount

HKR, NDI\Params\RecvIntModTime
HKR, "", RecvIntModTime

HKR, NDI\Params\AcceptGREbyOuterMAC
HKR, "", AcceptGREbyOuterMAC

HKR, NDI\Params\*HeaderDataSplit
HKR, "", *HeaderDataSplit

HKR, NDI\Params\*RssMaxProcNumber

HKR, "", *VMQLookaheadSplit

HKR, "", MaxNumberOfPacketsToIndicateThread
HKR, "", MaxNumberOfPacketsToIndicateDPC
HKR, "", InterupptToThreadThreshold
HKR, "", rx_usecs_low
HKR, "", rx_usecs_high
HKR, "", UseRSSForRawIP
HKR, "", UseRSSForUDP
HKR, "", LSOSize
HKR, "", BlueFlame
HKR, "", MaxNumOfMCList

HKR,"",AverageFactor
HKR,"",AveragePollThreshold
HKR,"",ThisPollThreshold
HKR,"",pkt_rate_low
HKR,"",pkt_rate_high
HKR,"",SingleStream
HKR,"",RxSmallPacketBypass
HKR,"",TxHashDisrtibution
HKR,"",TxForwardingProcessor
HKR,"",DefaultRecvRingProcessor
HKR,"",TxInterruptProcessor

HKR,"",NdkWithGlobalPause

[cx_vf_del.reg]
HKR, NDI\Params\*PriorityVLANTag

HKR, NDI\Params\VlanID
HKR, "", VlanID

HKR, NDI\Params\*FlowControl
HKR, "", *FlowControl

HKR, NDI\Params\*QOS
HKR, "", *QOS

HKR, NDI\Params\*NetworkDirect
HKR, "", *NetworkDirect

HKR, NDI\Params\RoceMaxFrameSize
HKR, "", RoceMaxFrameSize

[Ibbus_del.ParamsReg]
HKR,"Parameters",NdkDebugLevel
HKR,"Parameters",NdkDebugFlags
HKR,"Parameters",ModeFlags

;-----------------------------------------------------------------------------
; mlx4eth NT specific
;
[bindings.reg]
; use ndis5 as the upper bound because NT supports it
HKR, Ndi,                       Service,    0, "mlx4eth63"
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet,MLNX"

[vf_bindings.reg]
; use ndis5 as the upper bound because NT supports it
HKR, Ndi,                       Service,    0, "mlx4eth63"
HKR, Ndi\Interfaces,            UpperRange, 0, "ndisvf"
HKR, Ndi\Interfaces,            LowerRange, 0, "iovvf"

[mlx4eth63.reg]

;*NetworkDirect shadow value
HKR, "", NetworkDirectShadow, %FLG_ADDREG_NOCLOBBER%, "1"

[WinCtxTune_reg]
HKR,,icon,,"-5"
HKR,,EnumPropPages32,,"winctxtune_eth.dll,WinCtxTunePropPageProvider"

[mlx4eth63.Service]
DisplayName     = %mlx4eth63.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType		= 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\mlx4eth63.sys
LoadOrderGroup  = NDIS
AddReg          = Ibbus.ParamsReg
DelReg          = Ibbus_del.ParamsReg
AddReg			= BootFlags.ParamsReg

[Ibbus.ParamsReg]
HKR,"Parameters","NdkModeFlags",%REG_DWORD_NO_CLOBBER%,0x00000001
HKR,"Parameters","ModeFlags",%REG_DWORD_NO_CLOBBER%,0x00000001

[BootFlags.ParamsReg]
HKR,,BootFlags,0x00010003,0x1 ; CM_SERVICE_NETWORK_BOOT_LOAD

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\drivers\mlx4eth63.sys;%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;-----------------------------------------------------------------------------
; DestinationDirs
;

[DestinationDirs]
mlx4eth63.CopyFiles    = 12
Wctxtune.CopyFiles     = 11
[mlx4eth63.CopyFiles]
mlx4eth63.sys,,,2


[Wctxtune.CopyFiles]
winctxtune_eth.dll,,,2




[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %DiskDescription%,mlx4eth63.sys,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
mlx4eth63.sys = 1,, ; on distribution disk 1
winctxtune_eth.dll = 1


[Strings]
Mellanox                 = "Mellanox Technologies Ltd."
MSFT                     = "Microsoft Corporation"
IgnoreFCS				 = "Ignore FCS errors"
ReceiveFrameDescriptors  = "Receive Frame Descriptors"
TransmitControlBlocks    = "Transmit Control Blocks"
Disabled                 = "Disabled"
Enabled                  = "Enabled"
MaxFrameSize             = "Jumbo Packet"
RxBufferAlignment        = "Rx Buffer Alignment"
EncapOverhead			 = "Encapsulation Overhead"
ThreadPoll				 = "Number of Polls on Receive"
ND_STR                   = "NetworkDirect Functionality"
RecvCompletionMethod	 = "Receive Completion Method"
RecvRingSize             = "Receive Buffers"
SendRingSize             = "Send Buffers"
Polling                  = "Polling"
Interrupts               = "Interrupts"
Adaptive                 = "Adaptive"
No_rebalnce              = "Disabled"
NDIS_RSS                 = "Enabled"
RssMode                  = "Receive Side Scaling"
NumaNodeId               = "Preferred NUMA node"
NumaNodeId_default       = "Default Settings"
node0                    = "Node 0"
node1                    = "Node 1"
node2                    = "Node 2"
node3                    = "Node 3"
node4                    = "Node 4"
node5                    = "Node 5"
node6                    = "Node 6"
node7                    = "Node 7"
RssBaseProcNumber        = "RSS Base Processor Number"
MaxRssProcessors         = "Maximum number of RSS Processors"
NumRSSQueues              = "Maximum Number of RSS Queues"
RscIPv4                   = "Recv Segment Coalescing (IPv4)"
RscIPv6                   = "Recv Segment Coalescing (IPv6)"
RssProfile                = "RSS load balancing Profile"
Closest_Processor         = "ClosestProcessor"
Closest_Processor_Static  = "ClosestProcessorStatic"
Numa_Scaling              = "NumaScaling"
Numa_Scaling_Static       = "NumaScalingStatic"
Conservative_Scaling      = "ConservativeScaling"
FailOver                 = "Fail Over"
RxIntModeration		 	 = "Rx Interrupt Moderation Type"
Static                   = "Static"
FlowControl              = "Flow Control"
InterruptModeration      = "Interrupt Moderation"
TxEnabled				 = "Tx Enabled"
RxEnabled				 = "Rx Enabled"
TxRxEnabled				 = "Rx & Tx Enabled"
IPChecksumOffloadIPv4    = "IPV4 Checksum Offload"
TCPUDPChecksumOffloadIPv4= "TCP/UDP Checksum Offload (IPv4)"
TCPUDPChecksumOffloadIPv6= "TCP/UDP Checksum Offload (IPv6)"
LsoV2IPv4		 = "Large Send Offload V2 (IPv4)"
LsoV2IPv6		 = "Large Send Offload V2 (IPv6)"

PriorityVLANTag          = "Priority & Vlan Tag"
PriorityVlanDisabled     = "Priority & VLAN Disabled"
PriorityEnabled          = "Priority Enabled"
VlanEnabled              = "VLAN Enabled"
PriorityVlanEnabled      = "Priority & VLAN Enabled"
VlanID					 = "VLAN ID"
NetworkAddress			 = "Locally Administered Address"

QOS                      = "Quality Of Service"
VMQ 					 = "Virtual Machine Queues"
VMQVlanFiltering		 = "VMQ VLAN Filtering"
RoceMaxFrameSize         = "R/RoCE Max Frame Size"
MaxSizeWithinMaxFramSize = "Auto"

EncapsulatedPacketTaskOffload = "Encapsulated Task Offload"








SwitchName		 = "Name of the default NIC switch"
DefaultSwitchName        = "Default Switch"
SwitchId		 = "Id of the default NIC switch"
SwitchType		 = "Type of the default NIC switch"
SwitchFlags		 = "Flags of the default NIC switch"
SwitchNumVFs		 = "Number of VFs of the default NIC switch"
Sriov			 = "SR-IOV"




mlx4eth63_CX.DeviceDesc    = "Mellanox ConnectX Ethernet Adapter"
mlx4eth63_CX2.DeviceDesc   = "Mellanox ConnectX-2 Ethernet Adapter"
mlx4eth63_CX3.DeviceDesc   = "Mellanox ConnectX-3 Ethernet Adapter"
mlx4eth63_CX3Pro.DeviceDesc = "Mellanox ConnectX-3 Pro Ethernet Adapter"
mlx4eth63_vCX3.DeviceDesc  = "Mellanox ConnectX-3 Virtual Function Ethernet Adapter"

mlx4eth63_CX3_VEA.DeviceDesc	= "Mellanox ConnectX-3 Virtual Ethernet Adapter"
mlx4eth63_CX3Pro_VEA.DeviceDesc = "Mellanox ConnectX-3 Pro Virtual Ethernet Adapter"

;;;;; cards of other companies
mlx4eth63_CX3Pro.801f.DeviceDesc = "HP Ethernet 10G 2-port 546SFP+ Adapter"
mlx4eth63_CX3Pro.8020.DeviceDesc = "HP Ethernet 10G 2-port 546FLR-SFP+ Adapter"
mlx4eth63_vCX3.801f.DeviceDesc = "HP Ethernet 10G 2-port 546SFP+ Virtual Ethernet Adapter"
mlx4eth63_vCX3.8020.DeviceDesc = "HP Ethernet 10G 2-port 546FLR-SFP+ Virtual Ethernet Adapter"
mlx4eth63_CX3Pro_VEA.801f.DeviceDesc = "HP Ethernet 10G 2-port 546SFP+ Virtual Ethernet Adapter"
mlx4eth63_CX3Pro_VEA.8020.DeviceDesc = "HP Ethernet 10G 2-port 546FLR-SFP+ Virtual Ethernet Adapter"
mlx4eth63_CX3_VEA.18cd.DeviceDesc = "HP 10Gb 2-port 544FLR-QSFP Virtual Ethernet Adapter"
mlx4eth63_CX3.18cd.DeviceDesc  = "HP 10Gb 2-port 544FLR-QSFP Ethernet Adapter"
mlx4eth63_vCX3.18cd.DeviceDesc  = "HP 10Gb 2-port 544FLR-QSFP Virtual Ethernet Adapter"

mlx4eth63_CX3Pro.22f1.DeviceDesc  = "HP InfiniBand QDR/Ethernet 10Gb 2-port 544+M Ethernet Adapter"
mlx4eth63_vCX3Pro.22f1.DeviceDesc  = "HP InfiniBand QDR/Ethernet 10Gb 2-port 544+M Virtual Ethernet Adapter"
mlx4eth63_CX3Pro.22f2.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+M Ethernet Adapter"
mlx4eth63_vCX3Pro.22f2.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+M Virtual Ethernet Adapter"
mlx4eth63_CX3Pro.22f3.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+QSFP Ethernet Adapter"
mlx4eth63_vCX3Pro.22f3.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+QSFP Virtual Ethernet Adapter"
mlx4eth63_CX3Pro.22f4.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+FLR-QSFP Ethernet Adapter"
mlx4eth63_vCX3Pro.22f4.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+FLR-QSFP Virtual Ethernet Adapter"
mlx4eth63_CX3Pro.22f5.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb 2-port 544+FLR-QSFP Ethernet Adapter"
mlx4eth63_vCX3Pro.22f5.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb 2-port 544+FLR-QSFP Virtual Ethernet Adapter"
; VEA
mlx4eth63_CX3_VEA.22f1.DeviceDesc  = "HP InfiniBand QDR/Ethernet 10Gb 2-port 544+M Virtual Ethernet Adapter"
mlx4eth63_CX3_VEA.22f2.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+M Virtual Ethernet Adapter"
mlx4eth63_CX3_VEA.22f3.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+QSFP Virtual Ethernet Adapter"
mlx4eth63_CX3_VEA.22f4.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb/40Gb 2-port 544+FLR-QSFP Virtual Ethernet Adapter"
mlx4eth63_CX3_VEA.22f5.DeviceDesc  = "HP InfiniBand FDR/Ethernet 10Gb 2-port 544+FLR-QSFP Virtual Ethernet Adapter"

; Cards for ATTO Inc. description
mlx4eth63_CX3Pro.0090.DeviceDesc  = "ATTO FastFrame NQ41 Ethernet Adapter"
mlx4eth63_CX3Pro.0091.DeviceDesc  = "ATTO FastFrame NQ42 Ethernet Adapter"
mlx4eth63_CX3Pro.0092.DeviceDesc  = "ATTO FastFrame NQ11 Ethernet Adapter"
mlx4eth63_CX3Pro.0093.DeviceDesc  = "ATTO FastFrame NQ12 Ethernet Adapter"

;VEA for ATTO
mlx4eth63_CX3Pro_VEA.0090.DeviceDesc  = "ATTO FastFrame NQ41 Virtual Ethernet Adapter"
mlx4eth63_CX3Pro_VEA.0091.DeviceDesc  = "ATTO FastFrame NQ42 Virtual Ethernet Adapter"
mlx4eth63_CX3Pro_VEA.0092.DeviceDesc  = "ATTO FastFrame NQ11 Virtual Ethernet Adapter"
mlx4eth63_CX3Pro_VEA.0093.DeviceDesc  = "ATTO FastFrame NQ12 Virtual Ethernet Adapter"


mlx4eth63.Service.DispName = "Mellanox ConnectX based Ethernet Adapter (NDIS 6.3) Driver"
DiskDescription 	  = "Mellanox Driver Disk 1"

RxIntModerationProfile         = "Rx Interrupt Moderation Profile"
TxIntModerationProfile         = "Tx Interrupt Moderation Profile"
LowLatency                = "Low Latency"
Moderate                  = "Moderate"
Aggressive                = "Aggressive"

TxBwPrecedence			= "Tx Throughput Port Arbiter"
Default					= "Best Effort (Default)"
Precending				= "Guaranteed"

REG_MULTI_SZ              = 0x00010000
REG_DWORD                 = 0x00010001
REG_DWORD_NO_CLOBBER	  = 0x00010003
FLG_ADDREG_NOCLOBBER      = 0x00000002

