; ************************************************************
; ************************************************************
; **  Filename: ValleyView2System.inf                       **
; **  Abstract: Assigns the null driver to devices          **
; **            for yellow-bang removal and                 **
; **            brands Intel(R) devices                     ** 
; ************************************************************
; ************************************************************

[Version]
Signature=$WINDOWS NT$
Class=System
ClassGUID={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
CatalogFile=ValleyView2.cat
DriverVer=07/18/1968, 10.1.3.1

[SourceDisksNames]

[SourceDisksFiles]

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=INTEL,NTx86,NTamd64,NTx86.6.1,NTamd64.6.1,NTx86.6.3.1,NTamd64.6.3.1

[INTEL.NTx86]
%PCI\VEN_8086&DEV_0F00Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F00
%ACPI\VEN_8086&DEV_0F06Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F06
%ACPI\VEN_8086&DEV_0F0EDesc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F0E
%PCI\VEN_8086&DEV_0F12Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F12
%PCI\VEN_8086&DEV_0F1CDesc%=Needs_ISAPNP_DRV,PCI\VEN_8086&DEV_0F1C
%ACPI\VEN_8086&DEV_0F40Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F40
%ACPI\VEN_8086&DEV_0F41Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F41
%ACPI\VEN_8086&DEV_0F42Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F42
%ACPI\VEN_8086&DEV_0F43Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F43
%ACPI\VEN_8086&DEV_0F44Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F44
%ACPI\VEN_8086&DEV_0F45Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F45
%ACPI\VEN_8086&DEV_0F46Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F46
%ACPI\VEN_8086&DEV_0F47Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F47
%PCI\VEN_8086&DEV_0F48Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F48
%PCI\VEN_8086&DEV_0F4ADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4A
%PCI\VEN_8086&DEV_0F4CDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4C
%PCI\VEN_8086&DEV_0F4EDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4E

[INTEL.NTx86.6.1]
%PCI\VEN_8086&DEV_0F00Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F00
%ACPI\VEN_8086&DEV_0F06Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F06
%ACPI\VEN_8086&DEV_0F08Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F08
%ACPI\VEN_8086&DEV_0F09Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F09
%ACPI\VEN_8086&DEV_0F0EDesc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F0E
%PCI\VEN_8086&DEV_0F12Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F12
%PCI\VEN_8086&DEV_0F1CDesc%=Needs_ISAPNP_DRV,PCI\VEN_8086&DEV_0F1C
%ACPI\VEN_8086&DEV_0F40Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F40
%ACPI\VEN_8086&DEV_0F41Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F41
%ACPI\VEN_8086&DEV_0F42Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F42
%ACPI\VEN_8086&DEV_0F43Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F43
%ACPI\VEN_8086&DEV_0F44Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F44
%ACPI\VEN_8086&DEV_0F45Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F45
%ACPI\VEN_8086&DEV_0F46Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F46
%ACPI\VEN_8086&DEV_0F47Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F47
%PCI\VEN_8086&DEV_0F48Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F48
%PCI\VEN_8086&DEV_0F4ADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4A
%PCI\VEN_8086&DEV_0F4CDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4C
%PCI\VEN_8086&DEV_0F4EDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4E

[INTEL.NTx86.6.3.1]
%PCI\VEN_8086&DEV_0F00Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F00
%ACPI\VEN_8086&DEV_0F06Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F06
%ACPI\VEN_8086&DEV_0F0EDesc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F0E
%PCI\VEN_8086&DEV_0F12Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F12
%PCI\VEN_8086&DEV_0F1CDesc%=Needs_ISAPNP_DRV,PCI\VEN_8086&DEV_0F1C
%ACPI\VEN_8086&DEV_0F40Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F40
%ACPI\VEN_8086&DEV_0F41Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F41
%ACPI\VEN_8086&DEV_0F42Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F42
%ACPI\VEN_8086&DEV_0F43Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F43
%ACPI\VEN_8086&DEV_0F44Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F44
%ACPI\VEN_8086&DEV_0F45Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F45
%ACPI\VEN_8086&DEV_0F46Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F46
%ACPI\VEN_8086&DEV_0F47Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F47
%PCI\VEN_8086&DEV_0F48Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F48
%PCI\VEN_8086&DEV_0F4ADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4A
%PCI\VEN_8086&DEV_0F4CDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4C
%PCI\VEN_8086&DEV_0F4EDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4E

[INTEL.NTamd64]
%PCI\VEN_8086&DEV_0F00Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F00
%ACPI\VEN_8086&DEV_0F06Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F06
%ACPI\VEN_8086&DEV_0F0EDesc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F0E
%PCI\VEN_8086&DEV_0F12Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F12
%PCI\VEN_8086&DEV_0F1CDesc%=Needs_ISAPNP_DRV,PCI\VEN_8086&DEV_0F1C
%ACPI\VEN_8086&DEV_0F40Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F40
%ACPI\VEN_8086&DEV_0F41Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F41
%ACPI\VEN_8086&DEV_0F42Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F42
%ACPI\VEN_8086&DEV_0F43Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F43
%ACPI\VEN_8086&DEV_0F44Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F44
%ACPI\VEN_8086&DEV_0F45Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F45
%ACPI\VEN_8086&DEV_0F46Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F46
%ACPI\VEN_8086&DEV_0F47Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F47
%PCI\VEN_8086&DEV_0F48Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F48
%PCI\VEN_8086&DEV_0F4ADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4A
%PCI\VEN_8086&DEV_0F4CDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4C
%PCI\VEN_8086&DEV_0F4EDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4E

[INTEL.NTamd64.6.1]
%PCI\VEN_8086&DEV_0F00Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F00
%ACPI\VEN_8086&DEV_0F06Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F06
%ACPI\VEN_8086&DEV_0F08Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F08
%ACPI\VEN_8086&DEV_0F09Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F09
%ACPI\VEN_8086&DEV_0F0EDesc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F0E
%PCI\VEN_8086&DEV_0F12Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F12
%PCI\VEN_8086&DEV_0F1CDesc%=Needs_ISAPNP_DRV,PCI\VEN_8086&DEV_0F1C
%ACPI\VEN_8086&DEV_0F40Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F40
%ACPI\VEN_8086&DEV_0F41Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F41
%ACPI\VEN_8086&DEV_0F42Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F42
%ACPI\VEN_8086&DEV_0F43Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F43
%ACPI\VEN_8086&DEV_0F44Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F44
%ACPI\VEN_8086&DEV_0F45Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F45
%ACPI\VEN_8086&DEV_0F46Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F46
%ACPI\VEN_8086&DEV_0F47Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F47
%PCI\VEN_8086&DEV_0F48Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F48
%PCI\VEN_8086&DEV_0F4ADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4A
%PCI\VEN_8086&DEV_0F4CDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4C
%PCI\VEN_8086&DEV_0F4EDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4E

[INTEL.NTamd64.6.3.1]
%PCI\VEN_8086&DEV_0F00Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F00
%ACPI\VEN_8086&DEV_0F06Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F06
%ACPI\VEN_8086&DEV_0F0EDesc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F0E
%PCI\VEN_8086&DEV_0F12Desc%=Needs_NO_DRV,PCI\VEN_8086&DEV_0F12
%PCI\VEN_8086&DEV_0F1CDesc%=Needs_ISAPNP_DRV,PCI\VEN_8086&DEV_0F1C
%ACPI\VEN_8086&DEV_0F40Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F40
%ACPI\VEN_8086&DEV_0F41Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F41
%ACPI\VEN_8086&DEV_0F42Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F42
%ACPI\VEN_8086&DEV_0F43Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F43
%ACPI\VEN_8086&DEV_0F44Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F44
%ACPI\VEN_8086&DEV_0F45Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F45
%ACPI\VEN_8086&DEV_0F46Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F46
%ACPI\VEN_8086&DEV_0F47Desc%=Needs_NO_DRV,ACPI\VEN_8086&DEV_0F47
%PCI\VEN_8086&DEV_0F48Desc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F48
%PCI\VEN_8086&DEV_0F4ADesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4A
%PCI\VEN_8086&DEV_0F4CDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4C
%PCI\VEN_8086&DEV_0F4EDesc%=Needs_PCI_DRV,PCI\VEN_8086&DEV_0F4E

[Needs_NO_DRV]
Include=machine.inf
Needs=NO_DRV

[Needs_NO_DRV.Services]
Include=machine.inf
Needs=NO_DRV.Services

[Needs_ISAPNP_DRV]
Include=machine.inf
Needs=ISAPNP_DRV

[Needs_ISAPNP_DRV.Services]
Include=machine.inf
Needs=ISAPNP_DRV.Services

[Needs_PCI_DRV]
Include=machine.inf
Needs=PCI_DRV

[Needs_PCI_DRV.Services]
Include=machine.inf
Needs=PCI_DRV.Services

[Needs_PCI_DRV.HW]
Include=machine.inf
Needs=PCI_DRV.HW

[Strings]
INTEL="INTEL"
PCI\VEN_8086&DEV_0F00Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor SoC Transaction Router - 0F00"
ACPI\VEN_8086&DEV_0F06Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - DMA - 0F06"
ACPI\VEN_8086&DEV_0F08Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - PWM Port 1 - 0F08"
ACPI\VEN_8086&DEV_0F09Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - PWM Port 2 - 0F09"
ACPI\VEN_8086&DEV_0F0EDesc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - SPI Port - 0F0E"
PCI\VEN_8086&DEV_0F12Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Platform Control Unit - SMBus Port - 0F12"
PCI\VEN_8086&DEV_0F1CDesc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Platform Control Unit - LPC: Bridge to Intel Legacy Block - 0F1C"
ACPI\VEN_8086&DEV_0F40Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - DMA - 0F40"
ACPI\VEN_8086&DEV_0F41Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - I2C Port 1 - 0F41"
ACPI\VEN_8086&DEV_0F42Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - I2C Port 2 - 0F42"
ACPI\VEN_8086&DEV_0F43Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - I2C Port 3 - 0F43"
ACPI\VEN_8086&DEV_0F44Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - I2C Port 4 - 0F44"
ACPI\VEN_8086&DEV_0F45Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - I2C Port 5 - 0F45"
ACPI\VEN_8086&DEV_0F46Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - I2C Port 6 - 0F46"
ACPI\VEN_8086&DEV_0F47Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor Serial IO (SIO) - I2C Port 7 - 0F47"
PCI\VEN_8086&DEV_0F48Desc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor PCI Express - Root Port 1 - 0F48"
PCI\VEN_8086&DEV_0F4ADesc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor PCI Express - Root Port 2 - 0F4A"
PCI\VEN_8086&DEV_0F4CDesc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor PCI Express - Root Port 3 - 0F4C"
PCI\VEN_8086&DEV_0F4EDesc="Intel(R) Atom(TM)/Celeron(R)/Pentium(R) Processor PCI Express - Root Port 4 - 0F4E"




; Copyright (c) 2003-2017 Intel Corporation
; 
; ********************************************************************************
; Intel is making no claims of usability, efficacy or warranty.
; ********************************************************************************
; Information in this document is provided in connection with Intel products. No
; license, express or implied, by estoppel or otherwise, to any intellectual
; property rights is granted by this document. Intel assumes no liability
; whatsoever, and Intel disclaims any express or implied warranty, relating to
; sale and/or use of Intel products including liability or warranties relating to
; fitness for a particular purpose, merchantability, or infringement of any
; patent, copyright or other intellectual property right. Intel products are not
; intended for use in medical, life saving, or life sustaining applications.
; ********************************************************************************
; Intel Corporation disclaims all warranties and liabilities for the use of this
; document and the information contained herein, and assumes no responsibility for
; any errors which may appear in this document, nor does Intel make a commitment
; to update the information contained herein. Intel reserves the right to make
; changes to this document at any time, without notice.
; ********************************************************************************
; ********************************************************************************
; 
; * Third-party brands and names are the property of their respective owners.
