;*******************************************************************************
; Copyright (c) 2002-2016 Broadcom Corporation.
;
; L2 Ndis INF.
;
; History:
;    7/1/13 havk               Inception.
;
;*******************************************************************************

[Version]
signature   = "$Windows NT$"
class       = net
classguid   = {4d36e972-e325-11ce-bfc1-08002be10318}
provider    = %brcm%
catalogfile = bnxtnd.cat
DriverVer = 04/08/2022,222.0.126.0

[manufacturer]
%brcm% = broadcom,NTx86,ntamd64

[controlflags]
excludefromselect = *

[broadcom.NTx86]
; Empty section for other OSes and architectures




[broadcom.ntamd64]
;*******************************************************************************
; Physical device ID's.
;*******************************************************************************

;*******************************************************************************
; Cumulus physical device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_16c9&subsys_020314E4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16c9&subsys_020314E4
%pci\ven_14e4&dev_16ca&subsys_040314E4.DeviceDesc% = bcm_link50_fec_x64,            pci\ven_14e4&dev_16ca&subsys_040314E4 ; 57304
%pci\ven_14e4&dev_16ca&subsys_040214E4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16ca&subsys_040214E4 ; 57304
%pci\ven_14e4&dev_16ca&subsys_040514E4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16ca&subsys_040514E4 ; 57304
%pci\ven_14e4&dev_16c9&subsys_020514E4.DeviceDesc% = bcm_link10_fec_x64,            pci\ven_14e4&dev_16c9&subsys_020514E4 ; 57302
%pci\ven_14e4&dev_16c9&subsys_020614E4.DeviceDesc% = bcm_link10_fec_x64,            pci\ven_14e4&dev_16c9&subsys_020614E4 ; 57302
%pci\ven_14e4&dev_16c9&subsys_020714E4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16c9&subsys_020714E4 ; 57302
%pci\ven_14e4&dev_16c9&subsys_020814E4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16c9&subsys_020814E4 ; 57302
%pci\ven_14e4&dev_16ca&subsys_3043108e.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16ca&subsys_3043108e ; 57304
%pci\ven_14e4&dev_16ca&subsys_040614e4.DeviceDesc% = bcm_link25_fecplus_x64_wol,    pci\ven_14e4&dev_16ca&subsys_040614e4
%pci\ven_14e4&dev_16ca&subsys_040a14e4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16ca&subsys_040a14e4
%pci\ven_14e4&dev_16ca&subsys_040414e4.DeviceDesc% = bcm_link50_fecplus_x64_wol,    pci\ven_14e4&dev_16ca&subsys_040414e4
%pci\ven_14e4&dev_16ca&subsys_414214e4.DeviceDesc% = bcm_link25_fecplus_x64_wol,    pci\ven_14e4&dev_16ca&subsys_414214e4
%pci\ven_14e4&dev_16ca&subsys_304414e4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16ca&subsys_304414e4

;*******************************************************************************
; Cumulus+ physical device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_16ce&subsys_16ce14e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16ce&subsys_16ce14e4
%pci\ven_14e4&dev_16cf&subsys_312017aa.DeviceDesc% = bcm_link25_fecplus_x64,        pci\ven_14e4&dev_16cf&subsys_312017aa
%pci\ven_14e4&dev_16cf&subsys_16cf14e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16cf&subsys_16cf14e4
%pci\ven_14e4&dev_16df&subsys_16df14e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma,   pci\ven_14e4&dev_16df&subsys_16df14e4
%pci\ven_14e4&dev_16df&subsys_140414e4.DeviceDesc% = bcm_link25_fecplus_x64,        pci\ven_14e4&dev_16df&subsys_140414e4
%pci\ven_14e4&dev_16df&subsys_120214e4.DeviceDesc% = bcm_link25_fecplus_x64,        pci\ven_14e4&dev_16df&subsys_120214e4
%pci\ven_14e4&dev_16df&subsys_140214e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16df&subsys_140214e4
%pci\ven_14e4&dev_16df&subsys_140314e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma,   pci\ven_14e4&dev_16df&subsys_140314e4
%pci\ven_14e4&dev_16e0&subsys_16e014e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16e0&subsys_16e014e4
%pci\ven_14e4&dev_16e4&subsys_16e414e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16e4&subsys_16e414e4
%pci\ven_14e4&dev_16df&subsys_4869108e.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16df&subsys_4869108e
%pci\ven_14e4&dev_16df&subsys_140514e4.DeviceDesc% = bcm_link25_fecplus_x64,        pci\ven_14e4&dev_16df&subsys_140514e4
%pci\ven_14e4&dev_16cf&subsys_120214e4.DeviceDesc% = bcm_link25_fecplus_x64_wol,    pci\ven_14e4&dev_16cf&subsys_120214e4

;*******************************************************************************
; Whitney physical device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_16d0&subsys_402014E4.DeviceDesc% = bcm_link10_fec_x64,            pci\ven_14e4&dev_16d0&subsys_402014E4 ; 57402
%pci\ven_14e4&dev_16d1&subsys_404114E4.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16d1&subsys_404114E4 ; 57404
%pci\ven_14e4&dev_16d1&subsys_312017aa.DeviceDesc% = bcm_link25_fec_x64,            pci\ven_14e4&dev_16d1&subsys_312017aa
%pci\ven_14e4&dev_16d2&subsys_060214E4.DeviceDesc% = bcm_link10_fec_x64,            pci\ven_14e4&dev_16d2&subsys_060214E4 ; 57406
%pci\ven_14e4&dev_16d2&subsys_416017aa.DeviceDesc% = bcm_link10_fec_x64,            pci\ven_14e4&dev_16d2&subsys_416017aa

;*******************************************************************************
; Whitney+ physical device ID's.
;*******************************************************************************

%pci\ven_14E4&dev_16D6&subsys_412014E4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_412014E4
%pci\ven_14E4&dev_16D6&subsys_412114E4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d6&subsys_412114E4
%pci\ven_14E4&dev_16D6&subsys_16d614E4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14E4&dev_16D6&subsys_16d614E4 ; **
%pci\ven_14e4&dev_16d7&subsys_16d714e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_16d714e4 ; **
%pci\ven_14e4&dev_16d7&subsys_414114e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_414114e4
%pci\ven_14e4&dev_16d7&subsys_140514e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_140514e4 ; 57414A0
%pci\ven_14e4&dev_16d7&subsys_414014e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_414014e4
%pci\ven_14e4&dev_16d8&subsys_416114e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d8&subsys_416114e4
%pci\ven_14e4&dev_16d8&subsys_416014e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_416014e4
%pci\ven_14e4&dev_16d8&subsys_160214e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d8&subsys_160214E4 ; 57314
%pci\ven_14e4&dev_16d8&subsys_30031259.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d8&subsys_30031259
%pci\ven_14e4&dev_16d8&subsys_416017aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,        pci\ven_14e4&dev_16d8&subsys_416017aa
%pci\ven_14e4&dev_16d8&subsys_416117aa.DeviceDesc% = bcm_link10_fecplus_x64,        pci\ven_14e4&dev_16d8&subsys_416117aa
%pci\ven_14E4&dev_16d8&subsys_1feb1028.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14E4&dev_16d8&subsys_1feb1028
%pci\ven_14e4&dev_16d8&subsys_16d814e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d8&subsys_16d814e4 ; **
%pci\ven_14e4&dev_16d9&subsys_16d914e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d9&subsys_16d914e4 ; **
%pci\ven_14e4&dev_16e2&subsys_16e214e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16e2&subsys_16e214e4 ; **
%pci\ven_14e4&dev_16e3&subsys_16e314e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16e3&subsys_16e314e4 ; **
%pci\ven_14e4&dev_16d9&subsys_4866108e.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d9&subsys_4866108e
%pci\ven_14e4&dev_16e2&subsys_4866108e.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16e2&subsys_4866108e
%pci\ven_14e4&dev_16d8&subsys_1fea1028.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_1fea1028 ; **
%pci\ven_14e4&dev_16d8&subsys_07e51028.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_07e51028 ; **
%pci\ven_14e4&dev_16d6&subsys_412017aa.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d6&subsys_412017aa
%pci\ven_14e4&dev_16d7&subsys_140314e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_140314e4
%pci\ven_14e4&dev_16d7&subsys_140214e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_140214e4
%pci\ven_14e4&dev_16d7&subsys_140414e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_140414e4
%pci\ven_14e4&dev_16d6&subsys_120214e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d6&subsys_120214e4
%pci\ven_14e4&dev_16d7&subsys_3044108e.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_3044108e
%pci\ven_14e4&dev_16d7&subsys_4869108e.DeviceDesc% = bcm_link25_fecplus_x64_rdma,   pci\ven_14e4&dev_16d7&subsys_4869108e
%pci\ven_14e4&dev_16d7&subsys_414314e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_414314e4
%pci\ven_14e4&dev_16d6&subsys_412314e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_412314e4
%pci\ven_14e4&dev_16d6&subsys_412414e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_412414e4
%pci\ven_14e4&dev_16d6&subsys_30041259.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d6&subsys_30041259
%pci\ven_14e4&dev_16d7&subsys_414414e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_414414e4
%pci\ven_14e4&dev_16d8&subsys_416314e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,   pci\ven_14e4&dev_16d8&subsys_416314e4
%pci\ven_14e4&dev_16d7&subsys_094e15d9.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_094e15d9
%pci\ven_14e4&dev_16d7&subsys_092815d9.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_092815d9
%pci\ven_14e4&dev_16d8&subsys_099615d9.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_099615d9
%pci\ven_14e4&dev_16d8&subsys_1a0815d9.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_1a0815d9
%pci\ven_14e4&dev_16d8&subsys_1a0915d9.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_1a0915d9
%pci\ven_14e4&dev_16d8&subsys_060214E4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_060214E4
%pci\ven_14e4&dev_16d7&subsys_4877108e.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_4877108e
%pci\ven_14e4&dev_16d8&subsys_8b17152d.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_8b17152d
%pci\ven_14e4&dev_16e2&subsys_8b18152d.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16e2&subsys_8b18152d
%pci\ven_14e4&dev_16e3&subsys_8b19152d.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16e3&subsys_8b19152d
%pci\ven_14e4&dev_16d8&subsys_16d815d9.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_16d815d9
%pci\ven_14e4&dev_16d7&subsys_140714e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_140714e4
%pci\ven_14e4&dev_16d8&subsys_416514e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_416514e4
%pci\ven_14e4&dev_16d6&subsys_412514e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_412514e4
%pci\ven_14e4&dev_16d7&subsys_414514e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_414514e4
%pci\ven_14e4&dev_16d7&subsys_414614e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,       pci\ven_14e4&dev_16d7&subsys_414614e4
%pci\ven_14e4&dev_16d6&subsys_412614e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,       pci\ven_14e4&dev_16d6&subsys_412614e4
%pci\ven_14e4&dev_16d8&subsys_416614e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,       pci\ven_14e4&dev_16d8&subsys_416614e4
%pci\ven_14e4&dev_16d6&subsys_8b20152d.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_8b20152d
%pci\ven_14e4&dev_16d6&subsys_8b22152d.DeviceDesc% = bcm_link25_25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_8b22152d
%pci\ven_14e4&dev_16d7&subsys_8b21152d.DeviceDesc% = bcm_link25_25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_8b21152d
%pci\ven_14e4&dev_16d7&subsys_8b27152d.DeviceDesc% = bcm_link25_25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_8b27152d
%pci\ven_14e4&dev_16d7&subsys_1b1e15d9.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_1b1e15d9
%pci\ven_14e4&dev_16d7&subsys_1b2615d9.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_1b2615d9
%pci\ven_14e4&dev_16d7&subsys_29961259.DeviceDesc% = bcm_link40_fecplus_x64,            pci\ven_14e4&dev_16d7&subsys_29961259
%pci\ven_14e4&dev_16d8&subsys_404817aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_16d8&subsys_404817aa
%pci\ven_14e4&dev_16d8&subsys_416217aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_416217aa
%pci\ven_14e4&dev_16d7&subsys_414017aa.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_414017aa
%pci\ven_14e4&dev_16d8&subsys_416317aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_416317aa
%pci\ven_14e4&dev_16d7&subsys_410517aa.DeviceDesc% = bcm_link25_fecplus_x64_rdma,       pci\ven_14e4&dev_16d7&subsys_410517aa
%pci\ven_14e4&dev_16d8&subsys_159214e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_159214e4
%pci\ven_14e4&dev_16d8&subsys_159314e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_159314e4
%pci\ven_14e4&dev_16d6&subsys_159414e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_159414e4
%pci\ven_14e4&dev_16d6&subsys_159514e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_159514e4
%pci\ven_14e4&dev_16d7&subsys_159614e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_159614e4
%pci\ven_14e4&dev_16d7&subsys_159714e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_159714e4
%pci\ven_14e4&dev_16d8&subsys_190110d3.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_190110d3
%pci\ven_14e4&dev_16d7&subsys_1b7315d9.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_1b7315d9
%pci\ven_14e4&dev_16d7&subsys_8b28152d.DeviceDesc% = bcm_link10_10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_8b28152d
%pci\ven_14e4&dev_16d8&subsys_10001458.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_10001458
%pci\ven_14e4&dev_16d7&subsys_16d715d9.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_16d715d9
%pci\ven_14e4&dev_16d8&subsys_202018d4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_202018d4
%pci\ven_14e4&dev_16d7&subsys_1033193d.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d7&subsys_1033193d
%pci\ven_14e4&dev_16d6&subsys_1024193d.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d6&subsys_1024193d
%pci\ven_14e4&dev_16d8&subsys_405117aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,   pci\ven_14e4&dev_16d8&subsys_405117aa


;*******************************************************************************
; Stratus physical device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_16f1&subsys_16f114e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_nots,     pci\ven_14e4&dev_16f1&subsys_16f114e4
%pci\ven_14e4&dev_16f1&subsys_452014e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma_nots,      pci\ven_14e4&dev_16f1&subsys_452014e4
%pci\ven_14e4&dev_1614&subsys_454014e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_nots,     pci\ven_14e4&dev_1614&subsys_454014e4
%pci\ven_14e4&dev_1614&subsys_454114e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_nots,     pci\ven_14e4&dev_1614&subsys_454114e4
%pci\ven_14e4&dev_1614&subsys_8b11152d.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol_nots,  pci\ven_14e4&dev_1614&subsys_8b11152d
%pci\ven_14e4&dev_1614&subsys_410017aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol_nots,  pci\ven_14e4&dev_1614&subsys_410017aa
%pci\ven_14e4&dev_1614&subsys_410217aa.DeviceDesc% = bcm_link25_fecplus_x64_rdma_wol_nots,  pci\ven_14e4&dev_1614&subsys_410217aa
%pci\ven_14e4&dev_1614&subsys_410117aa.DeviceDesc% = bcm_link25_fecplus_x64_rdma_nots,      pci\ven_14e4&dev_1614&subsys_410117aa
%pci\ven_14e4&dev_1614&subsys_404717aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_nots,      pci\ven_14e4&dev_1614&subsys_404717aa
%pci\ven_14e4&dev_1614&subsys_1b2715d9.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol_nots, pci\ven_14e4&dev_1614&subsys_1b2715d9
%pci\ven_14e4&dev_1614&subsys_d34014e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_nots,      pci\ven_14e4&dev_1614&subsys_d34014e4
%pci\ven_14e4&dev_1614&subsys_d14014e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_nots,      pci\ven_14e4&dev_1614&subsys_d14014e4

;*******************************************************************************
; Stingray physical device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_16f0&subsys_16f014e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_16f0&subsys_16f014e4
%pci\ven_14e4&dev_d802&subsys_802014e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma,      pci\ven_14e4&dev_d802&subsys_802014e4
%pci\ven_14e4&dev_d802&subsys_d80214e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma,      pci\ven_14e4&dev_d802&subsys_d80214e4
%pci\ven_14e4&dev_d804&subsys_d80414e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_d804&subsys_d80414e4
%pci\ven_14e4&dev_d802&subsys_802114e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,      pci\ven_14e4&dev_d802&subsys_802114e4
%pci\ven_14e4&dev_d802&subsys_802414e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,      pci\ven_14e4&dev_d802&subsys_802414e4
%pci\ven_14e4&dev_d802&subsys_802814e4.DeviceDesc% = bcm_link25_fecplus_x64_rdma,      pci\ven_14e4&dev_d802&subsys_802814e4
%pci\ven_14e4&dev_d804&subsys_804014e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_d804&subsys_804014e4
%pci\ven_14e4&dev_d802&subsys_802314e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,      pci\ven_14e4&dev_d802&subsys_802314e4
%pci\ven_14e4&dev_d802&subsys_802314e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,      pci\ven_14e4&dev_d802&subsys_802314e4


;*******************************************************************************
; Thor physical device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_1752&subsys_100014e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,      pci\ven_14e4&dev_1752&subsys_100014e4
%pci\ven_14e4&dev_1751&subsys_112814e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1751&subsys_112814e4
%pci\ven_14e4&dev_1751&subsys_111614e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1751&subsys_111614e4
%pci\ven_14e4&dev_1750&subsys_175014e4.DeviceDesc% = bcm_link200_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_175014e4 ; 57508
%pci\ven_14e4&dev_1751&subsys_175114e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1751&subsys_175114e4 ; 57504
%pci\ven_14e4&dev_1752&subsys_175214e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma,      pci\ven_14e4&dev_1752&subsys_175214e4 ; 57502
%pci\ven_14e4&dev_1751&subsys_504514e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_504514e4
%pci\ven_14e4&dev_1751&subsys_504614e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_504614e4
%pci\ven_14e4&dev_1751&subsys_504914e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_504914e4
%pci\ven_14e4&dev_1752&subsys_541014e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1752&subsys_541014e4
%pci\ven_14e4&dev_1752&subsys_100214e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,      pci\ven_14e4&dev_1752&subsys_100214e4
%pci\ven_14e4&dev_1752&subsys_100314e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma,      pci\ven_14e4&dev_1752&subsys_100314e4
%pci\ven_14e4&dev_1750&subsys_520814e4.DeviceDesc% = bcm_link200_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1750&subsys_520814e4
%pci\ven_14e4&dev_1751&subsys_504714e4.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_504714e4
%pci\ven_14e4&dev_1751&subsys_504814e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_504814e4
%pci\ven_14e4&dev_1751&subsys_110014e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1751&subsys_110014e4
%pci\ven_14e4&dev_1750&subsys_210014e4.DeviceDesc% = bcm_link200_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_210014e4
%pci\ven_14e4&dev_1750&subsys_220014e4.DeviceDesc% = bcm_link200_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_220014e4
%pci\ven_14e4&dev_1751&subsys_542514e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_542514e4
%pci\ven_14e4&dev_1751&subsys_510014e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1751&subsys_510014e4
%pci\ven_14e4&dev_1752&subsys_515014e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1752&subsys_515014e4
%pci\ven_14e4&dev_1750&subsys_1b3e15d9.DeviceDesc% = bcm_link200_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1750&subsys_1b3e15d9
%pci\ven_14e4&dev_1751&subsys_525014e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_525014e4
%pci\ven_14e4&dev_1751&subsys_425014e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_425014e4
%pci\ven_14e4&dev_1750&subsys_404c17aa.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_404c17aa
%pci\ven_14e4&dev_1751&subsys_510514e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1751&subsys_510514e4
%pci\ven_14e4&dev_1751&subsys_510414e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1751&subsys_510414e4
%pci\ven_14e4&dev_1751&subsys_510114e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1751&subsys_510114e4
%pci\ven_14e4&dev_1751&subsys_510214e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1751&subsys_510214e4
%pci\ven_14e4&dev_1751&subsys_510314e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1751&subsys_510314e4
%pci\ven_14e4&dev_1752&subsys_515114e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1752&subsys_515114e4
%pci\ven_14e4&dev_1752&subsys_515214e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1752&subsys_515214e4
%pci\ven_14e4&dev_1752&subsys_515314e4.DeviceDesc% = bcm_link50_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1752&subsys_515314e4
%pci\ven_14e4&dev_1752&subsys_410017aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1752&subsys_410017aa
%pci\ven_14e4&dev_1751&subsys_410217aa.DeviceDesc% = bcm_thor25_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_410217aa
%pci\ven_14e4&dev_1751&subsys_410317aa.DeviceDesc% = bcm_link50_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_410317aa
%pci\ven_14e4&dev_1751&subsys_410117aa.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_410117aa
%pci\ven_14e4&dev_1752&subsys_404717aa.DeviceDesc% = bcm_link10_fecplus_x64_rdma,      pci\ven_14e4&dev_1752&subsys_404717aa
%pci\ven_14e4&dev_1751&subsys_09D41028.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_09D41028
%pci\ven_14e4&dev_1750&subsys_1b8115d9.DeviceDesc% = bcm_link200_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1750&subsys_1b8115d9
%pci\ven_14e4&dev_1750&subsys_520914e4.DeviceDesc% = bcm_link200_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1750&subsys_520914e4
%pci\ven_14e4&dev_1750&subsys_d12414e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_d12414e4
%pci\ven_14e4&dev_1751&subsys_d14214e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_d14214e4
%pci\ven_14e4&dev_1750&subsys_df2414e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_df2414e4
%pci\ven_14e4&dev_1751&subsys_159814e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_159814e4
%pci\ven_14e4&dev_1751&subsys_159914e4.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_159914e4
%pci\ven_14e4&dev_1750&subsys_159a14e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_159a14e4
%pci\ven_14e4&dev_1750&subsys_159b14e4.DeviceDesc% = bcm_link100_fecplus_x64_rdma,     pci\ven_14e4&dev_1750&subsys_159b14e4
%pci\ven_14e4&dev_1750&subsys_410317aa.DeviceDesc% = bcm_link100_fecplus_x64_rdma_wol, pci\ven_14e4&dev_1750&subsys_410317aa
%pci\ven_14e4&dev_1751&subsys_410717aa.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_410717aa
%pci\ven_14e4&dev_1751&subsys_405017aa.DeviceDesc% = bcm_thor25_fecplus_x64_rdma_wol,  pci\ven_14e4&dev_1751&subsys_405017aa
%pci\ven_14e4&dev_1751&subsys_0b1b1028.DeviceDesc% = bcm_thor25_fecplus_x64_rdma,      pci\ven_14e4&dev_1751&subsys_0b1b1028





;*******************************************************************************
; Whitney NPAR, Non-RoCE device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_16d4&subsys_402014E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16d4&subsys_402014E4 ; 57402
%pci\ven_14e4&dev_16d4&subsys_16d014E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16d4&subsys_16d014E4 ; **
%pci\ven_14e4&dev_16e7&subsys_16d114E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e7&subsys_16d114E4 ; **
%pci\ven_14e4&dev_16e7&subsys_404114E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e7&subsys_404114E4 ; 57404
%pci\ven_14e4&dev_16e7&subsys_040214E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e7&subsys_040214E4 ; 57404
%pci\ven_14e4&dev_16d4&subsys_040214E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16d4&subsys_040214E4 ; 57404
%pci\ven_14e4&dev_16e7&subsys_312017aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e7&subsys_312017aa
%pci\ven_14e4&dev_16e8&subsys_060214E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e8&subsys_060214E4 ; 57406
%pci\ven_14e4&dev_16e8&subsys_406014E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e8&subsys_406014E4 ; 57406
%pci\ven_14e4&dev_16e8&subsys_416017aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e8&subsys_416017aa
%pci\ven_14e4&dev_16e8&subsys_16d214e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16e8&subsys_16d214e4 ; **
%pci\ven_14e4&dev_16ea&subsys_16d514e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ea&subsys_16d514e4 ; **
%pci\ven_14e4&dev_16ea&subsys_16e914e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ea&subsys_16e914e4 ; **

;*******************************************************************************
; Whitney+ NPAR, Non-RoCE device ID's.
;*******************************************************************************

%pci\ven_14E4&dev_16de&subsys_412014E4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_412014E4
%pci\ven_14E4&dev_16de&subsys_412114E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16de&subsys_412114E4
%pci\ven_14E4&dev_16de&subsys_16d614E4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14E4&dev_16de&subsys_16d614E4 ; **
%pci\ven_14e4&dev_16ec&subsys_16d714e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_16d714e4 ; **
%pci\ven_14e4&dev_16ec&subsys_414114e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_414114e4
%pci\ven_14e4&dev_16ec&subsys_140514e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_140514e4 ; 57414A0
%pci\ven_14e4&dev_16ec&subsys_414014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_414014e4
%pci\ven_14e4&dev_16ee&subsys_416114e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_416114e4
%pci\ven_14e4&dev_16ee&subsys_416014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_416014e4
%pci\ven_14e4&dev_16ee&subsys_160214e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ee&subsys_160214E4 ; 57314
%pci\ven_14e4&dev_16ee&subsys_416017aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ee&subsys_416017aa
%pci\ven_14e4&dev_16ee&subsys_416117aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ee&subsys_416117aa
%pci\ven_14e4&dev_16ee&subsys_16d814e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ee&subsys_16d814e4 ; **
%pci\ven_14e4&dev_16ee&subsys_16e314e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ee&subsys_16e314e4 ; **
%pci\ven_14e4&dev_16ee&subsys_1fea1028.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_1fea1028
%pci\ven_14e4&dev_16ee&subsys_1feb1028.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_1feb1028
%pci\ven_14e4&dev_16ee&subsys_07e51028.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_07e51028
%pci\ven_14e4&dev_16cc&subsys_16d914e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16cc&subsys_16d914e4 ; **
%pci\ven_14e4&dev_16cc&subsys_16e214e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16cc&subsys_16e214e4 ; **
%pci\ven_14e4&dev_16cc&subsys_4866108e.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16cc&subsys_4866108e
%pci\ven_14e4&dev_16de&subsys_412017aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16de&subsys_412017aa
%pci\ven_14e4&dev_16ec&subsys_140314e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_140314e4
%pci\ven_14e4&dev_16ec&subsys_140214e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_140214e4
%pci\ven_14e4&dev_16ec&subsys_140414e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_140414e4
%pci\ven_14e4&dev_16de&subsys_120214e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16de&subsys_120214e4
%pci\ven_14e4&dev_16ec&subsys_3044108e.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_3044108e
%pci\ven_14e4&dev_16ec&subsys_4869108e.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_4869108e
%pci\ven_14e4&dev_16ec&subsys_414314e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_414314e4
%pci\ven_14e4&dev_16de&subsys_412314e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_412314e4
%pci\ven_14e4&dev_16de&subsys_412414e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_412414e4
%pci\ven_14e4&dev_16ec&subsys_414414e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_414414e4
%pci\ven_14e4&dev_16ee&subsys_416314e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ee&subsys_416314e4
%pci\ven_14e4&dev_16ec&subsys_094e15d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_094e15d9
%pci\ven_14e4&dev_16ec&subsys_092815d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_092815d9
%pci\ven_14e4&dev_16ee&subsys_099615d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_099615d9
%pci\ven_14e4&dev_16ee&subsys_1a0815d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_1a0815d9
%pci\ven_14e4&dev_16ee&subsys_1a0915d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_1a0915d9
%pci\ven_14e4&dev_16ec&subsys_4877108e.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_4877108e
%pci\ven_14e4&dev_16ee&subsys_8b17152d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_8b17152d
%pci\ven_14e4&dev_16cc&subsys_8b18152d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16cc&subsys_8b18152d
%pci\ven_14e4&dev_16ee&subsys_8b19152d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_8b19152d
%pci\ven_14e4&dev_16ee&subsys_16d815d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_16d815d9
%pci\ven_14e4&dev_16ec&subsys_140714e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_140714e4
%pci\ven_14e4&dev_16ee&subsys_416514e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_416514e4
%pci\ven_14e4&dev_16de&subsys_412514e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_412514e4
%pci\ven_14e4&dev_16ec&subsys_414514e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_414514e4
%pci\ven_14e4&dev_16ec&subsys_414614e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_414614e4
%pci\ven_14e4&dev_16de&subsys_412614e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_412614e4
%pci\ven_14e4&dev_16ee&subsys_416614e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_416614e4
%pci\ven_14e4&dev_16ec&subsys_1b1e15d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_1b1e15d9
%pci\ven_14e4&dev_16ec&subsys_1b2615d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_1b2615d9
%pci\ven_14e4&dev_16ee&subsys_404817aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_404817aa
%pci\ven_14e4&dev_16ee&subsys_416217aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_416217aa
%pci\ven_14e4&dev_16ec&subsys_414017aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_414017aa
%pci\ven_14e4&dev_16ee&subsys_416317aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_416317aa
%pci\ven_14e4&dev_16ec&subsys_410517aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ec&subsys_410517aa
%pci\ven_14e4&dev_16ee&subsys_159214e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_159214e4
%pci\ven_14e4&dev_16ee&subsys_159314e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_159314e4
%pci\ven_14e4&dev_16de&subsys_159414e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_159414e4
%pci\ven_14e4&dev_16de&subsys_159514e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_159514e4
%pci\ven_14e4&dev_16ec&subsys_159614e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_159614e4
%pci\ven_14e4&dev_16ec&subsys_159714e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_159714e4
%pci\ven_14e4&dev_16ee&subsys_190110d3.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_190110d3
%pci\ven_14e4&dev_16ec&subsys_1b7315d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_1b7315d9
%pci\ven_14e4&dev_16de&subsys_8b20152d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_8b20152d
%pci\ven_14e4&dev_16de&subsys_8b22152d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_8b22152d
%pci\ven_14e4&dev_16ec&subsys_8b21152d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_8b21152d
%pci\ven_14e4&dev_16ec&subsys_8b28152d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_8b28152d
%pci\ven_14e4&dev_16ee&subsys_10001458.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_10001458
%pci\ven_14e4&dev_16ec&subsys_16d715d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_16d715d9
%pci\ven_14e4&dev_16ee&subsys_202018d4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_202018d4
%pci\ven_14e4&dev_16ec&subsys_1033193d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ec&subsys_1033193d
%pci\ven_14e4&dev_16de&subsys_1024193d.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16de&subsys_1024193d
%pci\ven_14e4&dev_16ee&subsys_405117aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_16ee&subsys_405117aa
%pci\ven_14e4&dev_16ee&subsys_30031259.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16ee&subsys_30031259
%pci\ven_14e4&dev_16de&subsys_30041259.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_16de&subsys_30041259


;*******************************************************************************
; Stratus NPAR, Non-RoCE device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_1604&subsys_452014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_452014e4
%pci\ven_14e4&dev_1604&subsys_454014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_454014e4
%pci\ven_14e4&dev_1604&subsys_454114e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_454114e4
%pci\ven_14e4&dev_1604&subsys_16f014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_16f014e4
%pci\ven_14e4&dev_1604&subsys_16f114e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_16f114e4
%pci\ven_14e4&dev_1604&subsys_160414e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1604&subsys_160414e4
%pci\ven_14e4&dev_1604&subsys_1b2715d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1604&subsys_1b2715d9
%pci\ven_14e4&dev_1604&subsys_410017aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1604&subsys_410017aa
%pci\ven_14e4&dev_1604&subsys_410217aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1604&subsys_410217aa
%pci\ven_14e4&dev_1604&subsys_410117aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_410117aa
%pci\ven_14e4&dev_1604&subsys_404717aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_404717aa
%pci\ven_14e4&dev_1604&subsys_d34014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_d34014e4
%pci\ven_14e4&dev_1604&subsys_d14014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1604&subsys_d14014e4

;*******************************************************************************
; Stingray NPAR, Non-RoCE device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_1794&subsys_802014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1794&subsys_802014e4
%pci\ven_14e4&dev_1794&subsys_802114e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1794&subsys_802114e4
%pci\ven_14e4&dev_1794&subsys_802414e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1794&subsys_802414e4
%pci\ven_14e4&dev_1794&subsys_802814e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1794&subsys_802814e4
%pci\ven_14e4&dev_1796&subsys_804014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1796&subsys_804014e4
%pci\ven_14e4&dev_1794&subsys_802314e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1794&subsys_802314e4


;*******************************************************************************
; Thor NPAR, Non-RoCE device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_1800&subsys_100014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1800&subsys_100014e4
%pci\ven_14e4&dev_1801&subsys_112814e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_112814e4
%pci\ven_14e4&dev_1801&subsys_111614e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_111614e4
%pci\ven_14e4&dev_1802&subsys_1b3e15d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1802&subsys_1b3e15d9
%pci\ven_14e4&dev_1801&subsys_525014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_525014e4
%pci\ven_14e4&dev_1801&subsys_425014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_425014e4
%pci\ven_14e4&dev_1802&subsys_404c17aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1802&subsys_404c17aa
%pci\ven_14e4&dev_1801&subsys_510414e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_510414e4
%pci\ven_14e4&dev_1801&subsys_510114e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_510114e4
%pci\ven_14e4&dev_1801&subsys_510214e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_510214e4
%pci\ven_14e4&dev_1801&subsys_510314e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_510314e4
%pci\ven_14e4&dev_1800&subsys_515114e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_515114e4
%pci\ven_14e4&dev_1800&subsys_515214e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_515214e4
%pci\ven_14e4&dev_1800&subsys_515314e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_515314e4
%pci\ven_14e4&dev_1801&subsys_504514e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_504514e4
%pci\ven_14e4&dev_1801&subsys_504614e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_504614e4
%pci\ven_14e4&dev_1801&subsys_504914e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_504914e4
%pci\ven_14e4&dev_1800&subsys_541014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_541014e4
%pci\ven_14e4&dev_1800&subsys_100214e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_100214e4
%pci\ven_14e4&dev_1800&subsys_100314e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_100314e4
%pci\ven_14e4&dev_1802&subsys_520814e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1802&subsys_520814e4
%pci\ven_14e4&dev_1801&subsys_504714e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_504714e4
%pci\ven_14e4&dev_1801&subsys_504814e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_504814e4
%pci\ven_14e4&dev_1801&subsys_110014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_110014e4
%pci\ven_14e4&dev_1802&subsys_210014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1802&subsys_210014e4
%pci\ven_14e4&dev_1802&subsys_220014e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1802&subsys_220014e4
%pci\ven_14e4&dev_1801&subsys_542514e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_542514e4
%pci\ven_14e4&dev_1801&subsys_510514e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_510514e4
%pci\ven_14e4&dev_1801&subsys_510014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_510014e4
%pci\ven_14e4&dev_1800&subsys_515014e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_515014e4
%pci\ven_14e4&dev_1800&subsys_410017aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1800&subsys_410017aa
%pci\ven_14e4&dev_1801&subsys_410217aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_410217aa
%pci\ven_14e4&dev_1801&subsys_410317aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_410317aa
%pci\ven_14e4&dev_1801&subsys_410117aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_410117aa
%pci\ven_14e4&dev_1800&subsys_404717aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1800&subsys_404717aa
%pci\ven_14e4&dev_1801&subsys_09D41028.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_09D41028
%pci\ven_14e4&dev_1802&subsys_1b8115d9.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1802&subsys_1b8115d9
%pci\ven_14e4&dev_1802&subsys_520914e4.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1802&subsys_520914e4
%pci\ven_14e4&dev_1802&subsys_d12414e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1802&subsys_d12414e4
%pci\ven_14e4&dev_1801&subsys_d14214e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_d14214e4
%pci\ven_14e4&dev_1802&subsys_df2414e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1802&subsys_df2414e4
%pci\ven_14e4&dev_1801&subsys_159814e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_159814e4
%pci\ven_14e4&dev_1801&subsys_159914e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_159914e4
%pci\ven_14e4&dev_1802&subsys_159a14e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1802&subsys_159a14e4
%pci\ven_14e4&dev_1802&subsys_159b14e4.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1802&subsys_159b14e4
%pci\ven_14e4&dev_1802&subsys_410317aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1802&subsys_410317aa
%pci\ven_14e4&dev_1801&subsys_410717aa.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_410717aa
%pci\ven_14e4&dev_1801&subsys_405017aa.DeviceDesc% = bcm_npar_x64_wol,              pci\ven_14e4&dev_1801&subsys_405017aa
%pci\ven_14e4&dev_1801&subsys_0b1b1028.DeviceDesc% = bcm_npar_x64,                  pci\ven_14e4&dev_1801&subsys_0b1b1028


;*******************************************************************************
; Whitney+ NPAR, RoCE device ID's.
;*******************************************************************************

%pci\ven_14E4&dev_16eb&subsys_412014E4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_412014E4
%pci\ven_14E4&dev_16eb&subsys_412114E4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16eb&subsys_412114E4
%pci\ven_14E4&dev_16eb&subsys_16d614E4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14E4&dev_16eb&subsys_16d614E4 ; **
%pci\ven_14e4&dev_16ed&subsys_16d714e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_16d714e4 ; **
%pci\ven_14e4&dev_16ed&subsys_414114e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_414114e4
%pci\ven_14e4&dev_16ed&subsys_140514e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_140514e4 ; 57414A0
%pci\ven_14e4&dev_16ed&subsys_414014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_414014e4
%pci\ven_14e4&dev_16ef&subsys_416114e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_416114e4
%pci\ven_14e4&dev_16ef&subsys_416014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_416014e4
%pci\ven_14e4&dev_16ef&subsys_160214e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ef&subsys_160214E4 ; 57314
%pci\ven_14e4&dev_16ef&subsys_416017aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ef&subsys_416017aa
%pci\ven_14e4&dev_16ef&subsys_416117aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ef&subsys_416117aa
%pci\ven_14e4&dev_16ef&subsys_16d814e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ef&subsys_16d814e4 ; **
%pci\ven_14e4&dev_16ef&subsys_16e314e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ef&subsys_16e314e4 ; **
%pci\ven_14e4&dev_16ef&subsys_1fea1028.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_1fea1028
%pci\ven_14e4&dev_16ef&subsys_1feb1028.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_1feb1028
%pci\ven_14e4&dev_16ef&subsys_07e51028.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_07e51028
%pci\ven_14e4&dev_16c0&subsys_16d914e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16c0&subsys_16d914e4 ; **
%pci\ven_14e4&dev_16c0&subsys_16e214e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16c0&subsys_16e214e4 ; **
%pci\ven_14e4&dev_16c0&subsys_4866108e.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16c0&subsys_4866108e
%pci\ven_14e4&dev_16eb&subsys_412017aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16eb&subsys_412017aa
%pci\ven_14e4&dev_16ed&subsys_140314e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_140314e4
%pci\ven_14e4&dev_16ed&subsys_140214e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_140214e4
%pci\ven_14e4&dev_16ed&subsys_140414e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_140414e4
%pci\ven_14e4&dev_16eb&subsys_120214e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16eb&subsys_120214e4
%pci\ven_14e4&dev_16ed&subsys_3044108e.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_3044108e
%pci\ven_14e4&dev_16ed&subsys_4869108e.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_4869108e
%pci\ven_14e4&dev_16ed&subsys_414314e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_414314e4
%pci\ven_14e4&dev_16eb&subsys_412314e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_412314e4
%pci\ven_14e4&dev_16eb&subsys_412414e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_412414e4
%pci\ven_14e4&dev_16ed&subsys_414414e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_414414e4
%pci\ven_14e4&dev_16ef&subsys_416314e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ef&subsys_416314e4
%pci\ven_14e4&dev_16ed&subsys_094e15d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_094e15d9
%pci\ven_14e4&dev_16ed&subsys_092815d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_092815d9
%pci\ven_14e4&dev_16ef&subsys_099615d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_099615d9
%pci\ven_14e4&dev_16ef&subsys_1a0815d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_1a0815d9
%pci\ven_14e4&dev_16ef&subsys_1a0915d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_1a0915d9
%pci\ven_14e4&dev_16ed&subsys_4877108e.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_4877108e
%pci\ven_14e4&dev_16ef&subsys_8b17152d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_8b17152d
%pci\ven_14e4&dev_16c0&subsys_8b18152d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16c0&subsys_8b18152d
%pci\ven_14e4&dev_16ef&subsys_8b19152d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_8b19152d
%pci\ven_14e4&dev_16ef&subsys_16d815d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_16d815d9
%pci\ven_14e4&dev_16ed&subsys_140714e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_140714e4
%pci\ven_14e4&dev_16ef&subsys_416514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_416514e4
%pci\ven_14e4&dev_16eb&subsys_412514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_412514e4
%pci\ven_14e4&dev_16ed&subsys_414514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_414514e4
%pci\ven_14e4&dev_16ed&subsys_414614e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_414614e4
%pci\ven_14e4&dev_16eb&subsys_412614e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_412614e4
%pci\ven_14e4&dev_16ef&subsys_416614e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_416614e4
%pci\ven_14e4&dev_16ed&subsys_1b1e15d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_1b1e15d9
%pci\ven_14e4&dev_16ed&subsys_1b2615d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_1b2615d9
%pci\ven_14e4&dev_16ef&subsys_404817aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_404817aa
%pci\ven_14e4&dev_16ef&subsys_416217aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_416217aa
%pci\ven_14e4&dev_16ed&subsys_414017aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_414017aa
%pci\ven_14e4&dev_16ef&subsys_416317aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_416317aa
%pci\ven_14e4&dev_16ed&subsys_410517aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ed&subsys_410517aa
%pci\ven_14e4&dev_16ef&subsys_159214e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_159214e4
%pci\ven_14e4&dev_16ef&subsys_159314e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_159314e4
%pci\ven_14e4&dev_16eb&subsys_159414e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_159414e4
%pci\ven_14e4&dev_16eb&subsys_159514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_159514e4
%pci\ven_14e4&dev_16ed&subsys_159614e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_159614e4
%pci\ven_14e4&dev_16ed&subsys_159714e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_159714e4
%pci\ven_14e4&dev_16ef&subsys_190110d3.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_190110d3
%pci\ven_14e4&dev_16ed&subsys_1b7315d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_1b7315d9
%pci\ven_14e4&dev_16eb&subsys_8b20152d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_8b20152d
%pci\ven_14e4&dev_16eb&subsys_8b22152d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_8b22152d
%pci\ven_14e4&dev_16ed&subsys_8b21152d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_8b21152d
%pci\ven_14e4&dev_16ed&subsys_8b28152d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_8b28152d
%pci\ven_14e4&dev_16ef&subsys_10001458.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_10001458
%pci\ven_14e4&dev_16ed&subsys_16d715d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_16d715d9
%pci\ven_14e4&dev_16ef&subsys_202018d4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_202018d4
%pci\ven_14e4&dev_16ed&subsys_1033193d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ed&subsys_1033193d
%pci\ven_14e4&dev_16eb&subsys_1024193d.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16eb&subsys_1024193d
%pci\ven_14e4&dev_16ef&subsys_405117aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_16ef&subsys_405117aa
%pci\ven_14e4&dev_16ef&subsys_30031259.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16ef&subsys_30031259
%pci\ven_14e4&dev_16eb&subsys_30041259.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_16eb&subsys_30041259


;*******************************************************************************
; Stratus NPAR, RoCE device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_1605&subsys_452014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_452014e4
%pci\ven_14e4&dev_1605&subsys_454014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_454014e4
%pci\ven_14e4&dev_1605&subsys_454114e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_454114e4
%pci\ven_14e4&dev_1605&subsys_16f014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_16f014e4
%pci\ven_14e4&dev_1605&subsys_16f114e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_16f114e4
%pci\ven_14e4&dev_1605&subsys_160514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1605&subsys_160514e4
%pci\ven_14e4&dev_1605&subsys_410017aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1605&subsys_410017aa
%pci\ven_14e4&dev_1605&subsys_410217aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1605&subsys_410217aa
%pci\ven_14e4&dev_1605&subsys_410117aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_410117aa
%pci\ven_14e4&dev_1605&subsys_404717aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_404717aa
%pci\ven_14e4&dev_1605&subsys_1b2715d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1605&subsys_1b2715d9
%pci\ven_14e4&dev_1605&subsys_d34014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_d34014e4
%pci\ven_14e4&dev_1605&subsys_d14014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1605&subsys_d14014e4

;*******************************************************************************
; Stingray NPAR, RoCE device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_1795&subsys_802014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1795&subsys_802014e4
%pci\ven_14e4&dev_1795&subsys_802114e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1795&subsys_802114e4
%pci\ven_14e4&dev_1795&subsys_802414e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1795&subsys_802414e4
%pci\ven_14e4&dev_1795&subsys_802814e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1795&subsys_802814e4
%pci\ven_14e4&dev_1797&subsys_804014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1797&subsys_804014e4
%pci\ven_14e4&dev_1795&subsys_802314e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1795&subsys_802314e4


;*******************************************************************************
; Thor NPAR, RoCE device ID's.
;*******************************************************************************

%pci\ven_14e4&dev_1803&subsys_100014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1803&subsys_100014e4
%pci\ven_14e4&dev_1804&subsys_112814e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_112814e4
%pci\ven_14e4&dev_1804&subsys_111614e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_111614e4
%pci\ven_14e4&dev_1804&subsys_504514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_504514e4
%pci\ven_14e4&dev_1804&subsys_504614e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_504614e4
%pci\ven_14e4&dev_1804&subsys_504914e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_504914e4
%pci\ven_14e4&dev_1803&subsys_541014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_541014e4
%pci\ven_14e4&dev_1803&subsys_100214e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_100214e4
%pci\ven_14e4&dev_1803&subsys_100314e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_100314e4
%pci\ven_14e4&dev_1805&subsys_520814e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1805&subsys_520814e4
%pci\ven_14e4&dev_1804&subsys_504714e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_504714e4
%pci\ven_14e4&dev_1804&subsys_504814e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_504814e4
%pci\ven_14e4&dev_1804&subsys_110014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_110014e4
%pci\ven_14e4&dev_1805&subsys_210014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1805&subsys_210014e4
%pci\ven_14e4&dev_1805&subsys_220014e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1805&subsys_220014e4
%pci\ven_14e4&dev_1804&subsys_542514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_542514e4
%pci\ven_14e4&dev_1804&subsys_510014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_510014e4
%pci\ven_14e4&dev_1804&subsys_510514e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_510514e4
%pci\ven_14e4&dev_1803&subsys_515014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_515014e4
%pci\ven_14e4&dev_1805&subsys_1b3e15d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1805&subsys_1b3e15d9
%pci\ven_14e4&dev_1804&subsys_525014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_525014e4
%pci\ven_14e4&dev_1804&subsys_425014e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_425014e4
%pci\ven_14e4&dev_1805&subsys_404c17aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1805&subsys_404c17aa
%pci\ven_14e4&dev_1804&subsys_510414e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_510414e4
%pci\ven_14e4&dev_1804&subsys_510114e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_510114e4
%pci\ven_14e4&dev_1804&subsys_510214e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_510214e4
%pci\ven_14e4&dev_1804&subsys_510314e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_510314e4
%pci\ven_14e4&dev_1803&subsys_515114e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_515114e4
%pci\ven_14e4&dev_1803&subsys_515214e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_515214e4
%pci\ven_14e4&dev_1803&subsys_515314e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_515314e4
%pci\ven_14e4&dev_1803&subsys_410017aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1803&subsys_410017aa
%pci\ven_14e4&dev_1804&subsys_410217aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_410217aa
%pci\ven_14e4&dev_1804&subsys_410317aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_410317aa
%pci\ven_14e4&dev_1804&subsys_410117aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_410117aa
%pci\ven_14e4&dev_1803&subsys_404717aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1803&subsys_404717aa
%pci\ven_14e4&dev_1804&subsys_09D41028.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_09D41028
%pci\ven_14e4&dev_1805&subsys_1b8115d9.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1805&subsys_1b8115d9
%pci\ven_14e4&dev_1805&subsys_520914e4.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1805&subsys_520914e4
%pci\ven_14e4&dev_1805&subsys_d12414e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1805&subsys_d12414e4
%pci\ven_14e4&dev_1804&subsys_d14214e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_d14214e4
%pci\ven_14e4&dev_1805&subsys_df2414e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1805&subsys_df2414e4
%pci\ven_14e4&dev_1804&subsys_159814e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_159814e4
%pci\ven_14e4&dev_1804&subsys_159914e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_159914e4
%pci\ven_14e4&dev_1805&subsys_159a14e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1805&subsys_159a14e4
%pci\ven_14e4&dev_1805&subsys_159b14e4.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1805&subsys_159b14e4
%pci\ven_14e4&dev_1805&subsys_410317aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1805&subsys_410317aa
%pci\ven_14e4&dev_1804&subsys_410717aa.DeviceDesc% = bcm_npar_x64_rdma,             pci\ven_14e4&dev_1804&subsys_410717aa
%pci\ven_14e4&dev_1804&subsys_405017aa.DeviceDesc% = bcm_npar_x64_rdma_wol,         pci\ven_14e4&dev_1804&subsys_405017aa
%pci\ven_14e4&dev_1804&subsys_0b1b1028.DeviceDesc% = bcm_npar_x64_rdma,              pci\ven_14e4&dev_1804&subsys_0b1b1028


;*******************************************************************************
; VF, Non-RoCE device ID's.
;*******************************************************************************
; Cumulus
%pci\ven_14e4&dev_16cb.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_16cb                 ; 
; Cumulus+
%pci\ven_14e4&dev_16e1.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_16e1                 ; 
; Whitney
%pci\ven_14e4&dev_16d3.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_16d3                 ; 
; Whitney+
%pci\ven_14e4&dev_16dc.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_16dc                 ;
; Stratus
%pci\ven_14e4&dev_1609.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_1609                 ; 
; Stingray
%pci\ven_14e4&dev_d800.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_d800                 ;

; Thor
%pci\ven_14e4&dev_1806.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_1806                 ;


;
%pci\ven_14e4&dev_16f4.DeviceDesc%        = bcm_vf_nhv_x64,                         pci\ven_14e4&dev_16f4                 ;

;*******************************************************************************
; VF, RoCE device ID's.
;*******************************************************************************
; Whitney+
%pci\ven_14e4&dev_16c1.DeviceDesc%        = bcm_vf_r_nhv_x64,                       pci\ven_14e4&dev_16c1                 ; 
; Cumulus+
%pci\ven_14e4&dev_16e5.DeviceDesc%        = bcm_vf_r_nhv_x64,                       pci\ven_14e4&dev_16e5                 ;
; Stratus
%pci\ven_14e4&dev_1606.DeviceDesc%        = bcm_vf_r_nhv_x64,                       pci\ven_14e4&dev_1606                 ;
; Stingray
%pci\ven_14e4&dev_d801.DeviceDesc%        = bcm_vf_r_nhv_x64,                       pci\ven_14e4&dev_d801                 ;

; Thor
%pci\ven_14e4&dev_1807.DeviceDesc%        = bcm_vf_r_nhv_x64,                       pci\ven_14e4&dev_1807                 ;


;*******************************************************************************
; VF for Hyper-V, Non-RoCE device ID's.
;*******************************************************************************
; Cumulus
%pci\ven_14e4&dev_16c2.DeviceDesc%         = bcm_vf_hv_x64,                         pci\ven_14e4&dev_16c2                 ; 
; Cumulus+
%pci\ven_14e4&dev_16c3.DeviceDesc%         = bcm_vf_hv_x64,                         pci\ven_14e4&dev_16c3                 ; 
; Whitney
%pci\ven_14e4&dev_16c4.DeviceDesc%         = bcm_vf_hv_x64,                         pci\ven_14e4&dev_16c4                 ; 
; Whitney+
%pci\ven_14e4&dev_16c5.DeviceDesc%         = bcm_vf_hv_x64,                         pci\ven_14e4&dev_16c5                 ;
; Stratus
%pci\ven_14e4&dev_1607.DeviceDesc%         = bcm_vf_hv_x64,                         pci\ven_14e4&dev_1607                 ;
; Stingray
%pci\ven_14e4&dev_1792.DeviceDesc%         = bcm_vf_hv_x64,                         pci\ven_14e4&dev_1792                 ;

; Thor
%pci\ven_14e4&dev_1808.DeviceDesc%         = bcm_vf_hv_x64,                         pci\ven_14e4&dev_1808                 ;


;*******************************************************************************
; VF for Hyper-V, RoCE device ID's.
;*******************************************************************************
; Whitney+
%pci\ven_14e4&dev_16bd.DeviceDesc%         = bcm_vf_r_hv_x64,                       pci\ven_14e4&dev_16bd                 ;
%pci\ven_14e4&dev_16b6.DeviceDesc%         = bcm_vf_r_hv_x64,                       pci\ven_14e4&dev_16b6                 ;
; Cumulus+
%pci\ven_14e4&dev_16e6.DeviceDesc%         = bcm_vf_r_hv_x64,                       pci\ven_14e4&dev_16e6                 ; 
; Stratus
%pci\ven_14e4&dev_1608.DeviceDesc%         = bcm_vf_r_hv_x64,                       pci\ven_14e4&dev_1608                 ;
; Stingray
%pci\ven_14e4&dev_1793.DeviceDesc%         = bcm_vf_r_hv_x64,                       pci\ven_14e4&dev_1793                 ;

; Thor
%pci\ven_14e4&dev_1809.DeviceDesc%         = bcm_vf_r_hv_x64,                       pci\ven_14e4&dev_1809                 ;


;;; just for EA-1 bring up
%pci\ven_14e4&dev_2088.DeviceDesc%         = bcm_vf_r_hv_norsc_x64,                 pci\ven_14e4&dev_2088                 ;


;*******************************************************************************
; End of device ID's.
;*******************************************************************************

[BRCM_NVRAMPackageSecurity]
security = "O:BAG:BAD:P(A;;GA;;;SY)(A;;GA;;;BA)(A;;GR;;;BU)"

;*******************************************************************************
; x64 install sections.
;*******************************************************************************

[bcm_link200_fecplus_x64_rdma]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link200, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link200_fecplus_x64_rdma.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link200_fecplus_x64_rdma.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link200_fecplus_x64_rdma.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity









[bcm_link100_fecplus_x64_rdma]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link100, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg





copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link100_fecplus_x64_rdma.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link100_fecplus_x64_rdma.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link100_fecplus_x64_rdma.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link100_fecplus_x64_rdma_nots]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link100, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link100_fecplus_x64_rdma_nots.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link100_fecplus_x64_rdma_nots.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link100_fecplus_x64_rdma_nots.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;


;;; wol
[bcm_link100_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link100, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link100_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link100_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link100_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link100_fecplus_x64_rdma_wol_nots]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link100, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link100_fecplus_x64_rdma_wol_nots.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link100_fecplus_x64_rdma_wol_nots.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link100_fecplus_x64_rdma_wol_nots.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity


[bcm_link200_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link200, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link200_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link200_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link200_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of non-wol section ;;;;;;;;;;;;;;;;;







[bcm_link50_fecplus_x64_rdma]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link50, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link50_fecplus_x64_rdma.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link50_fecplus_x64_rdma.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link50_fecplus_x64_rdma.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link50_fecplus_x64_rdma_nots]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link50, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link50_fecplus_x64_rdma_nots.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link50_fecplus_x64_rdma_nots.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link50_fecplus_x64_rdma_nots.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;




;;; wol
[bcm_link50_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link50, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link50_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link50_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link50_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of non-wol section ;;;;;;;;;;;;;;;;;



;; no wol section
[bcm_link50_fecplus_x64_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link50, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link50_fecplus_x64_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link50_fecplus_x64_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link50_fecplus_x64_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of no wol section ;;;;;;;;;;;;;;;;;

[bcm_link50_fec_x64]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link50, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link50_fec_x64.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link50_fec_x64.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link50_fec_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;



[bcm_link40_fecplus_x64]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link40_40, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link40_fecplus_x64.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link40_fecplus_x64.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link40_fecplus_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;



[bcm_thor25_fecplus_x64_rdma]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link25_thor, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_thor25_fecplus_x64_rdma.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_thor25_fecplus_x64_rdma.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_thor25_fecplus_x64_rdma.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;

[bcm_link25_fecplus_x64_rdma]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_fecplus_x64_rdma.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_fecplus_x64_rdma.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_fecplus_x64_rdma.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link25_fecplus_x64_rdma_nots]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_fecplus_x64_rdma_nots.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_fecplus_x64_rdma_nots.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_fecplus_x64_rdma_nots.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;

;; no wol section

;; no wol section

[bcm_thor25_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link25_thor, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_thor25_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_thor25_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_thor25_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of no wol section ;;;;;;;;;;;;;;;;;

[bcm_link25_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link25_fecplus_x64_rdma_wol_nots]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_fecplus_x64_rdma_wol_nots.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_fecplus_x64_rdma_wol_nots.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_fecplus_x64_rdma_wol_nots.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link25_25_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link25_25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_25_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_25_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_25_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity


[bcm_link25_fecplus_x64]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_fecplus_x64.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_fecplus_x64.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_fecplus_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;

;; no wol section
[bcm_link25_fecplus_x64_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_fecplus_x64_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_fecplus_x64_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_fecplus_x64_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of no wol section ;;;;;;;;;;;;;;;;;


[bcm_link25_fec_x64]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link25, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link25_fec_x64.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link25_fec_x64.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link25_fec_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;




[bcm_link10_fecplus_x64_rdma]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link10, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link10_fecplus_x64_rdma.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link10_fecplus_x64_rdma.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link10_fecplus_x64_rdma.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link10_fecplus_x64_rdma_nots]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link10, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link10_fecplus_x64_rdma_nots.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link10_fecplus_x64_rdma_nots.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link10_fecplus_x64_rdma_nots.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;


;; wol section
[bcm_link10_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link10, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link10_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link10_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link10_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link10_fecplus_x64_rdma_wol_nots]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link10, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk
delreg          = params_ndk.delreg


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link10_fecplus_x64_rdma_wol_nots.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link10_fecplus_x64_rdma_wol_nots.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link10_fecplus_x64_rdma_wol_nots.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of wol section ;;;;;;;;;;;;;;;;;



[bcm_link10_fecplus_x64]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link10, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link10_fecplus_x64.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link10_fecplus_x64.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link10_fecplus_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;





[bcm_link10_10_fecplus_x64_rdma_wol]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_wol_cap, params_link10_10, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec, params_fecplus


addreg          = params_ndk


copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link10_10_fecplus_x64_rdma_wol.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link10_10_fecplus_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link10_10_fecplus_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

[bcm_link10_fec_x64]
characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg          = x64_addreg, params_nt, params_link10, params_mtu_9k, params_lso
addreg          = params_rss, params_rss_queues_16, params_ipv6_cksum, params_ipv6_lso, params_flow
addreg          = params_buf_desc, params_max_msix, params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_qos, params_fec



copyfiles       = x64_sys_file
bustype         = 5
*IfType         = 6      ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0      ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0

[bcm_link10_fec_x64.Services]
addservice      = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_link10_fec_x64.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_link10_fec_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity
;;;;;;; end of section ;;;;;;;;;;;;;;;;;




[bcm_vf_hv_x64]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_vf_addreg, params_nt_vf, params_mtu_vf, params_lso, params_rss, params_rss_queues_16
addreg               = params_ipv6_cksum, params_ipv6_lso, params_buf_desc, params_rsc_ipv4, params_rsc_ipv6
copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3

[bcm_vf_hv_x64.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_vf_hv_x64.hw]
addreg               = msix_support

[bcm_vf_hv_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of section ;;;;;;;;;;;;;;;;;


[bcm_vf_r_hv_x64]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_vf_addreg, params_nt_vf, params_mtu_vf, params_lso, params_rss, params_rss_queues_16
addreg               = params_ipv6_cksum, params_ipv6_lso, params_buf_desc, params_rsc_ipv4, params_rsc_ipv6, params_ndk
delreg               = params_ndk.delreg
copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3

[bcm_vf_r_hv_x64.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_vf_r_hv_x64.hw]
addreg               = msix_support

[bcm_vf_r_hv_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of section ;;;;;;;;;;;;;;;;;

[bcm_vf_r_hv_norsc_x64]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_vf_addreg, params_nt_vf, params_mtu_vf, params_lso, params_rss, params_rss_queues_16
addreg               = params_ipv6_cksum, params_ipv6_lso, params_buf_desc, params_ndk
delreg               = params_ndk.delreg
copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3

[bcm_vf_r_hv_norsc_x64.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_vf_r_hv_norsc_x64.hw]
addreg               = msix_support

[bcm_vf_r_hv_norsc_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of section ;;;;;;;;;;;;;;;;;

[bcm_vf_nhv_x64]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_addreg, params_nt_vf, params_mtu_vf, params_lso, params_rss, params_rss_queues_16, params_rss_queues_default_4
addreg               = params_ipv6_cksum, params_ipv6_lso, params_buf_desc, params_rsc_ipv4, params_rsc_ipv6
copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3

[bcm_vf_nhv_x64.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_vf_nhv_x64.hw]
addreg               = msix_support

[bcm_vf_nhv_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of section ;;;;;;;;;;;;;;;;;

[bcm_vf_r_nhv_x64]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_addreg, params_nt_vf, params_mtu_vf, params_lso, params_rss, params_rss_queues_16, params_rss_queues_default_4
addreg               = params_ipv6_cksum, params_ipv6_lso, params_buf_desc, params_rsc_ipv4, params_rsc_ipv6, params_ndk
delreg               = params_ndk.delreg
copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3

[bcm_vf_r_nhv_x64.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_vf_r_nhv_x64.hw]
addreg               = msix_support

[bcm_vf_r_nhv_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of section ;;;;;;;;;;;;;;;;;

[bcm_npar_x64]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_addreg, params_nt, params_mtu_9k, params_lso
addreg               = params_rss, params_rss_queues_8, params_rss_queues_default_4, params_qos
addreg               = params_ipv6_cksum, params_ipv6_lso, params_flow, params_buf_desc, params_rx_buffers_default_2000

addreg               = params_vmq, params_rsc_ipv4, params_rsc_ipv6




copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber  = 0

[bcm_npar_x64.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_npar_x64.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_npar_x64.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of section ;;;;;;;;;;;;;;;;;

;; no wol section
[bcm_npar_x64_wol]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_addreg, params_nt, params_wol_cap, params_mtu_9k, params_lso
addreg               = params_rss, params_rss_queues_8, params_rss_queues_default_4, params_qos
addreg               = params_ipv6_cksum, params_ipv6_lso, params_flow, params_buf_desc, params_rx_buffers_default_2000

addreg               = params_vmq, params_rsc_ipv4, params_rsc_ipv6




copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber  = 0

[bcm_npar_x64_wol.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_npar_x64_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_npar_x64_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of no wol section ;;;;;;;;;;;;;;;;;

[bcm_npar_x64_rdma]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_addreg, params_nt, params_mtu_9k, params_lso
addreg               = params_rss, params_rss_queues_8, params_rss_queues_default_4, params_qos
addreg               = params_ipv6_cksum, params_ipv6_lso, params_flow, params_buf_desc, params_rx_buffers_default_2000

addreg               = params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_ndk
delreg               = params_ndk.delreg




copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber  = 0

[bcm_npar_x64_rdma.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_npar_x64_rdma.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_npar_x64_rdma.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of section ;;;;;;;;;;;;;;;;;

;; no wol section
[bcm_npar_x64_rdma_wol]
characteristics      = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
addreg               = x64_addreg, params_nt, params_wol_cap, params_mtu_9k, params_lso
addreg               = params_rss, params_rss_queues_8, params_rss_queues_default_4, params_qos
addreg               = params_ipv6_cksum, params_ipv6_lso, params_flow, params_buf_desc, params_rx_buffers_default_2000

addreg               = params_vmq, params_rsc_ipv4, params_rsc_ipv6, params_ndk
delreg               = params_ndk.delreg




copyfiles            = x64_sys_file
bustype              = 5
*IfType              = 6   ; IF_TYPE_ETHERNET_CSMACD
*MediaType           = 0   ; NdisMedium802_3
*PhysicalMediaType   = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber  = 0

[bcm_npar_x64_rdma_wol.Services]
addservice           = bnxtnd, 2, x64_add_service, x64_eventlog

[bcm_npar_x64_rdma_wol.hw]
addreg          = msix_support


include         = pci.inf
needs           = PciSriovSupported.hw




[bcm_npar_x64_rdma_wol.WMI]
WMIInterface = {E8BA3968-D0EC-4CDE-ACAC-EA6AABBEF185},1,BRCM_NVRAMPackageSecurity

;;;;;;; end of no wol section ;;;;;;;;;;;;;;;;;

;*******************************************************************************
; x64 common sections.
;*******************************************************************************

[x64_add_service]
displayname     = %mp_srv_desc%
servicetype     = 1 
starttype       = 3
errorcontrol    = 1
servicebinary   = %12%\bnxtnd.sys

[x64_addreg]
hkr, ndi,            service,    0, "bnxtnd"
hkr, ndi\interfaces, upperrange, 0, "ndis5"
hkr, ndi\interfaces, lowerrange, 0, "ethernet"


[x64_vf_addreg]
hkr, ,               busnumber,  0, "0"
hkr, ndi,            service,    0, "bnxtnd"
hkr, ndi\interfaces, upperrange, 0, "ndisvf"
hkr, ndi\interfaces, lowerrange, 0, "iovvf"

[x64_eventlog]
addreg = x64_addreg_eventlog

[x64_addreg_eventlog]
hkr, , eventmessagefile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\bnxtnd.sys"
hkr, , typessupported  , 0x00010001, 7

;*******************************************************************************
; Registry parameters.
;*******************************************************************************

[msix_support]
hkr, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
hkr, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 0x02

[params_nt]
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4,      paramDesc, , %taskoffload_desc_ipv4%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4,      default,   , "3"
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4,      type,      , "enum"
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 0,         , %taskoffload_disabled%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 1,         , %taskoffload_tx_cksum%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 2,         , %taskoffload_rx_cksum%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 3,         , %taskoffload_rx_tx_cksum%

hkr, ndi\params\*PriorityVLANTag,       paramDesc, , %priority_vlan_desc%
hkr, ndi\params\*PriorityVLANTag,       default,   , "3"
hkr, ndi\params\*PriorityVLANTag,       type,      , "enum"
hkr, ndi\params\*PriorityVLANTag\enum,  0,         , %priority_vlan_disabled%
hkr, ndi\params\*PriorityVLANTag\enum,  1,         , %priority_enabled%
hkr, ndi\params\*PriorityVLANTag\enum,  2,         , %vlan_enabled%
hkr, ndi\params\*PriorityVLANTag\enum,  3,         , %priority_vlan_enabled%

hkr, ndi\params\VlanID, paramdesc, , %vlan_id_desc%
hkr, ndi\params\VlanID, default,   , "0"
hkr, ndi\params\VlanID, type,      , "dword"
hkr, ndi\params\VlanID, min,       , "0"
hkr, ndi\params\VlanID, max,       , "4094"
hkr, ndi\params\VlanID, step,      , "1"
hkr, ndi\params\VlanID, base,      , "10"

hkr, ndi\params\*InterruptModeration,      paramDesc, , %intr_mod_desc%
hkr, ndi\params\*InterruptModeration,      default,   , "1"
hkr, ndi\params\*InterruptModeration,      type,      , "enum"
hkr, ndi\params\*InterruptModeration\enum, 0,         , %disabled%
hkr, ndi\params\*InterruptModeration\enum, 1,         , %enabled%

hkr, ndi\params\InterruptModeration,      paramDesc, , %im_cfg_desc%
hkr, ndi\params\InterruptModeration,      default,   , "200"
hkr, ndi\params\InterruptModeration,      type,      , "enum"
hkr, ndi\params\InterruptModeration\enum, 100,       , %im_low_desc%
hkr, ndi\params\InterruptModeration\enum, 200,       , %im_med_desc%
hkr, ndi\params\InterruptModeration\enum, 300,       , %im_high_desc%

hkr, ndi\params\NetworkAddress, paramdesc, 0, %network_address%
hkr, ndi\params\NetworkAddress, default,   0, ""
hkr, ndi\params\NetworkAddress, type,      0, "edit"
hkr, ndi\params\NetworkAddress, limittext, 0, "12"
hkr, ndi\params\NetworkAddress, uppercase, 0, "1"
hkr, ndi\params\NetworkAddress, optional,  0, "1"

[params_nt_vf]
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4,      paramDesc, , %taskoffload_desc_ipv4%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4,      default,   , "3"
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4,      type,      , "enum"
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 0,         , %taskoffload_disabled%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 1,         , %taskoffload_tx_cksum%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 2,         , %taskoffload_rx_cksum%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv4\enum, 3,         , %taskoffload_rx_tx_cksum%

[params_max_msix]
hkr, ndi\params\max_num_msix_messages, paramDesc, , %max_num_msix_messages%
hkr, ndi\params\max_num_msix_messages, default,   0, "0"
hkr, ndi\params\max_num_msix_messages, type,      0, "dword"
hkr, ndi\params\max_num_msix_messages, min,       0, "16"
hkr, ndi\params\max_num_msix_messages, max,       0, "511"
hkr, ndi\params\max_num_msix_messages, base,      0, "10"
hkr, ndi\params\max_num_msix_messages, optional,  0, "1"


[params_vmq]
hkr, ndi\params\*VMQ,      paramDesc, , %vmq_desc%
hkr, ndi\params\*VMQ,      default,   , "1"
hkr, ndi\params\*VMQ,      type,      , "enum"
hkr, ndi\params\*VMQ\enum, 0,         , %disabled%
hkr, ndi\params\*VMQ\enum, 1,         , %enabled%







[params_rsc_ipv4]
hkr, ndi\params\*RscIPv4,  paramDesc, , %ipv4_rsc_desc%

hkr, ndi\params\*RscIPv4,  default,   , "0"


hkr, ndi\params\*RscIPv4,  type,      , "enum"
hkr, ndi\params\*RscIPv4\enum, 0,    , %disabled%
hkr, ndi\params\*RscIPv4\enum, 1,    , %enabled%

[params_rsc_ipv6]
hkr, ndi\params\*RscIPv6,  paramDesc, , %ipv6_rsc_desc%

hkr, ndi\params\*RscIPv6,  default,   , "0"


hkr, ndi\params\*RscIPv6,  type,      , "enum"
hkr, ndi\params\*RscIPv6\enum, 0,    , %disabled%
hkr, ndi\params\*RscIPv6\enum, 1,    , %enabled%


[params_qos]
hkr, ndi\params\*QOS,  paramDesc, , %qos_desc%
hkr, ndi\params\*QOS,  default,   , "1"
hkr, ndi\params\*QOS,  type,      , "enum"
hkr, ndi\params\*QOS\enum, 0,    , %disabled%
hkr, ndi\params\*QOS\enum, 1,    , %enabled%

[params_mtu_9k]
hkr, ndi\params\*JumboPacket,       paramdesc, , %mtu_desc%
hkr, ndi\params\*JumboPacket,       default,   , "1514"
hkr, ndi\params\*JumboPacket,       type,      , "long"
hkr, ndi\params\*JumboPacket,       min,       , "1514"
hkr, ndi\params\*JumboPacket,       max,       , "9174"

[params_mtu_vf]
hkr, ndi\params\*JumboPacket,       paramdesc, , %mtu_desc%
hkr, ndi\params\*JumboPacket,       default,   , "1514"
hkr, ndi\params\*JumboPacket,       type,      , "long"
hkr, ndi\params\*JumboPacket,       min,       , "1514"
hkr, ndi\params\*JumboPacket,       max,       , "9174"

[params_rss_queues_16]
hkr, ndi\params\*NumRSSQueues,         paramDesc, , %rss_queue_cnt_desc%
hkr, ndi\params\*NumRSSQueues,         default,   , "16"
HKR,Ndi\Params\*NumRssQueues,          type,      ,"long"
HKR,Ndi\Params\*NumRssQueues,          min,       ,"1"
HKR,Ndi\Params\*NumRssQueues,          max,       ,"16"

[params_rss_queues_8]
hkr, ndi\params\*NumRSSQueues,         paramDesc, , %rss_queue_cnt_desc%
hkr, ndi\params\*NumRSSQueues,         default,   , "8"
HKR,Ndi\Params\*NumRssQueues,          type,      ,"long"
HKR,Ndi\Params\*NumRssQueues,          min,       ,"1"
HKR,Ndi\Params\*NumRssQueues,          max,       ,"8"

[params_rss_queues_default_4]
hkr, ndi\params\*NumRSSQueues,         default,   , "4"

[params_wol_cap]
hkr, ndi\params\*WakeOnMagicPacket,      paramDesc, , %wake_on_magic_desc%
hkr, ndi\params\*WakeOnMagicPacket,      default,   , "1"
hkr, ndi\params\*WakeOnMagicPacket,      type,      , "enum"
hkr, ndi\params\*WakeOnMagicPacket\enum, 0,         , %disabled%
hkr, ndi\params\*WakeOnMagicPacket\enum, 1,         , %enabled%

hkr, ndi\params\*WakeOnPattern,      paramDesc, , %wake_on_pattern_desc%
hkr, ndi\params\*WakeOnPattern,      default,   , "1"
hkr, ndi\params\*WakeOnPattern,      type,      , "enum"
hkr, ndi\params\*WakeOnPattern\enum, 0,         , %disabled%
hkr, ndi\params\*WakeOnPattern\enum, 1,         , %enabled%

hkr, ndi\params\EnablePmeOnShutdown,      paramDesc, , %enable_pme_on_shutdown_desc%
hkr, ndi\params\EnablePmeOnShutdown,      default,   , "0"
hkr, ndi\params\EnablePmeOnShutdown,      type,      , "enum"
hkr, ndi\params\EnablePmeOnShutdown\enum, 0,         , %disabled%
hkr, ndi\params\EnablePmeOnShutdown\enum, 1,         , %enabled%

[params_buf_desc]
hkr, ndi\params\*TransmitBuffers, paramdesc, , %tx_bufs_desc%
hkr, ndi\params\*TransmitBuffers, default,   , "0"
hkr, ndi\params\*TransmitBuffers, type,      , "dword"
hkr, ndi\params\*TransmitBuffers, min,       , "0"
hkr, ndi\params\*TransmitBuffers, max,       , "5000"
hkr, ndi\params\*TransmitBuffers, step,      , "50"
hkr, ndi\params\*TransmitBuffers, base,      , "10"

hkr, ndi\params\*ReceiveBuffers, paramdesc, , %rx_bufs_desc%
hkr, ndi\params\*ReceiveBuffers, default,   , "0"
hkr, ndi\params\*ReceiveBuffers, type,      , "dword"
hkr, ndi\params\*ReceiveBuffers, min,       , "0"
hkr, ndi\params\*ReceiveBuffers, max,       , "15000"
hkr, ndi\params\*ReceiveBuffers, step,      , "500"
hkr, ndi\params\*ReceiveBuffers, base,      , "10"

[params_rx_buffers_default_2000]
hkr, ndi\params\*ReceiveBuffers,         default,   , "2000"

[params_ipv6_cksum]
hkr, ndi\params\*TCPUDPChecksumOffloadIPv6,      paramDesc, , %taskoffload_desc_ipv6%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv6,      default,   , "3"
hkr, ndi\params\*TCPUDPChecksumOffloadIPv6,      type,      , "enum"
hkr, ndi\params\*TCPUDPChecksumOffloadIPv6\enum, 0,         , %taskoffload_disabled%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv6\enum, 1,         , %taskoffload_tx_cksum%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv6\enum, 2,         , %taskoffload_rx_cksum%
hkr, ndi\params\*TCPUDPChecksumOffloadIPv6\enum, 3,         , %taskoffload_rx_tx_cksum%

[params_ipv6_lso]
hkr, ndi\params\*LSOv2IPv6,      paramDesc, , %lso_desc_ipv6%
hkr, ndi\params\*LSOv2IPv6,      default,   , "1"
hkr, ndi\params\*LSOv2IPv6,      type,      , "enum"
hkr, ndi\params\*LSOv2IPv6\enum, 0,         , %disabled%
hkr, ndi\params\*LSOv2IPv6\enum, 1,         , %enabled%



[params_flow]
hkr, ndi\params\*FlowControl,      paramdesc,  , %flow_ctrl%

hkr, ndi\params\*FlowControl,      default,    , "3"


hkr, ndi\params\*FlowControl,      type,       , "enum"
hkr, ndi\params\*FlowControl\enum, 0,          , %flow_ctrl_disabled%
hkr, ndi\params\*FlowControl\enum, 1,          , %flow_ctrl_tx%
hkr, ndi\params\*FlowControl\enum, 2,          , %flow_ctrl_rx%
hkr, ndi\params\*FlowControl\enum, 3,          , %flow_ctrl_rx_tx%
hkr, ndi\params\*FlowControl\enum, 4,          , %flow_ctrl_auto%

[params_rss]
hkr, ndi\params\*RSS,      paramDesc, , %rss_desc%
hkr, ndi\params\*RSS,      default,   , "1"
hkr, ndi\params\*RSS,      type,      , "enum"
hkr, ndi\params\*RSS\enum, 0,         , %disabled%
hkr, ndi\params\*RSS\enum, 1,         , %enabled%

hkr, ndi\Params\*NumaNodeId,                              paramDesc, , "%numa_node_desc%"
hkr, ndi\Params\*NumaNodeId,                              default,   , "65535"
hkr, ndi\Params\*NumaNodeId,                              type,      , "long"
hkr, ndi\Params\*NumaNodeId,                              min,       , "0"
hkr, ndi\Params\*NumaNodeId,                              max,       , "65535"
hkr, ndi\Params\*NumaNodeId,                              optional,  , "1"


hkr, ndi\params\*RSSProfile,                              paramDesc, , %rss_profile_desc%
hkr, ndi\params\*RSSProfile,                              default,   , "4"
hkr, ndi\params\*RSSProfile,                              type,      , "enum"
hkr, ndi\params\*RSSProfile\enum,                         1,         , %rss_profile_cp%
hkr, ndi\params\*RSSProfile\enum,                         2,         , %rss_profile_cps%
hkr, ndi\params\*RSSProfile\enum,                         3,         , %rss_profile_ns%
hkr, ndi\params\*RSSProfile\enum,                         4,         , %rss_profile_nss%
hkr, ndi\params\*RSSProfile\enum,                         5,         , %rss_profile_cs%
hkr, ndi\params\*RSSProfile,                              optional,  , "1"

hkr, ndi\Params\*RssBaseProcGroup,                        paramDesc, , "%rss_base_group_proc_number_desc%"
hkr, ndi\Params\*RssBaseProcGroup,                        default,   , "0"
hkr, ndi\Params\*RssBaseProcGroup,                        type,      , "long"
hkr, ndi\Params\*RssBaseProcGroup,                        min,       , "0"
hkr, ndi\Params\*RssBaseProcGroup,                        max,       , "65534"
hkr, ndi\params\*RssBaseProcGroup,                        optional,  , "1"



hkr, ndi\Params\*RssBaseProcNumber,                       paramDesc, , "%rss_base_proc_number_desc%"
hkr, ndi\Params\*RssBaseProcNumber,                       default,   , "0"
hkr, ndi\Params\*RssBaseProcNumber,                       type,      , "long"
hkr, ndi\Params\*RssBaseProcNumber,                       min,       , "0"
hkr, ndi\Params\*RssBaseProcNumber,                       max,       , "63"
hkr, ndi\Params\*RssBaseProcNumber,                       optional,  , "1"

hkr, ndi\Params\*MaxRssProcessors,                        paramDesc, , "%max_rss_processors_desc%"
hkr, ndi\Params\*MaxRssProcessors,                        default,   , "16"
hkr, ndi\Params\*MaxRssProcessors,                        type,      , "long"
hkr, ndi\Params\*MaxRssProcessors,                        min,       , "1"
hkr, ndi\Params\*MaxRssProcessors,                        max,       , "64"

hkr, ndi\Params\*MaxRssProcessors,                        optional,  , "1"


hkr, ndi\Params\*RssMaxProcNumber,                        paramDesc, , "%rss_max_proc_number_desc%"
hkr, ndi\Params\*RssMaxProcNumber,                        default,   , ""
hkr, ndi\Params\*RssMaxProcNumber,                        type,      , "long"
hkr, ndi\Params\*RssMaxProcNumber,                        min,       , "0"
hkr, ndi\Params\*RssMaxProcNumber,                        max,       , "63"
hkr, ndi\Params\*RssMaxProcNumber,                        optional,  , "1"

hkr, ndi\Params\*RSSMaxProcGroup,                         paramDesc, , "%rss_max_group_proc_number_desc%"
hkr, ndi\Params\*RSSMaxProcGroup,                         default,   , "0"
hkr, ndi\Params\*RSSMaxProcGroup,                         type,      , "long"
hkr, ndi\Params\*RSSMaxProcGroup,                         min,       , "0"
hkr, ndi\Params\*RSSMaxProcGroup,                         max,       , "65534"
hkr, ndi\Params\*RSSMaxProcGroup,                         optional,  , "1"


[params_link10]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "0"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        6,         , %speed_duplex_1Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%

hkr, ndi\params\*EEE,                                     paramDesc, , %eee_desc%
hkr, ndi\params\*EEE,                                     default,   , "1"
hkr, ndi\params\*EEE,                                     type,      , "enum"
hkr, ndi\params\*EEE\enum,                                0,         , %disabled%
hkr, ndi\params\*EEE\enum,                                1,         , %enabled%

[params_link10_10]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "7"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        6,         , %speed_duplex_1Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%

[params_link25_thor]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "0"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        25000,     , %speed_duplex_25Gb_fd%

[params_link25]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "0"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        6,         , %speed_duplex_1Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        25000,     , %speed_duplex_25Gb_fd%

[params_link25_25]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "25000"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        6,         , %speed_duplex_1Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        25000,     , %speed_duplex_25Gb_fd%


[params_link40_40]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "9"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        25000,     , %speed_duplex_25Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        9,         , %speed_duplex_40Gb_fd%

[params_link50]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "0"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        25000,     , %speed_duplex_25Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        9,         , %speed_duplex_40Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        50000,     , %speed_duplex_50Gb_fd%

[params_link100]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "0"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        25000,     , %speed_duplex_25Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        9,         , %speed_duplex_40Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        50000,     , %speed_duplex_50Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        100000,    , %speed_duplex_100Gb_fd%

[params_link200]
hkr, ndi\params\*SpeedDuplex,                             paramDesc, , %speed_duplex_desc%
hkr, ndi\params\*SpeedDuplex,                             default,   , "0"
hkr, ndi\params\*SpeedDuplex,                             type,      , "enum"
hkr, ndi\params\*SpeedDuplex\enum,                        0,         , %speed_duplex_auto%
hkr, ndi\params\*SpeedDuplex\enum,                        7,         , %speed_duplex_10Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        25000,     , %speed_duplex_25Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        9,         , %speed_duplex_40Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        50000,     , %speed_duplex_50Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        100000,    , %speed_duplex_100Gb_fd%
hkr, ndi\params\*SpeedDuplex\enum,                        200000,    , %speed_duplex_200Gb_fd%



[params_lso]
hkr, ndi\params\*LSOv2IPv4,      paramDesc, , %lso_desc_ipv4%
hkr, ndi\params\*LSOv2IPv4,      default,   , "1"
hkr, ndi\params\*LSOv2IPv4,      type,      , "enum"
hkr, ndi\params\*LSOv2IPv4\enum, 0,         , %disabled%
hkr, ndi\params\*LSOv2IPv4\enum, 1,         , %enabled%







[params_ndk]
hkr, ndi\params\*NetworkDirect,  paramDesc, , "NetworkDirect Functionality"
hkr, ndi\params\*NetworkDirect,  type,      , "enum"
hkr, ndi\params\*NetworkDirect,  default,   , "1"
hkr, ndi\params\*NetworkDirect\enum, 0,    , %disabled%
hkr, ndi\params\*NetworkDirect\enum, 1,    , %enabled%

HKR, Ndi\Params\*NetworkDirectTechnology,        ParamDesc,  0,  "NetworkDirect Technology"
HKR, Ndi\Params\*NetworkDirectTechnology,        Default,    0,  "4"
HKR, Ndi\Params\*NetworkDirectTechnology,        Type,       0,  "enum"
HKR, Ndi\Params\*NetworkDirectTechnology\enum,   4,          0,  "RoCEv2"

hkr, ndi\params\RoCEMtu,  paramDesc, , "RoCE MTU"
hkr, ndi\params\RoCEMtu,  type,      , "enum"
hkr, ndi\params\RoCEMtu,  default,   , "3"
hkr, ndi\params\RoCEMtu\enum, 1,    , %roce_mtu_256%
hkr, ndi\params\RoCEMtu\enum, 2,    , %roce_mtu_512%
hkr, ndi\params\RoCEMtu\enum, 3,    , %roce_mtu_1024%
hkr, ndi\params\RoCEMtu\enum, 4,    , %roce_mtu_2048%
hkr, ndi\params\RoCEMtu\enum, 5,    , %roce_mtu_4096%

[params_ndk.delreg]
hkr, ndi\params\RoCEVersion
hkr,, RoCEVersion





[params_fec]
hkr, ndi\Params\FEC,                         paramDesc, , "%fec_desc%"
hkr, ndi\Params\FEC,                         default,   , "0"
hkr, ndi\Params\FEC,                         type,      , "enum"
hkr, ndi\Params\FEC\enum,                    0,         , "%disabled%"
hkr, ndi\Params\FEC\enum,                    1,         , "%fec_cl74%"
hkr, ndi\Params\FEC\enum,                    3,         , "%fec_auto%"

;Only include if params_fec is included
[params_fecplus]
hkr, ndi\Params\FEC\enum,                    2,         , "%fec_cl91%"
hkr, ndi\Params\FEC\enum,                    4,         , "%fec_rs544_1xn%"
hkr, ndi\Params\FEC\enum,                    5,         , "%fec_rs544_ieee%"
hkr, ndi\Params\FEC\enum,                    6,         , "%fec_rs272_1xn%"
hkr, ndi\Params\FEC\enum,                    7,         , "%fec_rs272_ieee%"

;*******************************************************************************
; Destination directories
;*******************************************************************************

[destinationdirs]
defaultdestdir  = 11
x64_sys_file  = 12

[sourcedisksnames]
1 = %disk_desc%,,,

[sourcedisksfiles]
bnxtnd.sys = 1

[x64_sys_file]
bnxtnd.sys,,,1

;*******************************************************************************
; Localizable and non-localizable strings.
;*******************************************************************************

[strings]

; Non-Localizable strings
brcm = "Broadcom Corporation"

; Localizable strings
disk_desc                   = "Broadcom Installation Media"
mp_srv_desc                 = "Broadcom Cumulus Ethernet Adapter"


;*******************************************************************************
; Physical device strings.
;*******************************************************************************

;*******************************************************************************
; Cumulus physical device strings.
;*******************************************************************************



pci\ven_14e4&dev_16c9&subsys_020314E4.DeviceDesc = "Broadcom M125c NetXtreme C-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16ca&subsys_040314E4.DeviceDesc = "Broadcom P150c NetXtreme-C Single-port 40Gb/50Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ca&subsys_040214E4.DeviceDesc = "Broadcom P225c NetXtreme-C Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ca&subsys_040514E4.DeviceDesc = "Broadcom M225c NetXtreme C-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16ca&subsys_3043108e.DeviceDesc = "Broadcom NetXtreme-C Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16c9&subsys_020514E4.DeviceDesc = "Broadcom P210c NetXtreme-C Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16c9&subsys_020614E4.DeviceDesc = "Broadcom P210c NetXtreme-C Dual-port 10Gb Ethernet OCP Mezzanine Adapter"
pci\ven_14e4&dev_16c9&subsys_020714E4.DeviceDesc = "Broadcom M125c NetXtreme C-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16c9&subsys_020814E4.DeviceDesc = "Broadcom M125clp NetXtreme C-Series Ethernet OCP Type4 Adapter"
pci\ven_14e4&dev_16ca&subsys_040614e4.DeviceDesc = "Broadcom P225c NetXtreme-C Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ca&subsys_040a14e4.DeviceDesc = "Broadcom P225c NetXtreme-C Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ca&subsys_040414e4.DeviceDesc = "Broadcom M150c NetXtreme-C Single-port 40Gb/50Gb Ethernet OCP Mezzanine Adapter"
pci\ven_14e4&dev_16ca&subsys_414214e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet OCP Adapter"
pci\ven_14e4&dev_16ca&subsys_304414e4.DeviceDesc = "Broadcom NetXtreme-C Dual-port 10Gb/25Gb Ethernet PCIe Adapter"

;*******************************************************************************
; Cumulus+ physical device strings.
;*******************************************************************************

pci\ven_14e4&dev_16ce&subsys_16ce14e4.DeviceDesc = "Broadcom BCM57311 NetXtreme-C 10Gb RDMA Ethernet Controller" ;**
pci\ven_14e4&dev_16cf&subsys_312017aa.DeviceDesc = "Broadcom NX-C PCIe 25Gb 1-Port SFP28 Ethernet Adapter"
pci\ven_14e4&dev_16cf&subsys_16cf14e4.DeviceDesc = "Broadcom BCM57312 NetXtreme-C 10Gb/25Gb RDMA Ethernet Controller" ;**
pci\ven_14e4&dev_16df&subsys_16df14e4.DeviceDesc = "Broadcom BCM57314 NetXtreme-C 10Gb/25Gb/40Gb/50Gb RDMA Ethernet Controller" ;**
pci\ven_14e4&dev_16df&subsys_140414e4.DeviceDesc = "Broadcom M225cp NetXtreme C-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16df&subsys_120214e4.DeviceDesc = "Broadcom M125cp NetXtreme C-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16df&subsys_140214e4.DeviceDesc = "Broadcom P225cp NetXtreme-C Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16df&subsys_140314e4.DeviceDesc = "Broadcom P150cp NetXtreme-C single port 40Gb/50Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16e0&subsys_16e014e4.DeviceDesc = "Broadcom BCM57317 NetXtreme-C 10GBase-T RDMA Ethernet Controller" ;**
pci\ven_14e4&dev_16e4&subsys_16e414e4.DeviceDesc = "Broadcom BCM57317 NetXtreme-C 25Gb RDMA Ethernet Controller" ;**
pci\ven_14e4&dev_16df&subsys_140514e4.DeviceDesc = "Broadcom M225cp NetXtreme C-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16df&subsys_4869108e.DeviceDesc = "Oracle Dual Port 10Gb/25Gb SFP28 Cloud Ethernet Controller"

;*******************************************************************************
; Whitney physical device strings.
;*******************************************************************************

pci\ven_14e4&dev_16d0&subsys_402014E4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10Gb SFP+ Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d1&subsys_404114E4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d1&subsys_312017aa.DeviceDesc = "Broadcom NX-C Single-port 25G PCIe Adapter"
pci\ven_14e4&dev_16d2&subsys_060214E4.DeviceDesc = "Broadcom P210t NetXtreme-E Dual-port 10GBASE-T Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d2&subsys_416017aa.DeviceDesc = "Broadcom NX-E Dual-port 10GBASE-T PCIe Adapter"

;*******************************************************************************
; Whitney+ physical device strings.
;*******************************************************************************

pci\ven_14E4&dev_16D6&subsys_412014E4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10Gb SFP+ Ethernet Network Daughter Card"
pci\ven_14E4&dev_16D6&subsys_412114E4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10Gb SFP+ Ethernet PCIe Adapter"
pci\ven_14E4&dev_16D6&subsys_16d614E4.DeviceDesc = "Broadcom BCM57412 NetXtreme-E 10Gb RDMA Ethernet Controller" ; **
pci\ven_14e4&dev_16d7&subsys_16d714e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E 10Gb/25Gb RDMA Ethernet Controller" ; **
pci\ven_14e4&dev_16d7&subsys_414114e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_140514e4.DeviceDesc = "Broadcom P225ep NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_414014e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Network Daughter Card"
pci\ven_14e4&dev_16d8&subsys_416114e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d8&subsys_416014e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet Network Daughter Card"
pci\ven_14E4&dev_16d8&subsys_1feb1028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10Gb SFP+ Ethernet LOM" ; **
pci\ven_14e4&dev_16d8&subsys_160214e4.DeviceDesc = "Broadcom P210tep NetXtreme-E Dual-port 10GBASE-T Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d8&subsys_30031259.DeviceDesc = "Allied Telesis AT-ANC10T/2 Dual Port 10GBASE-T Adapter"
pci\ven_14e4&dev_16d8&subsys_416017aa.DeviceDesc = "Broadcom NX-E PCIe 10Gb 2-Port Base-T Ethernet Adapter"
pci\ven_14e4&dev_16d8&subsys_416117aa.DeviceDesc = "Broadcom NX-E ML2 10Gb 2-Port Base-T Ethernet Adapter"
pci\ven_14e4&dev_16d8&subsys_16d814e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E 10GBASE-T RDMA Ethernet Controller" ; **
pci\ven_14e4&dev_16d9&subsys_16d914e4.DeviceDesc = "Broadcom BCM57417 NetXtreme-E 10GBASE-T RDMA Ethernet Controller" ; **
pci\ven_14e4&dev_16e2&subsys_16e214e4.DeviceDesc = "Broadcom BCM57417 NetXtreme-E 10Gb/25Gb RDMA Ethernet Controller" ; **
pci\ven_14e4&dev_16e3&subsys_16e314e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E 10Gb RDMA Ethernet Controller" ; **
pci\ven_14e4&dev_16d9&subsys_4866108e.DeviceDesc = "Oracle Dual Port 10GBase-T Ethernet Controller"
pci\ven_14e4&dev_16e2&subsys_4866108e.DeviceDesc = "Oracle Dual Port 10Gb/25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_1fea1028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet LOM"
pci\ven_14e4&dev_16d8&subsys_07e51028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet LOM"
pci\ven_14e4&dev_16d6&subsys_412017aa.DeviceDesc = "Broadcom NX-E PCIe 25Gb 1-Port SFP28 Ethernet Adapter"
pci\ven_14e4&dev_16d7&subsys_140314e4.DeviceDesc = "Broadcom P150p NetXtreme-E Single-port 40Gb/50Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_140214e4.DeviceDesc = "Broadcom P225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_140414e4.DeviceDesc = "Broadcom M225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d6&subsys_120214e4.DeviceDesc = "Broadcom M125p NetXtreme E-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16d7&subsys_3044108e.DeviceDesc = "Oracle Dual Port 25Gb Ethernet Adapter"
pci\ven_14e4&dev_16d7&subsys_4869108e.DeviceDesc = "Oracle Dual Port 10Gb/25Gb SFP28 Cloud Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_414314e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 40Gb/50Gb Ethernet OCP Adapter"
pci\ven_14e4&dev_16d6&subsys_412314e4.DeviceDesc = "Broadcom M210p NetXtreme-E Dual-port 10Gb Ethernet OCP Adapter"
pci\ven_14e4&dev_16d6&subsys_412414e4.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d6&subsys_30041259.DeviceDesc = "Allied Telesis AT-ANC10Sa/2 10G Dual Port Adapter"
pci\ven_14e4&dev_16cf&subsys_120214e4.DeviceDesc = "Broadcom M125cp NetXtreme C-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_16d7&subsys_414414e4.DeviceDesc = "Broadcom M225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d8&subsys_416314e4.DeviceDesc = "Broadcom M210tp NetXtreme-E Dual-port 10GBASE-T Ethernet OCP Adapter"
pci\ven_14e4&dev_16d7&subsys_094e15d9.DeviceDesc = "Supermicro SIOM 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_092815d9.DeviceDesc = "Supermicro 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_099615d9.DeviceDesc = "Supermicro SIOM 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_1a0815d9.DeviceDesc = "Supermicro 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_1a0915d9.DeviceDesc = "Supermicro Ultra Riser 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_060214E4.DeviceDesc = "Broadcom P210tep NetXtreme-E Dual-port 10GBASE-T Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_4877108e.DeviceDesc = "Oracle Dual Port 10Gb/25Gb SFP28 Cloud Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_8b17152d.DeviceDesc = "Broadcom BCM57416 NetXtreme-E 10GBASE-T RDMA Ethernet Controller"
pci\ven_14e4&dev_16e2&subsys_8b18152d.DeviceDesc = "Broadcom BCM57417 NetXtreme-E 10Gb/25Gb RDMA Ethernet Controller"
pci\ven_14e4&dev_16e3&subsys_8b19152d.DeviceDesc = "Broadcom BCM57416 NetXtreme-E 10Gb RDMA Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_16d815d9.DeviceDesc = "Supermicro 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_140714e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Ethernet OCP Adapter"
pci\ven_14e4&dev_16d8&subsys_416514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d6&subsys_412514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d7&subsys_414514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d7&subsys_414614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d6&subsys_412614e4.DeviceDesc = "Broadcom NetXtreme E-Series  Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d8&subsys_416614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d6&subsys_8b20152d.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d6&subsys_8b22152d.DeviceDesc = "Broadcom P125p NetXtreme E-Series Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_8b21152d.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_8b27152d.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_1b1e15d9.DeviceDesc = "Supermicro Ultra Riser 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_1b2615d9.DeviceDesc = "Supermicro Ultra Riser 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_29961259.DeviceDesc = "Allied Telesis AT-ANC40 40Gb Fiber Ethernet"
pci\ven_14e4&dev_16d8&subsys_404817aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port PCIe Ethernet LOM"
pci\ven_14e4&dev_16d8&subsys_416217aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16d7&subsys_414017aa.DeviceDesc = "Broadcom 57414 10/25GbE SFP28 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16d8&subsys_416317aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16d7&subsys_410517aa.DeviceDesc = "Broadcom 57414 10/25GbE SFP28 2-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_16d8&subsys_159214e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d8&subsys_159314e4.DeviceDesc = "Broadcom P210tep NetXtreme-E Dual-port 10GBASE-T Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d6&subsys_159414e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d6&subsys_159514e4.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d7&subsys_159614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16d7&subsys_159714e4.DeviceDesc = "Broadcom P225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d8&subsys_190110d3.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_1b7315d9.DeviceDesc = "Supermicro AIOM 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_8b28152d.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d8&subsys_10001458.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_16d715d9.DeviceDesc = "Supermicro 10Gb/25Gb Ethernet Controller"
pci\ven_14e4&dev_16d8&subsys_202018d4.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16d7&subsys_1033193d.DeviceDesc = "Broadcom P225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d6&subsys_1024193d.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16d8&subsys_405117aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port PCIe Ethernet LOM"


;*******************************************************************************
; Stratus physical device strings.
;*******************************************************************************

pci\ven_14e4&dev_16f1&subsys_16f114e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E 10Gb/25Gb/40Gb/50Gb/100Gb RDMA Ethernet Controller"
pci\ven_14e4&dev_16f1&subsys_452014e4.DeviceDesc = "Broadcom M150pm NetXtreme E-Series Ethernet OCP Adapter"
pci\ven_14e4&dev_1614&subsys_454014e4.DeviceDesc = "Broadcom P1100p NetXtreme-E Single-port 50Gb/100Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_1614&subsys_454114e4.DeviceDesc = "Broadcom M1100pm NetXtreme E-Series Single-port 50Gb/100Gb Ethernet OCP Adapter"
pci\ven_14e4&dev_1614&subsys_8b11152d.DeviceDesc = "Broadcom 57454 NetXtreme-E Quad-port 25Gb Ethernet OCP Adapter"
pci\ven_14e4&dev_1614&subsys_410017aa.DeviceDesc = "Broadcom 57454 10GBASE-T 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1614&subsys_410217aa.DeviceDesc = "Broadcom 57454 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1614&subsys_410117aa.DeviceDesc = "Broadcom 57454 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1614&subsys_404717aa.DeviceDesc = "Broadcom 57454  10GBASE-T 4-Port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1614&subsys_1b2715d9.DeviceDesc = "Supermicro PCIe 100Gb QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1614&subsys_d34014e4.DeviceDesc = "Broadcom NetXtreme-E N410SDBT BCM57454 4x10G BT OCP3.0 Ethernet"
pci\ven_14e4&dev_1614&subsys_d14014e4.DeviceDesc = "Broadcom NetXtreme-E P410SDBT BCM57454 4x10G BT PCIE Ethernet"

;*******************************************************************************
; Stingray physical device strings.
;*******************************************************************************

pci\ven_14e4&dev_16f0&subsys_16f014e4.DeviceDesc = "Broadcom NetXtreme-S Ethernet Controller"
pci\ven_14e4&dev_d802&subsys_802014e4.DeviceDesc = "Broadcom PS150-H16 NetXtreme-S Single-port 50Gb PCIe SmartNIC"
pci\ven_14e4&dev_d802&subsys_d80214e4.DeviceDesc = "Broadcom NetXtreme-S 50G Ethernet Controller"
pci\ven_14e4&dev_d804&subsys_d80414e4.DeviceDesc = "Broadcom NetXtreme-S 100G Ethernet Controller"
pci\ven_14e4&dev_d802&subsys_802114e4.DeviceDesc = "Broadcom PS225-H16 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_d802&subsys_802414e4.DeviceDesc = "Broadcom PS225-H04 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_d802&subsys_802814e4.DeviceDesc = "Broadcom PS225-H08 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_d804&subsys_804014e4.DeviceDesc = "Broadcom PS1100-H08 NetXtreme-S Single-port 100Gb PCIe SmartNIC"
pci\ven_14e4&dev_d802&subsys_802314e4.DeviceDesc = "Broadcom PS410T-H04 NetXtreme-S Stingray 4x10G 10GBase-T PCIe SmartNIC"


;*******************************************************************************
; Thor physical device strings.
;*******************************************************************************

pci\ven_14e4&dev_1752&subsys_100014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_112814e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_111614e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_175014e4.DeviceDesc = "Broadcom BCM57508 NetXtreme-E 200G Ethernet Controller"
pci\ven_14e4&dev_1751&subsys_175114e4.DeviceDesc = "Broadcom BCM57504 NetXtreme-E 100G Ethernet Controller"
pci\ven_14e4&dev_1752&subsys_175214e4.DeviceDesc = "Broadcom BCM57502 NetXtreme-E 50G Ethernet Controller"
pci\ven_14e4&dev_1751&subsys_504514e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_504614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_504914e4.DeviceDesc = "Broadcom NetXtreme E-Series  Dual-port 50Gb PCIe Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_541014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_100214e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T PCIe Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_100314e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10G SFP+ PCIe Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_520814e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_504714e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10Gb SFP+ OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_504814e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_110014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_210014e4.DeviceDesc = "Broadcom NetXtreme-E Dual-port 100Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_1750&subsys_220014e4.DeviceDesc = "Broadcom NetXtreme-E Single-port 200Gb HA Ethernet PCIe Adapter"
pci\ven_14e4&dev_1751&subsys_542514e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_510014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_515014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_1b3e15d9.DeviceDesc = "Supermicro PCIe 100Gb 2-ports QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1751&subsys_525014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-Port 25Gb Ethernet Network Daughter Card"
pci\ven_14e4&dev_1751&subsys_425014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_404c17aa.DeviceDesc = "Broadcom 57508 100GbE QSFP 2-port PCIe 4 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_510514e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 DSFP Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_510414e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_510114e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_510214e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_510314e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_515114e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_515214e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_515314e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_410017aa.DeviceDesc = "Broadcom 57502 10GBASE-T 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_410217aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_410317aa.DeviceDesc = "Broadcom 57504 50GbE SFP56 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_410117aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1752&subsys_404717aa.DeviceDesc = "Broadcom 57502 10GBASE-T 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_09D41028.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb Ethernet LOM"
pci\ven_14e4&dev_1750&subsys_1b8115d9.DeviceDesc = "Supermicro AIOM 100Gb 2-ports QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1750&subsys_520914e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_d12414e4.DeviceDesc = "Broadcom NetXtreme-E P2100D BCM57508 2x100G QSFP PCIE Ethernet"
pci\ven_14e4&dev_1751&subsys_d14214e4.DeviceDesc = "Broadcom NetXtreme-E P425D BCM57504 4x25G SFP28 PCIE Ethernet"
pci\ven_14e4&dev_1750&subsys_df2414e4.DeviceDesc = "Broadcom NetXtreme-E NGM2100D BCM57508 2x100G KR Mezz Ethernet"
pci\ven_14e4&dev_1751&subsys_159814e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_159914e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_159a14e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1750&subsys_159b14e4.DeviceDesc = "Broadcom NetXtreme-E-Series Dual-port 100Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_1750&subsys_410317aa.DeviceDesc = "Broadcom 57508 100GbE QSFP56 2-Port OCP Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_410717aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_405017aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1751&subsys_0b1b1028.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb Ethernet LOM"







;*******************************************************************************
; Whitney NPAR, Non-RoCE device strings.
;*******************************************************************************

pci\ven_14e4&dev_16d4&subsys_402014E4.DeviceDesc = "Broadcom BCM57402 NetXtreme-E Partition"
pci\ven_14e4&dev_16d4&subsys_16d014E4.DeviceDesc = "Broadcom BCM57402 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16e7&subsys_16d114E4.DeviceDesc = "Broadcom BCM57404 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16e7&subsys_040214E4.DeviceDesc = "Broadcom BCM57404 NetXtreme-E Partition"
pci\ven_14e4&dev_16e7&subsys_404114E4.DeviceDesc = "Broadcom BCM57404 NetXtreme-E Partition"
pci\ven_14e4&dev_16e7&subsys_312017aa.DeviceDesc = "Broadcom NX-C Single-port 25G PCIe Adapter"
pci\ven_14e4&dev_16e8&subsys_060214E4.DeviceDesc = "Broadcom BCM57406 NetXtreme-E Partition"
pci\ven_14e4&dev_16e8&subsys_406014E4.DeviceDesc = "Broadcom BCM57406 NetXtreme-E Partition"
pci\ven_14e4&dev_16e8&subsys_416017aa.DeviceDesc = "Broadcom NX-E Dual-port 10GBASE-T PCIe Adapter"
pci\ven_14e4&dev_16e8&subsys_16d214e4.DeviceDesc = "Broadcom BCM57406 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16ea&subsys_16d514e4.DeviceDesc = "Broadcom BCM57407 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16ea&subsys_16e914e4.DeviceDesc = "Broadcom BCM57407 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16d4&subsys_040214E4.DeviceDesc = "Broadcom NetXtreme-E Partition"

;*******************************************************************************
; Whitney+ NPAR, Non-RoCE device strings.
;*******************************************************************************

pci\ven_14E4&dev_16de&subsys_412014E4.DeviceDesc = "Broadcom BCM57412 NetXtreme-E Partition"
pci\ven_14E4&dev_16de&subsys_412114E4.DeviceDesc = "Broadcom BCM57412 NetXtreme-E Partition"
pci\ven_14E4&dev_16de&subsys_16d614E4.DeviceDesc = "Broadcom BCM57412 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16ec&subsys_16d714e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16ec&subsys_414114e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_140514e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_414014e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Partition"
pci\ven_14e4&dev_16ee&subsys_416114e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E Partition"
pci\ven_14e4&dev_16ee&subsys_416014e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E Partition"
pci\ven_14e4&dev_16ee&subsys_160214e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E Partition"
pci\ven_14e4&dev_16ee&subsys_416017aa.DeviceDesc = "Broadcom NX-E PCIe 10Gb 2-Port Base-T Ethernet Adapter"
pci\ven_14e4&dev_16ee&subsys_416117aa.DeviceDesc = "Broadcom NX-E ML2 10Gb 2-Port Base-T Ethernet Adapter"
pci\ven_14e4&dev_16ee&subsys_16d814e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16ee&subsys_16e314e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16ee&subsys_1fea1028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet LOM"
pci\ven_14e4&dev_16ee&subsys_1feb1028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10G SFP+ Ethernet LOM"
pci\ven_14e4&dev_16ee&subsys_07e51028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet LOM"
pci\ven_14e4&dev_16cc&subsys_16d914e4.DeviceDesc = "Broadcom BCM57417 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16cc&subsys_16e214e4.DeviceDesc = "Broadcom BCM57417 NetXtreme-E Partition" ; **
pci\ven_14e4&dev_16cc&subsys_4866108e.DeviceDesc = "Broadcom BCM57417 NetXtreme-E Partition"
pci\ven_14e4&dev_16de&subsys_412017aa.DeviceDesc = "Broadcom NX-E PCIe 25Gb 1-Port SFP28 Ethernet Adapter"
pci\ven_14e4&dev_16ec&subsys_140314e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_140214e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_140414e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16de&subsys_120214e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_3044108e.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_4869108e.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_414314e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16de&subsys_412314e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16de&subsys_412414e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_414414e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ee&subsys_416314e4.DeviceDesc = "Broadcom NetXtreme-E Partition"
pci\ven_14e4&dev_16ec&subsys_094e15d9.DeviceDesc = "Supermicro SIOM 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ec&subsys_092815d9.DeviceDesc = "Supermicro 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ee&subsys_099615d9.DeviceDesc = "Supermicro SIOM 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ee&subsys_1a0815d9.DeviceDesc = "Supermicro 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ee&subsys_1a0915d9.DeviceDesc = "Supermicro Ultra Riser 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ec&subsys_4877108e.DeviceDesc = "Oracle Dual Port 10Gb/25Gb SFP28 Cloud Ethernet Controller"
pci\ven_14e4&dev_16ee&subsys_8b17152d.DeviceDesc = "Broadcom BCM57416 NetXtreme-E Partition"
pci\ven_14e4&dev_16cc&subsys_8b18152d.DeviceDesc = "Broadcom BCM57417 NetXtreme-E Partition"
pci\ven_14e4&dev_16ee&subsys_8b19152d.DeviceDesc = "Broadcom BCM57416 NetXtreme-E Partition"
pci\ven_14e4&dev_16ee&subsys_16d815d9.DeviceDesc = "Supermicro 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ec&subsys_140714e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Ethernet OCP Adapter"
pci\ven_14e4&dev_16ee&subsys_416514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16de&subsys_412514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ec&subsys_414514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ec&subsys_414614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16de&subsys_412614e4.DeviceDesc = "Broadcom NetXtreme E-Series  Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ee&subsys_416614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ec&subsys_1b1e15d9.DeviceDesc = "Supermicro Ultra Riser 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ec&subsys_1b2615d9.DeviceDesc = "Supermicro Ultra Riser 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ee&subsys_404817aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port PCIe Ethernet LOM"
pci\ven_14e4&dev_16ee&subsys_416217aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16ec&subsys_414017aa.DeviceDesc = "Broadcom 57414 10/25GbE SFP28 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16ee&subsys_416317aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16ec&subsys_410517aa.DeviceDesc = "Broadcom 57414 10/25GbE SFP28 2-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_16ee&subsys_159214e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ee&subsys_159314e4.DeviceDesc = "Broadcom P210tep NetXtreme-E Dual-port 10GBASE-T Ethernet PCIe Adapter"
pci\ven_14e4&dev_16de&subsys_159414e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16de&subsys_159514e4.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ec&subsys_159614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ec&subsys_159714e4.DeviceDesc = "Broadcom P225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ee&subsys_190110d3.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ec&subsys_1b7315d9.DeviceDesc = "Supermicro AIOM 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16de&subsys_8b20152d.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16de&subsys_8b22152d.DeviceDesc = "Broadcom P125p NetXtreme E-Series Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ec&subsys_8b21152d.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ec&subsys_8b28152d.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ee&subsys_10001458.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ec&subsys_16d715d9.DeviceDesc = "Supermicro 10Gb/25Gb Ethernet Controller"
pci\ven_14e4&dev_16ee&subsys_202018d4.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ec&subsys_1033193d.DeviceDesc = "Broadcom P225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16de&subsys_1024193d.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ee&subsys_405117aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port PCIe Ethernet LOM"
pci\ven_14e4&dev_16de&subsys_30041259.DeviceDesc = "Allied Telesis AT-ANC10Sa/2 Partition"
pci\ven_14e4&dev_16ee&subsys_30031259.DeviceDesc = "Allied Telesis AT-ANC10T/2 Partition"



;*******************************************************************************
; Stratus NPAR, Non-RoCE device strings.
;*******************************************************************************

pci\ven_14e4&dev_1604&subsys_452014e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E Partition"
pci\ven_14e4&dev_1604&subsys_454014e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E Partition"
pci\ven_14e4&dev_1604&subsys_454114e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E Partition"
pci\ven_14e4&dev_1604&subsys_16f014e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E Partition"
pci\ven_14e4&dev_1604&subsys_16f114e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E Partition"
pci\ven_14e4&dev_1604&subsys_160414e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E Partition"
pci\ven_14e4&dev_1604&subsys_410017aa.DeviceDesc = "Broadcom 57454 10GBASE-T 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1604&subsys_410217aa.DeviceDesc = "Broadcom 57454 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1604&subsys_410117aa.DeviceDesc = "Broadcom 57454 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1604&subsys_404717aa.DeviceDesc = "Broadcom 57454  10GBASE-T 4-Port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1604&subsys_1b2715d9.DeviceDesc = "Supermicro PCIe 100Gb QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1604&subsys_d34014e4.DeviceDesc = "Broadcom NetXtreme-E N410SDBT BCM57454 4x10G BT OCP3.0 Ethernet Partition"
pci\ven_14e4&dev_1604&subsys_d14014e4.DeviceDesc = "Broadcom NetXtreme-E P410SDBT BCM57454 4x10G BT PCIE Ethernet Partition"

;*******************************************************************************
; Stingray NPAR, Non-RoCE device strings.
;*******************************************************************************

pci\ven_14e4&dev_1794&subsys_802014e4.DeviceDesc = "Broadcom PS150-H16 NetXtreme-S Single-port 50Gb PCIe SmartNIC"
pci\ven_14e4&dev_1794&subsys_802114e4.DeviceDesc = "Broadcom PS225-H16 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_1794&subsys_802414e4.DeviceDesc = "Broadcom PS225-H04 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_1794&subsys_802814e4.DeviceDesc = "Broadcom PS225-H08 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_1796&subsys_804014e4.DeviceDesc = "Broadcom PS1100-H08 NetXtreme-S Single-port 100Gb PCIe SmartNIC"
pci\ven_14e4&dev_1794&subsys_802314e4.DeviceDesc = "Broadcom PS410T-H04 NetXtreme-S Stingray 4x10G 10GBase-T PCIe SmartNIC"


;*******************************************************************************
; Thor NPAR, Non-RoCE device strings.
;*******************************************************************************

pci\ven_14e4&dev_1800&subsys_100014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_112814e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_111614e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_504514e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_504614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_504914e4.DeviceDesc = "Broadcom NetXtreme E-Series  Dual-port 50Gb PCIe Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_541014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_100214e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T PCIe Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_100314e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10G SFP+ PCIe Ethernet Adapter"
pci\ven_14e4&dev_1802&subsys_520814e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_504714e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10Gb SFP+ OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_504814e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_110014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1802&subsys_210014e4.DeviceDesc = "Broadcom NetXtreme-E Dual-port 100Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_1802&subsys_220014e4.DeviceDesc = "Broadcom NetXtreme-E Single-port 200Gb HA Ethernet PCIe Adapter"
pci\ven_14e4&dev_1801&subsys_542514e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_510014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_510514e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP DSFP Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_515014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1802&subsys_1b3e15d9.DeviceDesc = "Supermicro PCIe 100Gb 2-ports QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1801&subsys_525014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-Port 25Gb Ethernet Network Daughter Card"
pci\ven_14e4&dev_1801&subsys_425014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Adapter"
pci\ven_14e4&dev_1802&subsys_404c17aa.DeviceDesc = "Broadcom 57508 100GbE QSFP 2-port PCIe 4 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_510414e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_510114e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_510214e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_510314e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_515114e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_515214e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_515314e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_410017aa.DeviceDesc = "Broadcom 57502 10GBASE-T 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_410217aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_410317aa.DeviceDesc = "Broadcom 57504 50GbE SFP56 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_410117aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1800&subsys_404717aa.DeviceDesc = "Broadcom 57502 10GBASE-T 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_09D41028.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb Ethernet LOM"
pci\ven_14e4&dev_1802&subsys_1b8115d9.DeviceDesc = "Supermicro AIOM 100Gb 2-ports QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1802&subsys_520914e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1802&subsys_d12414e4.DeviceDesc = "Broadcom NetXtreme-E P2100D BCM57508 2x100G QSFP PCIE Ethernet Partition"
pci\ven_14e4&dev_1801&subsys_d14214e4.DeviceDesc = "Broadcom NetXtreme-E P425D BCM57504 4x25G SFP28 PCIE Ethernet Partition"
pci\ven_14e4&dev_1802&subsys_df2414e4.DeviceDesc = "Broadcom NetXtreme-E NGM2100D BCM57508 2x100G KR Mezz Ethernet Partition"
pci\ven_14e4&dev_1801&subsys_159814e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 OCP 3.0 Ethernet Partition"
pci\ven_14e4&dev_1801&subsys_159914e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Partition"
pci\ven_14e4&dev_1802&subsys_159a14e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Partition"
pci\ven_14e4&dev_1802&subsys_159b14e4.DeviceDesc = "Broadcom NetXtreme-E-Series Dual-port 100Gb Ethernet PCIe Partition"
pci\ven_14e4&dev_1802&subsys_410317aa.DeviceDesc = "Broadcom 57508 100GbE QSFP56 2-Port OCP Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_410717aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_405017aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1801&subsys_0b1b1028.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb Ethernet LOM"



;*******************************************************************************
; Whitney+ NPAR, RoCE device strings.
;*******************************************************************************

pci\ven_14E4&dev_16eb&subsys_412014E4.DeviceDesc = "Broadcom BCM57412 NetXtreme-E RDMA Partition"
pci\ven_14E4&dev_16eb&subsys_412114E4.DeviceDesc = "Broadcom BCM57412 NetXtreme-E RDMA Partition"
pci\ven_14E4&dev_16eb&subsys_16d614E4.DeviceDesc = "Broadcom BCM57412 NetXtreme-E RDMA Partition" ; **
pci\ven_14e4&dev_16ed&subsys_16d714e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E RDMA Partition" ; **
pci\ven_14e4&dev_16ed&subsys_414114e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_140514e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_414014e4.DeviceDesc = "Broadcom BCM57414 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_416114e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_416014e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_160214e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_416017aa.DeviceDesc = "Broadcom NX-E PCIe 10Gb 2-Port Base-T Ethernet Adapter"
pci\ven_14e4&dev_16ef&subsys_416117aa.DeviceDesc = "Broadcom NX-E ML2 10Gb 2-Port Base-T Ethernet Adapter"
pci\ven_14e4&dev_16ef&subsys_16d814e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E RDMA Partition" ; **
pci\ven_14e4&dev_16ef&subsys_16e314e4.DeviceDesc = "Broadcom BCM57416 NetXtreme-E RDMA Partition" ; **
pci\ven_14e4&dev_16ef&subsys_1fea1028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T LOM"
pci\ven_14e4&dev_16ef&subsys_1feb1028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10G SFP+ Ethernet LOM"
pci\ven_14e4&dev_16ef&subsys_07e51028.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10G SFP+ Ethernet LOM"
pci\ven_14e4&dev_16c0&subsys_16d914e4.DeviceDesc = "Broadcom BCM57417 NetXtreme-E RDMA Partition" ; **
pci\ven_14e4&dev_16c0&subsys_16e214e4.DeviceDesc = "Broadcom BCM57417 NetXtreme-E RDMA Partition" ; **
pci\ven_14e4&dev_16c0&subsys_4866108e.DeviceDesc = "Broadcom BCM57417 NetXtreme-E Partition"
pci\ven_14e4&dev_16eb&subsys_412017aa.DeviceDesc = "Broadcom NX-E PCIe 25Gb 1-Port SFP28 Ethernet Adapter"
pci\ven_14e4&dev_16ed&subsys_140314e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_140214e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_140414e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16eb&subsys_120214e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_3044108e.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_4869108e.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_414314e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16eb&subsys_412314e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16eb&subsys_412414e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_414414e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_416314e4.DeviceDesc = "Broadcom NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ed&subsys_094e15d9.DeviceDesc = "Supermicro SIOM 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ed&subsys_092815d9.DeviceDesc = "Supermicro 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ef&subsys_099615d9.DeviceDesc = "Supermicro SIOM 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ef&subsys_1a0815d9.DeviceDesc = "Supermicro 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ef&subsys_1a0915d9.DeviceDesc = "Supermicro Ultra Riser 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ed&subsys_4877108e.DeviceDesc = "Oracle Dual Port 10Gb/25Gb SFP28 Cloud Ethernet Controller"
pci\ven_14e4&dev_16ef&subsys_8b17152d.DeviceDesc = "Broadcom BCM57416 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16c0&subsys_8b18152d.DeviceDesc = "Broadcom BCM57417 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_8b19152d.DeviceDesc = "Broadcom BCM57416 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_16d815d9.DeviceDesc = "Supermicro 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ed&subsys_140714e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Ethernet OCP Adapter"
pci\ven_14e4&dev_16ef&subsys_416514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16eb&subsys_412514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ed&subsys_414514e4.DeviceDesc = "Broadcom NetXtreme E-Series Advanced Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ed&subsys_414614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16eb&subsys_412614e4.DeviceDesc = "Broadcom NetXtreme E-Series  Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ef&subsys_416614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ed&subsys_1b1e15d9.DeviceDesc = "Supermicro Ultra Riser 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ed&subsys_1b2615d9.DeviceDesc = "Supermicro Ultra Riser 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16ef&subsys_404817aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port PCIe Ethernet LOM"
pci\ven_14e4&dev_16ef&subsys_416217aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16ed&subsys_414017aa.DeviceDesc = "Broadcom 57414 10/25GbE SFP28 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16ef&subsys_416317aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_16ed&subsys_410517aa.DeviceDesc = "Broadcom 57414 10/25GbE SFP28 2-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_16ef&subsys_159214e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10GBASE-T Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ef&subsys_159314e4.DeviceDesc = "Broadcom P210tep NetXtreme-E Dual-port 10GBASE-T Ethernet PCIe Adapter"
pci\ven_14e4&dev_16eb&subsys_159414e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 10Gb SFP+ Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16eb&subsys_159514e4.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ed&subsys_159614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 25Gb SFP28 Ethernet OCP 3.0 Adapter"
pci\ven_14e4&dev_16ed&subsys_159714e4.DeviceDesc = "Broadcom P225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ef&subsys_190110d3.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ed&subsys_1b7315d9.DeviceDesc = "Supermicro AIOM 25Gb SFP28 Ethernet Controller"
pci\ven_14e4&dev_16eb&subsys_8b20152d.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16eb&subsys_8b22152d.DeviceDesc = "Broadcom P125p NetXtreme E-Series Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ed&subsys_8b21152d.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ed&subsys_8b28152d.DeviceDesc = "Broadcom BCM57414 NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ef&subsys_10001458.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ed&subsys_16d715d9.DeviceDesc = "Supermicro 10Gb/25Gb Ethernet Controller"
pci\ven_14e4&dev_16ef&subsys_202018d4.DeviceDesc = "Broadcom NetXtreme-E Dual-port 10GBASE-T Ethernet Controller"
pci\ven_14e4&dev_16ed&subsys_1033193d.DeviceDesc = "Broadcom P225p NetXtreme-E Dual-port 10Gb/25Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16eb&subsys_1024193d.DeviceDesc = "Broadcom P210p NetXtreme-E Dual-port 10Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_16ef&subsys_405117aa.DeviceDesc = "Broadcom 57416 10GBASE-T 2-port PCIe Ethernet LOM"
pci\ven_14e4&dev_16eb&subsys_30041259.DeviceDesc = "Allied Telesis AT-ANC10Sa/2 RDMA Partition"
pci\ven_14e4&dev_16ef&subsys_30031259.DeviceDesc = "Allied Telesis AT-ANC10T/2 RDMA Partition"


;*******************************************************************************
; Stratus, RoCE device strings.
;*******************************************************************************

pci\ven_14e4&dev_1605&subsys_452014e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_1605&subsys_454014e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_1605&subsys_454114e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_1605&subsys_16f014e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_1605&subsys_16f114e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_1605&subsys_160514e4.DeviceDesc = "Broadcom BCM57320 NetXtreme-E RDMA Partition"
pci\ven_14e4&dev_1605&subsys_410017aa.DeviceDesc = "Broadcom 57454 10GBASE-T 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1605&subsys_410217aa.DeviceDesc = "Broadcom 57454 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1605&subsys_410117aa.DeviceDesc = "Broadcom 57454 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1605&subsys_404717aa.DeviceDesc = "Broadcom 57454  10GBASE-T 4-Port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1605&subsys_1b2715d9.DeviceDesc = "Supermicro PCIe 100Gb QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1605&subsys_d34014e4.DeviceDesc = "Broadcom NetXtreme-E N410SDBT BCM57454 4x10G BT OCP3.0 RDMA Partition"
pci\ven_14e4&dev_1605&subsys_d14014e4.DeviceDesc = "Broadcom NetXtreme-E P410SDBT BCM57454 4x10G BT PCIE RDMA Partition"

;*******************************************************************************
; Stingray, RoCE device strings.
;*******************************************************************************

pci\ven_14e4&dev_1795&subsys_802014e4.DeviceDesc = "Broadcom PS150-H16 NetXtreme-S Single-port 50Gb PCIe SmartNIC"
pci\ven_14e4&dev_1795&subsys_802114e4.DeviceDesc = "Broadcom PS225-H16 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_1795&subsys_802414e4.DeviceDesc = "Broadcom PS225-H04 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_1795&subsys_802814e4.DeviceDesc = "Broadcom PS225-H08 NetXtreme-S Dual-port 25Gb PCIe SmartNIC"
pci\ven_14e4&dev_1797&subsys_804014e4.DeviceDesc = "Broadcom PS1100-H08 NetXtreme-S Single-port 100Gb PCIe SmartNIC"
pci\ven_14e4&dev_1795&subsys_802314e4.DeviceDesc = "Broadcom PS410T-H04 NetXtreme-S Stingray 4x10G 10GBase-T PCIe SmartNIC"


;*******************************************************************************
; Thor, RoCE device strings.
;*******************************************************************************

pci\ven_14e4&dev_1803&subsys_100014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_112814e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_111614e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_504514e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_504614e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_504914e4.DeviceDesc = "Broadcom NetXtreme E-Series  Dual-port 50Gb PCIe Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_541014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_100214e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10GBASE-T PCIe Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_100314e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10G SFP+ PCIe Ethernet Adapter"
pci\ven_14e4&dev_1805&subsys_520814e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_504714e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 10Gb SFP+ OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_504814e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_110014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP Ethernet Adapter"
pci\ven_14e4&dev_1805&subsys_210014e4.DeviceDesc = "Broadcom NetXtreme-E Dual-port 100Gb Ethernet PCIe Adapter"
pci\ven_14e4&dev_1805&subsys_220014e4.DeviceDesc = "Broadcom NetXtreme-E Single-port 200Gb HA Ethernet PCIe Adapter"
pci\ven_14e4&dev_1804&subsys_542514e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_510014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_510514e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 DSFP Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_515014e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1805&subsys_1b3e15d9.DeviceDesc = "Supermicro PCIe 100Gb 2-ports QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1804&subsys_525014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-Port 25Gb Ethernet Network Daughter Card"
pci\ven_14e4&dev_1804&subsys_425014e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe Ethernet Adapter"
pci\ven_14e4&dev_1805&subsys_404c17aa.DeviceDesc = "Broadcom 57508 100GbE QSFP 2-port PCIe 4 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_510414e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_510114e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_510214e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_510314e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_515114e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_515214e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_515314e4.DeviceDesc = "Broadcom NetXtreme E-Series Single Port 50Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_410017aa.DeviceDesc = "Broadcom 57502 10GBASE-T 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_410217aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_410317aa.DeviceDesc = "Broadcom 57504 50GbE SFP56 2-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_410117aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1803&subsys_404717aa.DeviceDesc = "Broadcom 57502 10GBASE-T 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_09D41028.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb Ethernet LOM"
pci\ven_14e4&dev_1805&subsys_1b8115d9.DeviceDesc = "Supermicro AIOM 100Gb 2-ports QSFP28 Ethernet Controller"
pci\ven_14e4&dev_1805&subsys_520914e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 Ethernet Adapter"
pci\ven_14e4&dev_1805&subsys_d12414e4.DeviceDesc = "Broadcom NetXtreme-E P2100D BCM57508 2x100G QSFP PCIE RDMA Partition"
pci\ven_14e4&dev_1804&subsys_d14214e4.DeviceDesc = "Broadcom NetXtreme-E P425D BCM57504 4x25G SFP28 PCIE RDMA Partition"
pci\ven_14e4&dev_1805&subsys_df2414e4.DeviceDesc = "Broadcom NetXtreme-E NGM2100D BCM57508 2x100G KR Mezz RDMA Partition"
pci\ven_14e4&dev_1804&subsys_159814e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 OCP 3.0 RDMA Partition"
pci\ven_14e4&dev_1804&subsys_159914e4.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb SFP28 PCIe RDMA Partition"
pci\ven_14e4&dev_1805&subsys_159a14e4.DeviceDesc = "Broadcom NetXtreme E-Series Dual-port 100Gb OCP 3.0 RDMA Partition"
pci\ven_14e4&dev_1805&subsys_159b14e4.DeviceDesc = "Broadcom NetXtreme-E-Series Dual-port 100Gb Ethernet PCIe RDMA Partition"
pci\ven_14e4&dev_1805&subsys_410317aa.DeviceDesc = "Broadcom 57508 100GbE QSFP56 2-Port OCP Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_410717aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port PCIe Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_405017aa.DeviceDesc = "Broadcom 57504 10/25GbE SFP28 4-port OCP Ethernet Adapter"
pci\ven_14e4&dev_1804&subsys_0b1b1028.DeviceDesc = "Broadcom NetXtreme E-Series Quad-port 25Gb Ethernet LOM"



;*******************************************************************************
; VF, Non-RoCE device strings.
;*******************************************************************************
; Cumulus
pci\ven_14e4&dev_16cb.DeviceDesc = "Broadcom NetXtreme-C Virtual Function"
; Cumulus+
pci\ven_14e4&dev_16e1.DeviceDesc = "Broadcom NetXtreme-C Virtual Function"
; Whitney
pci\ven_14e4&dev_16d3.DeviceDesc = "Broadcom NetXtreme-E Virtual Function"
; Whitney+
pci\ven_14e4&dev_16dc.DeviceDesc = "Broadcom NetXtreme-E Virtual Function"
; Stratus
pci\ven_14e4&dev_1609.DeviceDesc = "Broadcom NetXtreme-E Virtual Function"
; Stingray
pci\ven_14e4&dev_d800.DeviceDesc = "Broadcom NetXtreme-S Virtual Function"

; Thor
pci\ven_14e4&dev_1806.DeviceDesc = "Broadcom NetXtreme-E Virtual Function"


pci\ven_14e4&dev_16f4.DeviceDesc = "Broadcom NetXtreme-S Virtual Function"

;*******************************************************************************
; VF, RoCE device strings.
;*******************************************************************************
; Cumulus+
pci\ven_14e4&dev_16e5.DeviceDesc = "Broadcom NetXtreme-C Virtual Function"
; Whitney+
pci\ven_14e4&dev_16c1.DeviceDesc = "Broadcom NetXtreme-E Virtual Function"
; Stratus
pci\ven_14e4&dev_1606.DeviceDesc = "Broadcom NetXtreme-E Virtual Function"
; Stingray
pci\ven_14e4&dev_d801.DeviceDesc = "Broadcom NetXtreme-S Virtual Function"

; Thor
pci\ven_14e4&dev_1807.DeviceDesc = "Broadcom NetXtreme-E Virtual Function"


;*******************************************************************************
; VF for Hyper-V, Non-RoCE device strings.
;*******************************************************************************
; Cumulus
pci\ven_14e4&dev_16c2.DeviceDesc = "Broadcom NetXtreme-C Virtual Function for Hyper-V"
; Cumulus+
pci\ven_14e4&dev_16c3.DeviceDesc = "Broadcom NetXtreme-C Virtual Function for Hyper-V"
; Whitney
pci\ven_14e4&dev_16c4.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"
; Whitney+
pci\ven_14e4&dev_16c5.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"
; Stratus
pci\ven_14e4&dev_1607.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"
; Stingray
pci\ven_14e4&dev_1792.DeviceDesc = "Broadcom NetXtreme-S Virtual Function for Hyper-V"

; Thor
pci\ven_14e4&dev_1808.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"


;*******************************************************************************
; VF for Hyper-V, RoCE device strings.
;*******************************************************************************
; Cumulus+
pci\ven_14e4&dev_16e6.DeviceDesc = "Broadcom NetXtreme-C Virtual Function for Hyper-V"
; Whitney+
pci\ven_14e4&dev_16bd.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"
pci\ven_14e4&dev_16b6.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"
; Stratus
pci\ven_14e4&dev_1608.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"
; Stingray
pci\ven_14e4&dev_1793.DeviceDesc = "Broadcom NetXtreme-S Virtual Function for Hyper-V"

; Thor
pci\ven_14e4&dev_1809.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"


pci\ven_14e4&dev_2088.DeviceDesc = "Broadcom NetXtreme-E Virtual Function for Hyper-V"


;*******************************************************************************
; End of device strings.
;*******************************************************************************

speed_duplex_desc           = "Speed & Duplex"
speed_duplex_auto           = "Auto Negotiation"
speed_duplex_10Mb_hd        = "10 Mbps Half Duplex"
speed_duplex_10Mb_fd        = "10 Mbps Full Duplex"
speed_duplex_100Mb_hd       = "100 Mbps Half Duplex"
speed_duplex_100Mb_fd       = "100 Mbps Full Duplex"
speed_duplex_1Gb_fd_an      = "1.0 Gbps Full Auto"
speed_duplex_1Gb_fd         = "1.0 Gbps Full Duplex"
speed_duplex_10Gb_fd        = "10 Gbps Full Duplex"
speed_duplex_20Gb_fd        = "20 Gbps Full Duplex"
speed_duplex_25Gb_fd        = "25 Gbps Full Duplex"
speed_duplex_40Gb_fd        = "40 Gbps Full Duplex"
speed_duplex_50Gb_fd        = "50 Gbps Full Duplex"
speed_duplex_100Gb_fd       = "100 Gbps Full Duplex"
speed_duplex_200Gb_fd       = "200 Gbps Full Duplex"

priority_vlan_desc          = "Priority & VLAN"
priority_vlan_disabled      = "Priority & VLAN disabled"
priority_enabled            = "Priority enabled"
vlan_enabled                = "VLAN enabled"
priority_vlan_enabled       = "Priority & VLAN enabled"

taskoffload_desc_ipv4       = "TCP/UDP Checksum Offload (IPv4)"
taskoffload_desc_ipv6       = "TCP/UDP Checksum Offload (IPv6)"
taskoffload_disabled        = "Disabled"
taskoffload_tx_cksum        = "Tx Enabled"
taskoffload_rx_cksum        = "Rx Enabled"
taskoffload_rx_tx_cksum     = "Rx & Tx Enabled"

flow_ctrl                   = "Flow Control"
flow_ctrl_disabled          = "Disabled"
flow_ctrl_rx                = "Rx Enabled"
flow_ctrl_tx                = "Tx Enabled"
flow_ctrl_rx_tx             = "Rx & Tx Enabled"
flow_ctrl_auto              = "Auto Negotiation"

enabled                     = "Enabled"
disabled                    = "Disabled"
wire_speed                  = "Ethernet@WireSpeed"
mtu_desc                    = "Jumbo Packet"
rss_queue_cnt_desc          = "Maximum Number of RSS Queues"
vlan_id_desc                = "VLAN ID"
network_address             = "Locally Administered Address"
eee_desc                    = "Energy-Efficient Ethernet"
lso_desc_ipv4               = "Large Send Offload V2 (IPv4)"
lso_desc_ipv6               = "Large Send Offload V2 (IPv6)"

rss_desc                    = "Receive Side Scaling"
rss_profile_desc            = "RSS load balancing profile"
rss_profile_cp              = "ClosestProcessor"
rss_profile_cps             = "ClosestProcessorStatic"
rss_profile_ns              = "NUMAScaling"
rss_profile_nss             = "NUMAScalingStatic"
rss_profile_cs              = "ConservativeScaling"
numa_node_desc              = "Preferred NUMA node"
tx_bufs_desc                = "Transmit Buffers (0=Auto)"
rx_bufs_desc                = "Receive Buffers (0=Auto)"
vmq_desc                    = "Virtual Machine Queues"
intr_mod_desc               = "Interrupt Moderation"
im_cfg_desc                 = "Interrupt Moderation Configuration"
im_low_desc                 = "Low"
im_med_desc                 = "Medium"
im_high_desc                = "High"
Wake_on_magic_desc          = "Wake On Magic Packet"
wake_on_pattern_desc        = "Wake On Pattern Match"
enable_pme_on_shutdown_desc = "Enable PME on shutdown"
sriov_desc                  = "SR-IOV"
ipv4_rsc_desc               = "Recv Segment Coalescing (IPv4)"
ipv6_rsc_desc               = "Recv Segment Coalescing (IPv6)"
</ndis63>
qos_desc                    = "Quality of Service"
nvgre_desc                  = "Encapsulated Task Offload"
max_rss_processors_desc     = "Maximum Number of RSS Processors"
rss_base_proc_number_desc   = "RSS Base Processor Number"
rss_max_proc_number_desc    = "Maximum RSS Processor Number"
rss_base_group_proc_number_desc = "RSS Base Processor Group"
rss_max_group_proc_number_desc = "RSS Max Processor Group"
max_num_msix_messages     = "Maximum Number of MSI-X Messages"

roce_mtu_256                = "256"
roce_mtu_512                = "512"
roce_mtu_1024               = "1024"
roce_mtu_2048               = "2048"
roce_mtu_4096               = "4096"
fec_cl74                    = "CL74 with Force Mode"
fec_cl91                    = "CL91 with Force Mode"
fec_rs544_1xn               = "RS544 1xn with Force Mode"
fec_rs544_ieee              = "RS544 IEEE with Force Mode"
fec_rs272_1xn               = "RS272 1xn with Force Mode"
fec_rs272_ieee              = "RS272 IEEE with Force Mode"
fec_auto                    = "Auto Negotiation"
fec_desc                    = "Forward Error Correction"
vf_spoofing_protection      = "VF Spoofing Protection"
MSFT                        = "Microsoft"

