;*******************************************************************************
; Copyright 2001-2022 Broadcom Limited.
; Copyright © 2005-2022 Broadcom. All Rights Reserved.
; The term “Broadcom” refers to Broadcom Inc. and/or its subsidiaries.
;
; INF for NTamd64.6.0 Windows Vista and Server 2008
;
; InfVersion   221.0.5.0B
;
;*******************************************************************************

[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile = b57nd60a.cat
Compatible  = 1
Provider    = %BRCM%
DriverVer   = 09/05/2022,221.0.5.0

[Manufacturer]
%BRCM% = Broadcom, NTamd64.6.0, NTamd64.6.1

;*******************************************************************************
; Vista install sections.
;*******************************************************************************
[Broadcom.NTamd64.6.0]
%3C998SX%           =  3C998SX_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C998T%            =  3C998T_LHinst.NTamd64.6.0,                   PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C999T%            =  3C999T_LHinst.NTamd64.6.0,                   PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%BCM5703%           =  BCM5703G_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1647
%BCM5703%           =  BCM5703G_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16a7
%BCM5703%           =  BCM5703G_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16C7
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703SW%         =  BCM5703SW_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704%           =  BCM5704G_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1648
%BCM5704S%          =  BCM5704S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16A8
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.0,              PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.0,              PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.0,              PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.0,              PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_16A8&SUBSYS_03331014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1654
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014
%BCM5705%           =  BCM5705_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1653
%BCM5705F%          =  BCM5705F_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_166e
%BCM5705F%          =  BCM5705F_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%BCM5705FHA%        =  BCM5705F_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705FHB%        =  BCM5705F_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5705M%          =  BCM5705MA2F2N_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%          =  BCM5705MA2F2N_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_165E&SUBSYS_127910cf
%BCM5705M%          =  BCM5705MA2F2N_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165E
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165E&SUBSYS_0727152d
%BCM5705M%          =  BCM5705M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165D
%BCM5714%           =  BCM5714G_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1668
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_166A&SUBSYS_03131014
%BCM5714%           =  BCM5780X_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_166A
%BCM5714%           =  BCM5780X_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_166A&SUBSYS_107F1734
%BCM5714%           =  BCM5714G_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1678
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1678&SUBSYS_032a1014
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1678&SUBSYS_108C1734
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1669
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1669&SUBSYS_03281014
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1679&SUBSYS_03671014
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64_i.6.0,            PCI\VEN_14e4&DEV_1669&SUBSYS_03861014
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64_i.6.0,            PCI\VEN_14e4&DEV_1669&SUBSYS_03871014
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_166B
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1679
%BCM5714S%          =  BCM5714SWol_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1679&SUBSYS_399710f1

%BCM5750A1%         =  BCM5750A1F3Me_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%         =  BCM5750A1F3Me_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1%         =  BCM5750A1F3MNe_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%         =  BCM5750A1F3MNe_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167D&SUBSYS_832a1033
%BCM5750A1%         =  BCM5750A1F3E_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5750A1%         =  BCM5750A1F3Ne_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%         =  BCM5750A1F3Ne_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033
%BCM5750A1%         =  BCM5750A1MeStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1601
%BCM5750A1%         =  BCM5750A1MeStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_167D
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD
%BCM5750A1%         =  BCM5750A1SPECIAL_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_81AA104D
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_108B1734
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_5047107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_5048107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_0280107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_0215107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_0460107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_0604107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1600&SUBSYS_03301014
%BCM5750A1%         =  BCM5750A1HALe_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1601&SUBSYS_202017AA
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1658
%BCM5750A1%         =  BCM5750A1G_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1659
%BCM5750A1%         =  BCM5750A1X_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014
%BCM5750A1%         =  BCM5750A1X_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1659&SUBSYS_02C61014
%BCM5750A1%         =  BCM5750A1X_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1676
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_00631025
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_10961734
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_167C
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_16F7
%BCM5750A1%         =  BCM5750MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_167D&SUBSYS_05771014
%BCM5750A1%         =  BCM5750MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_167D&SUBSYS_208117AA
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01791028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_01A71028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_01A81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1600&SUBSYS_01AD1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C11028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01CF1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C21028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01CC1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01D61028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_01CE1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1600&SUBSYS_02011028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_019c1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_01E01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_1677&SUBSYS_02071028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_16F7&SUBSYS_01BF1028

%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_01da1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_024E1028
%BCM5750A1CLNAHKD%  =  BCM5755A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167B&SUBSYS_01da1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_01de1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_01e11028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_01ec1028

%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167E
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167E&SUBSYS_01E41028
%BCM5750A1F%        =  BCM5750FHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014
%BCM5750A1STSP%     =  BCM5750A1STSP_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1659&SUBSYS_3260103c
%BCM5750B0%         =  BCM5750B0MHAL_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_10
%BCM5750B0F%        =  BCM5750B0MFHAL_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_10
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%           =  BCM5750X_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01

%BCM5754%           =  BCM5754A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167A
%BCM5754%           =  BCM5754A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_167A&SUBSYS_01fe1734
%BCM5754%           =  BCM5754A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167A&SUBSYS_10fe1734
%BCM5754%           =  BCM5754A1MeStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1672
%BCM5750A1CLNAHKD%  =  BCM5754A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1672&SUBSYS_01f71028
%BCM5750A1CLNAHKD%  =  BCM5754A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1672&SUBSYS_02021028

%BCM5755%           =  BCM5755A1MeStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1673
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673&SUBSYS_01fa1028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673&SUBSYS_01f91028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673&SUBSYS_02061028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673&SUBSYS_01fe1028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673&SUBSYS_02001028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673&SUBSYS_024A1028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1673&SUBSYS_01ff1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_169B&SUBSYS_02201028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_021D1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_021E1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_167A&SUBSYS_02141028

%BCM5750A1%         =  BCM5755A1MeStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1674
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1674&SUBSYS_01f81028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1674&SUBSYS_02041028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1674&SUBSYS_02641028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1674&SUBSYS_02651028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1674&SUBSYS_02621028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1674&SUBSYS_02631028

%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_02541028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_02551028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_02561028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_02571028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_025A1028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_025B1028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_1693&SUBSYS_02CA1028

%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01391025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_013B1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_013C1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_013D1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01421025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01431025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01451025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01471025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01481025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01491025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_014A1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_014B1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_01601025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_01611025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_019C1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_019D1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_019E1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_019F1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02001025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02011025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02021025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02031025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02041025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02051025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02061025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02071025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02081025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02091025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_020A1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_020B1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_020C1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_020D1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_020E1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_020F1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02101025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02111025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02121025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02131025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02141025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02151025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02161025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02191025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_021A1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_021B1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_021C1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_021D1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.0,         PCI\VEN_14e4&DEV_1684&SUBSYS_02211025

%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_0173107B
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_0174107B

%BCM5764M%          =  BCM5764M_LHinst_P_Lowest.NTamd64.6.0,        PCI\VEN_14e4&DEV_1684&SUBSYS_1309103C
%BCM5764M%          =  BCM5764M_LHinst_P_Lowest.NTamd64.6.0,        PCI\VEN_14e4&DEV_1684&SUBSYS_130A103C
%BCM5764M%          =  BCM5764M_LHinst_P_Lowest.NTamd64.6.0,        PCI\VEN_14e4&DEV_1684&SUBSYS_130B103C
%BCM5764M%          =  BCM5764M_LHinst_P.NTamd64.6.0,               PCI\VEN_14e4&DEV_1684&SUBSYS_1503103C
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_2821103C

%BCM5750A1CLNAHKD%  =  BCM5764MCLNAHKD.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_02811028
%BCM5750A1CLNAHKD%  =  BCM5764MCLNAHKD.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_02C31028
%BCM5750A1CLNAHKD%  =  BCM5764MCLNAHKD.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1684&SUBSYS_02D61028

%BCM5764M%          =  BCM5764MX_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_165B

%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_025B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04031025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04051025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04071025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_040A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_040B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04131025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04141025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04151025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04161025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04181025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04191025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_041B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04241025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04251025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_042A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_043F1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04401025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04411025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04491025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_044A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_044D1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04521025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04531025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_05671025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_05681025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_05691025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_056A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_056B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_02FB1028
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04611028
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04A51028
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1690&SUBSYS_E0001458

%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05671025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05681025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_056B1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05781025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05791025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_057A1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_057B1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05801025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05811025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_058B1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_058C1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_06811025

%BCM57765%          =  BCM57765_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16B4

%BCM57766%          =  BCM57766_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1682
%BCM57766%          =  BCM57766_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1682&SUBSYS_62011014
%BCM57766_OEM1%     =  BCM57766_LHinst_EAV.NTamd64.6.0,             PCI\VEN_14e4&DEV_1682&SUBSYS_EA00ECC0
%BCM57766%          =  BCM57766_LHinst_DMAr.NTamd64.6.0,            PCI\VEN_14E4&DEV_1682&SUBSYS_168214E4
%BCM57766%          =  BCM57766_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1682&SUBSYS_124C1734
%BCM57766%          =  BCM57766_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1686

%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1641
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1642
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1643
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1643&SUBSYS_823710F1
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1643&SUBSYS_57251458
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1643&SUBSYS_89A2152D
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1687&SUBSYS_08141028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1687&SUBSYS_093E1028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1687&SUBSYS_093F1028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1687&SUBSYS_09401028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1687&SUBSYS_09411028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1683
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1687
%BCM5762%           =  BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.0,  PCI\VEN_14e4&DEV_1687&SUBSYS_07F01028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1687&SUBSYS_09031028
%BCM5762%           =  BCM5762_LHinst_MRRS.NTamd64.6.0,            PCI\VEN_14e4&DEV_1687&SUBSYS_43B41022
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_2215103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_225E103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_225F103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_805A103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_805B103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_805C103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_807E103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_8084103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_8236103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_8238103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_8265103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_8266103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1687&SUBSYS_835B103C
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16F3
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_16F3&SUBSYS_57271458

%BCM5717%           =  BCM5717_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1655
%BCM5717%           =  BCM5717_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1655&SUBSYS_401317AA
%BCM5717%           =  BCM5717C0_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1665
%BCM5717%           =  BCM5717C0_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1665&SUBSYS_04D01014
%BCM5717%           =  BCM5717C0_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1665&SUBSYS_401117AA
%BCM5717%           =  BCM5718_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1656
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_30451054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_30461054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_30471054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_30521054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_306C1054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_306E1054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_30841054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_01801374
%BCM5717%           =  BCM5718_LHinst_OEM2.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_80071BCF
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_80131BCF
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.0,             PCI\VEN_14e4&DEV_1656&SUBSYS_80631BCF
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_041B1014
%BCM5717%           =  BCM5718S_LHinst_OEM2.NTamd64.6.0,            PCI\VEN_14e4&DEV_1656&SUBSYS_04311014
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_180414E4
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_180514E4
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_280414E4
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_280514E4
%BCM5717%           =  BCM5718S_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1656&SUBSYS_30681054
%BCM5718_OEM1%      =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_4D011186
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_400F17AA
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1656&SUBSYS_401017AA
%BCM5717%           =  BCM5718S_LHinst_OEM2.NTamd64.6.0,            PCI\VEN_14e4&DEV_1656&SUBSYS_401217AA

%BCM5719%           =  BCM5719_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1657
%BCM5719%           =  BCM5719_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1657&SUBSYS_402D17AA
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_30471054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_30551054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_30561054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_30861054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_01801374
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_80141BCF
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_804C1BCF
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_80541BCF
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_80641BCF
%BCM5719%           =  BCM5719C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_190414E4
%BCM5719%           =  BCM5719S_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_190514E4
%BCM5719_BRCM%      =  BCM5719C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_190914E4
%BCM5718S%          =  BCM5719S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_198014E4
%BCM5719C_OEMC%     =  BCM5719C_LHinst_OEMC.NTamd64.6.0,            PCI\VEN_14e4&DEV_1657&SUBSYS_00C01137
%BCM5719S_OEMC%     =  BCM5719S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_00C11137
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_04D11014
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_400E17AA
%BCM5719L%          =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_410417AA
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_202319E5
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_202619E5
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_202719E5
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_1025193d
%BCM5719I%          =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_02D21590
%BCM5719%           =  BCM5719A0_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1657&REV_00
%BCM5719%           =  BCM5719A0C_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1657&SUBSYS_190414E4&REV_00
%BCM5719%           =  BCM5719A0S_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1657&SUBSYS_190514E4&REV_00
%BCM5718S%          =  BCM5719A0S_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1657&SUBSYS_198014E4&REV_00
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1657&SUBSYS_201914E4

%BCM5720%           =  BCM5720_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_165F
%BCM5720%           =  BCM5720_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_165F&SUBSYS_402C17AA
%BCM5720%           =  BCM5720C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165F&SUBSYS_89AA152D
%BCM5720%           =  BCM5720C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165F&SUBSYS_8B16152D
%BCM5720L1%         =  BCM5720C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165F&SUBSYS_410717AA
%BCM5720L2%         =  BCM5720C_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165F&SUBSYS_410617AA
%BCM5720%           =  BCM5720C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_80591BCF
%BCM5720%           =  BCM5720C_LHinst_OEM1.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_80691BCF
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_200314E4
%BCM5720_BRCM%      =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_200914E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_412014E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_416014E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_000A1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_201814E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_001F1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F61028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F71028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F81028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F91028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_04FA1028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_05E51028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_06391028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_063B1028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_06A51028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_06A61028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_06A71028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_1F5B1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_1FEC1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_07F71028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_088E1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_08901028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_08911028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_088F1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_08FD1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_08FF1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_09001028
%BCM5720%           =  BCM5720S_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_04DC1028
%BCM5720%           =  BCM5720S_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_1F541028
%BCM5720L%          =  BCM5720S_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_165F15D9
%BCM5720_SMC%       =  BCM5720S_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_1B2E15D9
%BCM5720_Kura%      =  BCM5720S_LHinst_OEMD.NTamd64.6.0,            PCI\VEN_14e4&DEV_165F&SUBSYS_9130104D
%BCM5718S%          =  BCM5720S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165F&SUBSYS_208014E4

%BCM5755%           =  BCM5755A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167B
%BCM5755%           =  BCM5755A1eStarGX_LHinst.NTamd64.6.0,         PCI\VEN_14e4&DEV_165A
%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167B&SUBSYS_10B21734
%BCM5755%           =  BCM5755A1eStarG_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_165A&SUBSYS_02A61028

%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1675
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1680
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681

%BCM5755%           =  BCM5761_Jumbo.NTamd64.6.0,                   PCI\VEN_14e4&DEV_1680&SUBSYS_300014E4
%BCM5755%           =  BCM5761_Jumbo.NTamd64.6.0,                   PCI\VEN_14e4&DEV_1681&SUBSYS_300014E4
%BCM5755%           =  BCM5761_LHinst_CQ35234.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_06691025
%BCM5755%           =  BCM5761_LHinst_CQ35234.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_066B1025
%BCM5755%           =  BCM5761_LHinst_CQ35234.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_07091025
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_3047103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_1459103C
%BCM5761_OEM1%      =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_1850103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_357E103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_339C103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_84B81043
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_57611019
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_11AB1734
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_1681&SUBSYS_1007174B
%BCM5755%           =  BCM5761_LHinst_CQ47248.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_308217AA

%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_02641028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_02651028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_02621028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_02631028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_02511028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_02DB1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_02EF1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_04281028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_04291028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_04321028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_047B1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1680&SUBSYS_047C1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_02931028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_026D1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_026E1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_02FB1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_04331028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_049A1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_049B1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_04AC1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_04EB1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_04EC1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_053C1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1681&SUBSYS_053D1028

%BCM5755%           =  BCM5761S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1688
%BCM5755%           =  BCM5761S_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1689

%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c
%BCM5754%           =  BCM5754A1HEStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_167A&SUBSYS_3029103c
%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5755%           =  BCM5755A1DRSS_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5755%           =  BCM5755A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_167B&SUBSYS_2817103c
%BCM5755%           =  BCM5755A1EStarAuto_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_167B&SUBSYS_1306103c
%BCM5755%           =  BCM5755A1EStarAuto_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_167B&SUBSYS_1307103c
%BCM5755%           =  BCM5755A1EStarLowest_LHinst.NTamd64.6.0,     PCI\VEN_14e4&DEV_167B&SUBSYS_1308103c
%BCM5755%           =  BCM5755A1EStarAuto_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_167B&SUBSYS_12ff103c

%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167B&SUBSYS_100C17AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167B&SUBSYS_100F17AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167B&SUBSYS_101017AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167B&SUBSYS_101117AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167B&SUBSYS_101317AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167B&SUBSYS_101c17AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.0,        PCI\VEN_14e4&DEV_167B&SUBSYS_866917AA

%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1696
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1696&SUBSYS_12bb103c
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1696&SUBSYS_12bc103c
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1696&SUBSYS_000c103c
%BCM5786%           =  BCM5787A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169A
%BCM5786%           =  BCM5787A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169A&SUBSYS_101517aa
%BCM5786%           =  BCM5787A1F3E_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_169A&SUBSYS_13ee10cf
%BCM5786%           =  BCM5787A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169A&SUBSYS_101f17AA

%BCM5787%           =  BCM5787A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169B
%BCM5787%           =  BCM5787A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169B&SUBSYS_11291734
%BCM5787%           =  BCM5787A1eStar_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_169B&SUBSYS_115C1734
%BCM5787%           =  BCM5787A1HALe_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_169B&SUBSYS_203017AA
%BCM5787%           =  BCM5787A1HALe_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_169B&SUBSYS_100D17AA
%BCM5787%           =  BCM5787A1HALe_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_169B&SUBSYS_100E17AA
%BCM5787%           =  BCM5787A1F3E_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_169B&SUBSYS_139810cf
%BCM5787%           =  BCM5787A1MeStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_1693
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_30c0103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_30E0103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_30E3103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_30DD103c
%BCM5787M%          =  BCM5787A1Me_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_169C&SUBSYS_3030103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0,      PCI\VEN_14e4&DEV_1693&SUBSYS_30c2103c
%BCM5787M%          =  BCM5787A1Me_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1693&SUBSYS_3026103c
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1693&SUBSYS_203017AA
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1693&SUBSYS_20d517AA
%BCM5787MKDMNUN%    =  BCM5787MDisableGig_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_305617AA
%BCM5787MKDMNUN%    =  BCM5787MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1693&SUBSYS_386017AA
%BCM5787MKDMNUN%    =  BCM5787MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1693&SUBSYS_3A2317AA
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1693&SUBSYS_3D7F17AA
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1693&SUBSYS_3A2617AA
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1693&SUBSYS_139910cf

%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88111033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88121033
%bcm5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88361033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88421033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88611033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88621033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88631033
%BCM5787%           =  BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.0,     PCI\VEN_14e4&DEV_1693&SUBSYS_88741033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88831033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.0, PCI\VEN_14e4&DEV_1693&SUBSYS_88921033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A11033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A21033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A51033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A91033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88B01033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.0,       PCI\VEN_14e4&DEV_1693&SUBSYS_88B91033

%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_011A1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_011B1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_011C1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_011D1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_011E1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_011F1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01211025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01221025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01231025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01241025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01251025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01261025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01271025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01281025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01291025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_012A1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_012B1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_012C1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_012D1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_012E1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_012F1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01301025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01311025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01341025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01351025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.0,           PCI\VEN_14e4&DEV_1693&SUBSYS_01361025

%BCM5787F%          =  BCM5750A1FeStar_LHinst.NTamd64.6.0,          PCI\VEN_14e4&DEV_167F
%BCM5787F%          =  BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.0,      PCI\VEN_14e4&DEV_167F&SUBSYS_30c0103C
%BCM5787F%          =  BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.0,      PCI\VEN_14e4&DEV_167F&SUBSYS_30c2103C

%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_169C&SUBSYS_123c10cf
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_169C&SUBSYS_12f710cf
%BCM5788%           =  BCM5788F1N_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_169c&SUBSYS_82fa1033
%BCM5788%           =  BCM5788F1N_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_169c&SUBSYS_83011033
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101717aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101817aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101a17aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101b17aa
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169d
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_169d&SUBSYS_83101033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_169d&SUBSYS_83321033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_169d&SUBSYS_833a1033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_169d&SUBSYS_881b1033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_169d&SUBSYS_881c1033
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169d&SUBSYS_0280107b
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169d&SUBSYS_100317AA
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169d&SUBSYS_100517AA
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169d&SUBSYS_060017FF
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_16DD
%BCM5750B0%         =  BCM5750B0M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FF
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_170D
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_170E
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_170E&SUBSYS_05451014

%BCM5906%           =  BCM5906eStar_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1712
%BCM5906_ID4_FEA%   =  BCM5906Star_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1712&SUBSYS_2816103c
%BCM5906_ID4_FEB%   =  BCM5906Star_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1712&SUBSYS_170f103c


%BCM5906M%          =  BCM5906MeStar_LHinst.NTamd64.6.0,            PCI\VEN_14e4&DEV_1713
%BCM5906MH%         =  BCM5906Mstar_LHinst_CQ39100.NTamd64.6.0,     PCI\VEN_14e4&DEV_1713&SUBSYS_30c0103C
%BCM5906MH%         =  BCM5906Mstar_LHinst_CQ39100.NTamd64.6.0,     PCI\VEN_14e4&DEV_1713&SUBSYS_30c2103C
%BCM5906_ID4_FEA%   =  BCM5906Mstar_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1713&SUBSYS_2816103c
%BCM5906_ID4_FEB%   =  BCM5906Mstar_LHinst.NTamd64.6.0,             PCI\VEN_14e4&DEV_1713&SUBSYS_170f103c
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_386117AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_3D7E17AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_3C2C17AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_400617AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_3A2317AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_3A2A17AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_305617AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_306117AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.0,              PCI\VEN_14e4&DEV_1713&SUBSYS_389B17AA
%BCM5906M%          =  BCM5906F3M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_1713&SUBSYS_143410CF
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1713&SUBSYS_01F31028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1713&SUBSYS_02091028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1713&SUBSYS_02271028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1713&SUBSYS_02861028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1713&SUBSYS_02CA1028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1713&SUBSYS_02B61028

%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028

%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165E&SUBSYS_865d1028
%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165E&SUBSYS_20031028
%OEM1_DEV6%         = OEM1_DEV6_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_1653&SUBSYS_86531028


%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_0a0c103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_3095103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_3098103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_167D&SUBSYS_3099103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_3095103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_3098103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_3099103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_309F103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30ac103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30ad103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30a3103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30a2103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30b1103C
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1600&SUBSYS_3014103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c&REV_00
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169C&SUBSYS_099c103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_308b103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_308e103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3095103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3098103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3099103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_30aa103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_30a1103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_30b0103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.0,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3021103c
%OEM2_DEV1%         =  BCM5705M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165d&SUBSYS_00580E11
%OEM2_DEV1%         =  BCM5705M_LHinst.NTamd64.6.0,                 PCI\VEN_14e4&DEV_165d&SUBSYS_005A0E11
%OEM3_DEV1%         =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165e&SUBSYS_0890103c
%OEM3_DEV1%         =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165e&SUBSYS_0a0c103c
%OEM3_DEV2%         =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165e&SUBSYS_0894103c
%OEM3_DEV3%         =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165e&SUBSYS_088c103c
%OEM3_DEV4%         =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165e&SUBSYS_08bc103c
%OEM3_DEV4%         =  BCM5705MA2_LHinst.NTamd64.6.0,               PCI\VEN_14e4&DEV_165e&SUBSYS_099c103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1600&SUBSYS_3013103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1600&SUBSYS_3015103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_12f2103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.0,                PCI\VEN_14e4&DEV_1677&SUBSYS_3008103c
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,   PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,   PCI\VEN_14e4&DEV_1677&SUBSYS_3002103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,   PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0,   PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c&REV_00


;;------ MSI support ------
[BCM5750_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750X_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1X_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1G_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1HALe_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714G_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5780X_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714S_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714SHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5714SHAL_LHinst.NTamd64_i.6.0.hw]
AddReg = MsiSupportStd

[BCM5714SWol_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1STSP_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5789_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5789F1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5789F1N_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750B0MHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750B0MFHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750B0M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1SPECIAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd


[BCM5754A1MCLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1DRSS_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1Estar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1EstarG_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1EstarGX_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1HALeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1HALe_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1F3E_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1F3M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1F3MNeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787MHALe_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787MDisableGig_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750MHALe_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1MBDFS_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750FHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1CLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1CLDeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F3E_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F3Ne_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F3Me_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1F3MNe_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5901_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5788_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5788F1_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5788F1N_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906MHAL_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906F3M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906Star_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906Mstar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906Mstar_LHinst_CQ39100.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906MD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1EStarAuto_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1EStarLowest_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1MeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1eStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1eStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1MeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5754A1HEStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1MeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5755A1CLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1eStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5787A1MeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906eStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5750A1FeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5906MeStar_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5761_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5761_LHinst_CQ35234.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5761_LHinst_CQ47248.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5761_Jumbo.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5761S_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5764MX_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst_CQ35234.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst_P.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst_P_Lowest.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5764MCLNAHKD.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5761MCLNAHKD_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM57760_LHinst.NTamd64.6.0.hw]
AddReg = MsiSupportStd

[BCM5762_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5762_LHinst_MRRS.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5762RSS4_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM57765_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM57766_LHinst_EAV.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM57766_LHinst_DMAr.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM57766_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5717_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5717C0_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5718_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5718_LHinst_OEM1.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5718_LHinst_OEM2.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5718S_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5718S_LHinst_OEM1.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5718S_LHinst_OEM2.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst_OEMC.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst_OEMD.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst_OEM1.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719S_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719S_LHinst_OEMD.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719A0_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719A0C_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5719A0S_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5720_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5720C_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5720C_LHinst_OEM1.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5720C_LHinst_OEMD.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5720S_LHinst.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

[BCM5720S_LHinst_OEMD.NTamd64.6.0.hw]
AddReg = MsiXSupportStd

;;------ end of MSI support ----

[BCM5703G_LHinst.NTamd64.6.0]
DelReg          = DelReg_Generic, DelReg.ParamsC, DelReg.Jumbo
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5703G_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5704G_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.ParamsC, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOLNS, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704G_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750X_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750X_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1X_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1X_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1G_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWOL, ParamsWireSpeed, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1G_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1eStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1eStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1HALe_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1HALe_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LgSnd, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714G_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LgSnd, DelReg.Wol, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714G_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5780X_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5780X_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5714SWol_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsWOLTbi, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714SWol_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714SHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo , ParamsWOLTbi, ParamsDropVlan, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714SHAL_LHinst.NTamd64_i.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo , ParamsWOLTbi, ParamsDropVlan, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714SHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5714SHAL_LHinst.NTamd64_i.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1STSP_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1STSP_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5789_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5789_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5789F1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5789F1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5789F1N_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5789F1N_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750B0MHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750B0MHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750B0MFHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750B0MFHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog




[BCM5750B0M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750B0M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1SPECIAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xSPECIAL, ParamsCSPECIAL, ParamsWOLeStar, ParamsWireSpeedSPECIAL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1SPECIAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750A1M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1MeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1MeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5754A1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5754A1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5754A1eStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5754A1eStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, ParamsM, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5787MA1CLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog






[BCM5754A1MCLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, ParamsM, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5754A1MCLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, ParamsM, 5755vsta.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5755A1MCLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1CLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, 5755vsta.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5755A1CLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5754A1MeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4


[BCM5754A1MeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1DRSS_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSSDisabled
[BCM5755A1DRSS_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1Estar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1Estar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5754A1HEStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4

[BCM5754A1HEStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1EstarG_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWOLeStar, ParamsWireSpeed, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1EstarG_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1EstarGX_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWOLeStar, ParamsWireSpeed, ParamsTuning, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1EstarGX_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1EstarAuto_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSSDisabled

[BCM5755A1EstarAuto_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1EstarLowest_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSSDisabled

[BCM5755A1EstarLowest_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1MeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS


[BCM5755A1MeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1HALeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS


[BCM5755A1HALeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5761_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS
;AddReg = ParamsIpsecv4
;AddReg = ParamsIpsecv2

[BCM5761_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761_LHinst_CQ35234.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsCQ35234
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5761_LHinst_CQ35234.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761_LHinst_CQ47248.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsCQ47248
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS
;AddReg = ParamsIpsecv4
;AddReg = ParamsIpsecv2

[BCM5761_LHinst_CQ47248.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761_Jumbo.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSndJumboCombo_5761
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5761_Jumbo.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5761S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761S_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS
;AddReg = ParamsIpsecv4
AddReg = ParamsIpsecv2

[BCM5761S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5717_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5717.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5717_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5717C0_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5717C0.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5717C0_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5718_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5717.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718_LHinst_OEM1.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5717_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSizeEnabled
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718_LHinst_OEM1.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718_LHinst_OEM2.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5717_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718_LHinst_OEM2.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5718S.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718S_LHinst_OEM1.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5718S_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718S_LHinst_OEM1.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718S_LHinst_OEM2.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5718S_OEM2.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718S_LHinst_OEM2.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5719_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsRssQueues, ParamsEEE_CO, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst_OEMC.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL_OEMC, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst_OEMC.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst_OEMD.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst_OEMD.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst_OEM1.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5719_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSizeEnabled
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst_OEM1.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719S_LHinst_OEMD.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719S_LHinst_OEMD.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719A0_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsRssQueues, ParamsEEE_CO, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5719A0_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719A0C_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5719A0C_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719A0S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5719A0S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsRssQueues, ParamsEEE_CO, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720C_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720C_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720C_LHinst_OEM1.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5720_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSizeEnabled
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720C_LHinst_OEM1.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720C_LHinst_OEMD.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720C_LHinst_OEMD.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsJumbo, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720S_LHinst_OEMD.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720S_LHinst_OEMD.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5764M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5764M.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5764M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5764MX_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5764MR.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsTuning, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5764MX_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764M_LHinst_CQ35234.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5764M.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsCQ35234
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5764M_LHinst_CQ35234.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764M_LHinst_P.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSSDisabled

[BCM5764M_LHinst_P.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764M_LHinst_P_Lowest.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSSDisabled

[BCM5764M_LHinst_P_Lowest.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764MCLNAHKD.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg,  BCM5764M.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5764vsta.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5764MCLNAHKD.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57760_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57760.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM57760_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5762_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsJumbo, ParamsEEE, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5762_LHinst_MRRS.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsJumbo, ParamsEEE, ParamsRingSize, ParamsMRRS
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762_LHinst_MRRS.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsJumbo, ParamsEEE, ParamsRingSize, ParamsMRRS, ParamsJIRA26220
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5762RSS4_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueuesDef4, ParamsJumbo, ParamsEEE, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762RSS4_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57765_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57765.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsJumbo, ParamsEEE
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS
AddReg = ParamsTbt


[BCM57765_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57766_LHinst_EAV.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57766_EAV.Params, ParamsTuning55,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsRssQueues, ParamsJumbo, ParamsEEE, ParamsEAV
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM57766_LHinst_EAV.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57766_LHinst_DMAr.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57766.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsJumbo, ParamsEEE, ParamsDMAr
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS
AddReg = ParamsTbt

[BCM57766_LHinst_DMAr.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57766_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57766.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsJumbo, ParamsEEE
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS
AddReg = ParamsTbt

[BCM57766_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1eStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1eStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1HALe_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1HALe_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1F3E_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3E_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1F3M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsCQ29902_0
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1F3MNeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3MNeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx

[BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1MeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1MeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1Me_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1Me_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsCQ39100
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1Me_LHinst_CQ39100.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1MBDFS_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1MBDFS_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787MHALe_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787MHALe_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787MDisableGig_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsWOLLink, ParamsDisableGig
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787MDisableGig_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750MHALe_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750MHALe_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1FeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1FeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsCQ39100
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750FHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750FHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1CLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg_CLNAHKD_1, DelReg.Jumbo, DelReg.TaskOffload, DelReg.LAA
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1CLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1CLDeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg_CLNAHKD_1, DelReg.Jumbo, DelReg.Wol, DelReg.TaskOffload, DelReg.LAA
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1CLDeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3E_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3E_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3Ne_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3Ne_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3Me_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3Me_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3MNe_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3MNe_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705M.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705F_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705F.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705F_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705A2_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705A2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705A2_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705MA2_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705MA2_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705MA2F2_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705MA2F2_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705MA2F2N_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705MA2F2N_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5901_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5901.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5901_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5788_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5788_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5788F1_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5788F1_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5788F1N_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5788F1N_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5703S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5703S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5703SW_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5703SW_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5704S_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704S_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5704SW_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704SW_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5704SW_LHinst.NTamd64_d.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi, ParamsDropVlan
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704SW_LHinst.NTamd64_d.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[3C998T_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[3C998T_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[3C998SX_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[3C998SX_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[3C999T_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[3C999T_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[OEM1_DEV4_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, ParamsTuning, OEM1_DEV4.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[OEM1_DEV4_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[OEM1_DEV5_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, ParamsTuning, OEM1_DEV5.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[OEM1_DEV5_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[OEM1_DEV6_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, ParamsTuning, OEM1_DEV6.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[OEM1_DEV6_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906eStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906eStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906MeStar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906MeStar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906MD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol, DelReg.LAA, DelReg.TaskOffload, DelReg_CLNAHKD
AddReg          = LH_AddReg, BCM5788.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, 5906Mvsta.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906MD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5906MHAL_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906MHAL_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5906F3M_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LsoV1IPv4
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906F3M_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906Mstar_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906Mstar_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906Mstar_LHinst_CQ39100.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM, ParamsCQ39100
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906Mstar_LHinst_CQ39100.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906Star_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906Star_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761MCLNAHKD_LHinst.NTamd64.6.0]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5761_chip.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5761vsta.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5761MCLNAHKD_LHinst.NTamd64.6.0.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


;*******************************************************************************
; Windows 7 install sections.
;*******************************************************************************
[Broadcom.NTamd64.6.1]
%3C998SX%           =  3C998SX_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C998T%            =  3C998T_LHinst.NTamd64.6.1,                   PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C999T%            =  3C999T_LHinst.NTamd64.6.1,                   PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%BCM5703%           =  BCM5703G_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1647
%BCM5703%           =  BCM5703G_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16a7
%BCM5703%           =  BCM5703G_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16C7
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703SW%         =  BCM5703SW_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704%           =  BCM5704G_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1648
%BCM5704S%          =  BCM5704S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16A8
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.1,              PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.1,              PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.1,              PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64_d.6.1,              PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5704SW%         =  BCM5704SW_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_16A8&SUBSYS_03331014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1654
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014
%BCM5705%           =  BCM5705_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1653
%BCM5705F%          =  BCM5705F_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_166e
%BCM5705F%          =  BCM5705F_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%BCM5705FHA%        =  BCM5705F_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705FHB%        =  BCM5705F_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5705M%          =  BCM5705MA2F2N_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%          =  BCM5705MA2F2N_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%          =  BCM5705MA2F2_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_165E&SUBSYS_127910cf
%BCM5705M%          =  BCM5705MA2F2N_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165E
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5705M%          =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165E&SUBSYS_0727152d
%BCM5705M%          =  BCM5705M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165D
%BCM5714%           =  BCM5714G_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1668
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_166A&SUBSYS_03131014
%BCM5714%           =  BCM5780X_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_166A
%BCM5714%           =  BCM5780X_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_166A&SUBSYS_107F1734
%BCM5714%           =  BCM5714G_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1678
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1678&SUBSYS_032a1014
%BCM5714%           =  BCM5714_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1678&SUBSYS_108C1734
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1669
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1669&SUBSYS_03281014
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1679&SUBSYS_03671014
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64_i.6.1,            PCI\VEN_14e4&DEV_1669&SUBSYS_03861014
%BCM5714SW%         =  BCM5714SHAL_LHinst.NTamd64_i.6.1,            PCI\VEN_14e4&DEV_1669&SUBSYS_03871014
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_166B
%BCM5714S%          =  BCM5714S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1679
%BCM5714S%          =  BCM5714SWol_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1679&SUBSYS_399710f1

%BCM5750A1%         =  BCM5750A1F3Me_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%         =  BCM5750A1F3Me_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1%         =  BCM5750A1F3MNe_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%         =  BCM5750A1F3MNe_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167D&SUBSYS_832a1033
%BCM5750A1%         =  BCM5750A1F3E_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5750A1%         =  BCM5750A1F3Ne_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%         =  BCM5750A1F3Ne_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033
%BCM5750A1%         =  BCM5750A1MeStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1601
%BCM5750A1%         =  BCM5750A1MeStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_167D
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD
%BCM5750A1%         =  BCM5750A1SPECIAL_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_81AA104D
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_108B1734
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_5047107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_5048107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_0280107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_0215107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_0460107b
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_0604107b
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1600&SUBSYS_03301014
%BCM5750A1%         =  BCM5750A1HALe_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_1601&SUBSYS_202017AA
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1658
%BCM5750A1%         =  BCM5750A1G_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1659
%BCM5750A1%         =  BCM5750A1X_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014
%BCM5750A1%         =  BCM5750A1X_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1659&SUBSYS_02C61014
%BCM5750A1%         =  BCM5750A1X_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1676
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1677
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1677&SUBSYS_00631025
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1677&SUBSYS_10961734
%BCM5750A1%         =  BCM5750A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_167C
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_16F7
%BCM5750A1%         =  BCM5750MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_167D&SUBSYS_05771014
%BCM5750A1%         =  BCM5750MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_167D&SUBSYS_208117AA
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%      =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01791028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1600&SUBSYS_01A71028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1600&SUBSYS_01A81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1600&SUBSYS_01AD1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C11028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01CF1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01C21028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01CC1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01D61028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_01CE1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1600&SUBSYS_02011028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_019c1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_01E01028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_1677&SUBSYS_02071028
%BCM5750A1CLNAHKD%  =  BCM5750A1CLDeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_16F7&SUBSYS_01BF1028

%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_01da1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_024E1028
%BCM5750A1CLNAHKD%  =  BCM5755A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167B&SUBSYS_01da1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_01de1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_01e11028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_01ec1028

%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167E
%BCM5750A1F%        =  BCM5750A1F_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167E&SUBSYS_01E41028
%BCM5750A1F%        =  BCM5750FHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014
%BCM5750A1STSP%     =  BCM5750A1STSP_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_1659&SUBSYS_3260103c
%BCM5750B0%         =  BCM5750B0MHAL_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_10
%BCM5750B0F%        =  BCM5750B0MFHAL_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_10
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%           =  BCM5750X_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01

%BCM5754%           =  BCM5754A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167A
%BCM5754%           =  BCM5754A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_167A&SUBSYS_01fe1734
%BCM5754%           =  BCM5754A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167A&SUBSYS_10fe1734
%BCM5754%           =  BCM5754A1MeStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1672
%BCM5750A1CLNAHKD%  =  BCM5754A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1672&SUBSYS_01f71028
%BCM5750A1CLNAHKD%  =  BCM5754A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1672&SUBSYS_02021028

%BCM5755%           =  BCM5755A1MeStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1673
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1673&SUBSYS_01fa1028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1673&SUBSYS_01f91028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1673&SUBSYS_02061028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1673&SUBSYS_01fe1028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1673&SUBSYS_02001028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1673&SUBSYS_024A1028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1673&SUBSYS_01ff1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_169B&SUBSYS_02201028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_021D1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_021E1028
%BCM5750A1CLNAHKD%  =  BCM5754A1CLNAHKD_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_167A&SUBSYS_02141028

%BCM5750A1%         =  BCM5755A1MeStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1674
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1674&SUBSYS_01f81028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1674&SUBSYS_02041028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1674&SUBSYS_02641028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1674&SUBSYS_02651028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1674&SUBSYS_02621028
%BCM5750A1CLNAHKD%  =  BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1674&SUBSYS_02631028

%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1693&SUBSYS_02541028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1693&SUBSYS_02551028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1693&SUBSYS_02561028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1693&SUBSYS_02571028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1693&SUBSYS_025A1028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1693&SUBSYS_025B1028
%BCM5787M%          =  BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_1693&SUBSYS_02CA1028

%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01391025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_013B1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_013C1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_013D1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01421025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01431025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01451025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01471025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01481025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_01491025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_014A1025
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_014B1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_01601025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_01611025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_019C1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_019D1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_019E1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_019F1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02001025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02011025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02021025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02031025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02041025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02051025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02061025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02071025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02081025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02091025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_020A1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_020B1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_020C1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_020D1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_020E1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_020F1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02101025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02111025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02121025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02131025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02141025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02151025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02161025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02191025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_021A1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_021B1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_021C1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_021D1025
%BCM5764M%          =  BCM5764M_LHinst_CQ35234.NTamd64.6.1,         PCI\VEN_14e4&DEV_1684&SUBSYS_02211025

%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_0173107B
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_0174107B

%BCM5764M%          =  BCM5764M_LHinst_P_Lowest.NTamd64.6.1,        PCI\VEN_14e4&DEV_1684&SUBSYS_1309103C
%BCM5764M%          =  BCM5764M_LHinst_P_Lowest.NTamd64.6.1,        PCI\VEN_14e4&DEV_1684&SUBSYS_130A103C
%BCM5764M%          =  BCM5764M_LHinst_P_Lowest.NTamd64.6.1,        PCI\VEN_14e4&DEV_1684&SUBSYS_130B103C
%BCM5764M%          =  BCM5764M_LHinst_P.NTamd64.6.1,               PCI\VEN_14e4&DEV_1684&SUBSYS_1503103C
%BCM5764M%          =  BCM5764M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_2821103C

%BCM5750A1CLNAHKD%  =  BCM5764MCLNAHKD.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_02811028
%BCM5750A1CLNAHKD%  =  BCM5764MCLNAHKD.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_02C31028
%BCM5750A1CLNAHKD%  =  BCM5764MCLNAHKD.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1684&SUBSYS_02D61028

%BCM5764M%          =  BCM5764MX_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_165B

%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_025B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04031025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04051025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04071025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_040A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_040B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04131025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04141025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04151025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04161025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04181025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04191025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_041B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04241025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04251025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_042A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_043F1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04401025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04411025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04491025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_044A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_044D1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04521025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04531025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_05671025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_05681025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_05691025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_056A1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_056B1025
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_02FB1028
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04611028
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_04A51028
%BCM57760%          =  BCM57760_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1690&SUBSYS_E0001458

%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05671025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05681025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_056B1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05781025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05791025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_057A1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_057B1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05801025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_05811025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_058B1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_058C1025
%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B0&SUBSYS_06811025

%BCM57765%          =  BCM57765_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16B4

%BCM57766%          =  BCM57766_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1682
%BCM57766%          =  BCM57766_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1682&SUBSYS_62011014
%BCM57766_OEM1%     =  BCM57766_LHinst_EAV.NTamd64.6.1,             PCI\VEN_14e4&DEV_1682&SUBSYS_EA00ECC0
%BCM57766%          =  BCM57766_LHinst_DMAr.NTamd64.6.1,            PCI\VEN_14E4&DEV_1682&SUBSYS_168214E4
%BCM57766%          =  BCM57766_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1682&SUBSYS_124C1734
%BCM57766%          =  BCM57766_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1686

%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1641
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1642
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1643
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1643&SUBSYS_823710F1
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1643&SUBSYS_57251458
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1643&SUBSYS_89A2152D
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1687&SUBSYS_08141028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1687&SUBSYS_093E1028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1687&SUBSYS_093F1028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1687&SUBSYS_09401028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1687&SUBSYS_09411028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1683
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1687
%BCM5762%           =  BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.1,  PCI\VEN_14e4&DEV_1687&SUBSYS_07F01028
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1687&SUBSYS_09031028
%BCM5762%           =  BCM5762_LHinst_MRRS.NTamd64.6.1,            PCI\VEN_14e4&DEV_1687&SUBSYS_43B41022
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_2215103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_225E103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_225F103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_805A103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_805B103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_805C103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_807E103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_8084103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_8236103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_8238103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_8265103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_8266103C
%BCM5761_OEM1%      =  BCM5762RSS4_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1687&SUBSYS_835B103C
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16F3
%BCM5762%           =  BCM5762_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_16F3&SUBSYS_57271458

%BCM5717%           =  BCM5717_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1655
%BCM5717%           =  BCM5717_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1655&SUBSYS_401317AA
%BCM5717%           =  BCM5717C0_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1665
%BCM5717%           =  BCM5717C0_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1665&SUBSYS_04D01014
%BCM5717%           =  BCM5717C0_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1665&SUBSYS_401117AA
%BCM5717%           =  BCM5718_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1656
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_30451054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_30461054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_30471054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_30521054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_306C1054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_306E1054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_30841054
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_01801374
%BCM5717%           =  BCM5718_LHinst_OEM2.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_80071BCF
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_80131BCF
%BCM5717%           =  BCM5718_LHinst_OEM1.NTamd64.6.1,             PCI\VEN_14e4&DEV_1656&SUBSYS_80631BCF
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_041B1014
%BCM5717%           =  BCM5718S_LHinst_OEM2.NTamd64.6.1,            PCI\VEN_14e4&DEV_1656&SUBSYS_04311014
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_180414E4
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_180514E4
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_280414E4
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_280514E4
%BCM5717%           =  BCM5718S_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1656&SUBSYS_30681054
%BCM5718_OEM1%      =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_4D011186
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_400F17AA
%BCM5717%           =  BCM5718S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1656&SUBSYS_401017AA
%BCM5717%           =  BCM5718S_LHinst_OEM2.NTamd64.6.1,            PCI\VEN_14e4&DEV_1656&SUBSYS_401217AA

%BCM5719%           =  BCM5719_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1657
%BCM5719%           =  BCM5719_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1657&SUBSYS_402D17AA
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_30471054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_30551054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_30561054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_30861054
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_01801374
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_80141BCF
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_804C1BCF
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_80541BCF
%BCM5719%           =  BCM5719C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_80641BCF
%BCM5719%           =  BCM5719C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_190414E4
%BCM5719%           =  BCM5719S_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_190514E4
%BCM5719_BRCM%      =  BCM5719C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_190914E4
%BCM5718S%          =  BCM5719S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_198014E4
%BCM5719C_OEMC%     =  BCM5719C_LHinst_OEMC.NTamd64.6.1,            PCI\VEN_14e4&DEV_1657&SUBSYS_00C01137
%BCM5719S_OEMC%     =  BCM5719S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_00C11137
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_04D11014
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_400E17AA
%BCM5719L%          =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_410417AA
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_202319E5
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_202619E5
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_202719E5
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_1025193d
%BCM5719I%          =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_02D21590
%BCM5719%           =  BCM5719A0_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1657&REV_00
%BCM5719%           =  BCM5719A0C_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1657&SUBSYS_190414E4&REV_00
%BCM5719%           =  BCM5719A0S_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1657&SUBSYS_190514E4&REV_00
%BCM5718S%          =  BCM5719A0S_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1657&SUBSYS_198014E4&REV_00
%BCM5719%           =  BCM5719C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1657&SUBSYS_201914E4

%BCM5720%           =  BCM5720_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_165F
%BCM5720%           =  BCM5720_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_165F&SUBSYS_402C17AA
%BCM5720%           =  BCM5720C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165F&SUBSYS_89AA152D
%BCM5720%           =  BCM5720C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165F&SUBSYS_8B16152D
%BCM5720%           =  BCM5720C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165F&SUBSYS_8B2F152D
%BCM5720L1%         =  BCM5720C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165F&SUBSYS_410717AA
%BCM5720L2%         =  BCM5720C_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165F&SUBSYS_410617AA
%BCM5720%           =  BCM5720C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_80591BCF
%BCM5720%           =  BCM5720C_LHinst_OEM1.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_80691BCF
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_200314E4
%BCM5720_BRCM%      =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_200914E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_412014E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_416014E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_000A1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_201814E4
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_001F1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F61028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F71028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F81028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_04F91028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_04FA1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_08911028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_088F1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_08FD1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_08FF1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_09001028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_05E51028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_06391028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_063B1028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_06A51028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_06A61028
%BCM5755%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_06A71028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_1F5B1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_1FEC1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_07F71028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_088E1028
%BCM5720%           =  BCM5720C_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_08901028
%BCM5720%           =  BCM5720S_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_04DC1028
%BCM5720%           =  BCM5720S_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_1F541028
%BCM5720L%          =  BCM5720S_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_165F15D9
%BCM5720_SMC%       =  BCM5720S_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_1B2E15D9
%BCM5720_Kura%      =  BCM5720S_LHinst_OEMD.NTamd64.6.1,            PCI\VEN_14e4&DEV_165F&SUBSYS_9130104D
%BCM5718S%          =  BCM5720S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165F&SUBSYS_208014E4

%BCM5755%           =  BCM5755A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167B
%BCM5755%           =  BCM5755A1eStarGX_LHinst.NTamd64.6.1,         PCI\VEN_14e4&DEV_165A
%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167B&SUBSYS_10B21734
%BCM5755%           =  BCM5755A1eStarG_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_165A&SUBSYS_02A61028

%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1675
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1680
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681

%BCM5755%           =  BCM5761_Jumbo.NTamd64.6.1,                   PCI\VEN_14e4&DEV_1680&SUBSYS_300014E4
%BCM5755%           =  BCM5761_Jumbo.NTamd64.6.1,                   PCI\VEN_14e4&DEV_1681&SUBSYS_300014E4
%BCM5755%           =  BCM5761_LHinst_CQ35234.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_06691025
%BCM5755%           =  BCM5761_LHinst_CQ35234.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_066B1025
%BCM5755%           =  BCM5761_LHinst_CQ35234.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_07091025
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_3047103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_1459103C
%BCM5761_OEM1%      =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_1850103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_357E103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_339C103C
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_84B81043
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_57611019
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_11AB1734
%BCM5755%           =  BCM5761_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_1681&SUBSYS_1007174B
%BCM5755%           =  BCM5761_LHinst_CQ47248.NTamd64.6.1,         PCI\VEN_14e4&DEV_1681&SUBSYS_308217AA

%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_02641028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_02651028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_02621028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_02631028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_02511028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_02DB1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_02EF1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_04281028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_04291028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_04321028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_047B1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1680&SUBSYS_047C1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_02931028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_026D1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_026E1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_02FB1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_04331028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_049A1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_049B1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_04AC1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_04EB1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_04EC1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_053C1028
%BCM5750A1CLNAHKD%  =  BCM5761MCLNAHKD_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1681&SUBSYS_053D1028

%BCM5755%           =  BCM5761S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1688
%BCM5755%           =  BCM5761S_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1689

%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c
%BCM5754%           =  BCM5754A1HEStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_167A&SUBSYS_3029103c
%BCM5755%           =  BCM5755A1EStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5755%           =  BCM5755A1DRSS_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5755%           =  BCM5755A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_167B&SUBSYS_2817103c
%BCM5755%           =  BCM5755A1EStarAuto_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_167B&SUBSYS_1306103c
%BCM5755%           =  BCM5755A1EStarAuto_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_167B&SUBSYS_1307103c
%BCM5755%           =  BCM5755A1EStarLowest_LHinst.NTamd64.6.1,     PCI\VEN_14e4&DEV_167B&SUBSYS_1308103c
%BCM5755%           =  BCM5755A1EStarAuto_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_167B&SUBSYS_12ff103c

%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_167B&SUBSYS_100C17AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_167B&SUBSYS_100F17AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_167B&SUBSYS_101017AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_167B&SUBSYS_101117AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_167B&SUBSYS_101317AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_167B&SUBSYS_101c17AA
%BCM5755%           =  BCM5755A1HALeStar_LHinst.NTamd64.6.1,        PCI\VEN_14e4&DEV_167B&SUBSYS_866917AA

%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1696
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1696&SUBSYS_12bb103c
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1696&SUBSYS_12bc103c
%BCM5782%           =  BCM5705A2_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1696&SUBSYS_000c103c
%BCM5786%           =  BCM5787A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_169A
%BCM5786%           =  BCM5787A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_169A&SUBSYS_101517aa
%BCM5786%           =  BCM5787A1F3E_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_169A&SUBSYS_13ee10cf
%BCM5786%           =  BCM5787A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_169A&SUBSYS_101f17AA

%BCM5787%           =  BCM5787A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_169B
%BCM5787%           =  BCM5787A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_169B&SUBSYS_11291734
%BCM5787%           =  BCM5787A1eStar_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_169B&SUBSYS_115C1734
%BCM5787%           =  BCM5787A1HALe_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_169B&SUBSYS_203017AA
%BCM5787%           =  BCM5787A1HALe_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_169B&SUBSYS_100D17AA
%BCM5787%           =  BCM5787A1HALe_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_169B&SUBSYS_100E17AA
%BCM5787%           =  BCM5787A1F3E_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_169B&SUBSYS_139810cf
%BCM5787%           =  BCM5787A1MeStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_1693
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1,      PCI\VEN_14e4&DEV_1693&SUBSYS_30c0103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1,      PCI\VEN_14e4&DEV_1693&SUBSYS_30E0103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1,      PCI\VEN_14e4&DEV_1693&SUBSYS_30E3103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1,      PCI\VEN_14e4&DEV_1693&SUBSYS_30DD103c
%BCM5787M%          =  BCM5787A1Me_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_169C&SUBSYS_3030103c
%BCM5787M%          =  BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1,      PCI\VEN_14e4&DEV_1693&SUBSYS_30c2103c
%BCM5787M%          =  BCM5787A1Me_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1693&SUBSYS_3026103c
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1693&SUBSYS_203017AA
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1693&SUBSYS_20d517AA
%BCM5787MKDMNUN%    =  BCM5787MDisableGig_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_305617AA
%BCM5787MKDMNUN%    =  BCM5787MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1693&SUBSYS_386017AA
%BCM5787MKDMNUN%    =  BCM5787MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1693&SUBSYS_3A2317AA
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1693&SUBSYS_3D7F17AA
%BCM5787%           =  BCM5787MHALe_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1693&SUBSYS_3A2617AA
%BCM5787%           =  BCM5787A1F3M_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1693&SUBSYS_139910cf

%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88111033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88121033
%bcm5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88361033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88421033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88611033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88621033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88631033
%BCM5787%           =  BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.1,     PCI\VEN_14e4&DEV_1693&SUBSYS_88741033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88831033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.1, PCI\VEN_14e4&DEV_1693&SUBSYS_88921033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A11033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A21033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A51033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88A91033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88B01033
%BCM5787%           =  BCM5787A1F3MNeStar_LHinst.NTamd64.6.1,       PCI\VEN_14e4&DEV_1693&SUBSYS_88B91033

%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_011A1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_011B1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_011C1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_011D1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_011E1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_011F1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01211025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01221025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01231025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01241025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01251025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01261025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01271025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01281025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01291025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_012A1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_012B1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_012C1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_012D1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_012E1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_012F1025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01301025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01311025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01341025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01351025
%BCM5787%           =  BCM5787A1MBDFS_LHinst.NTamd64.6.1,           PCI\VEN_14e4&DEV_1693&SUBSYS_01361025

%BCM5787F%          =  BCM5750A1FeStar_LHinst.NTamd64.6.1,          PCI\VEN_14e4&DEV_167F
%BCM5787F%          =  BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.1,      PCI\VEN_14e4&DEV_167F&SUBSYS_30c0103C
%BCM5787F%          =  BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.1,      PCI\VEN_14e4&DEV_167F&SUBSYS_30c2103C

%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_169C&SUBSYS_123c10cf
%BCM5788%           =  BCM5788F1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_169C&SUBSYS_12f710cf
%BCM5788%           =  BCM5788F1N_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_169c&SUBSYS_82fa1033
%BCM5788%           =  BCM5788F1N_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_169c&SUBSYS_83011033
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101717aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101817aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101a17aa
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_101b17aa
%BCM5789%           =  BCM5789F1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169d
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_169d&SUBSYS_83101033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_169d&SUBSYS_83321033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_169d&SUBSYS_833a1033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_169d&SUBSYS_881b1033
%BCM5789%           =  BCM5789F1N_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_169d&SUBSYS_881c1033
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169d&SUBSYS_0280107b
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169d&SUBSYS_100317AA
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169d&SUBSYS_100517AA
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169d&SUBSYS_060017FF
%BCM5789%           =  BCM5789_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_16DD
%BCM5750B0%         =  BCM5750B0M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FF
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_170D
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_170E
%BCM5901%           =  BCM5901_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_170E&SUBSYS_05451014

%BCM5906%           =  BCM5906eStar_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1712
%BCM5906_ID4_FEA%   =  BCM5906Star_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1712&SUBSYS_2816103c
%BCM5906_ID4_FEB%   =  BCM5906Star_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1712&SUBSYS_170f103c


%BCM5906M%          =  BCM5906MeStar_LHinst.NTamd64.6.1,            PCI\VEN_14e4&DEV_1713
%BCM5906MH%         =  BCM5906Mstar_LHinst_CQ39100.NTamd64.6.1,     PCI\VEN_14e4&DEV_1713&SUBSYS_30c0103C
%BCM5906MH%         =  BCM5906Mstar_LHinst_CQ39100.NTamd64.6.1,     PCI\VEN_14e4&DEV_1713&SUBSYS_30c2103C
%BCM5906_ID4_FEA%   =  BCM5906Mstar_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1713&SUBSYS_2816103c
%BCM5906_ID4_FEB%   =  BCM5906Mstar_LHinst.NTamd64.6.1,             PCI\VEN_14e4&DEV_1713&SUBSYS_170f103c
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_386117AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_3D7E17AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_3C2C17AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_400617AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_3A2317AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_3A2A17AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_305617AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_306117AA
%BCM5906M%          =  BCM5906MHAL_LHinst.NTamd64.6.1,              PCI\VEN_14e4&DEV_1713&SUBSYS_389B17AA
%BCM5906M%          =  BCM5906F3M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_1713&SUBSYS_143410CF
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1713&SUBSYS_01F31028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1713&SUBSYS_02091028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1713&SUBSYS_02271028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1713&SUBSYS_02861028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1713&SUBSYS_02CA1028
%BCM5906M%          =  BCM5906MD_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1713&SUBSYS_02B61028

%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV4%         = OEM1_DEV4_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028

%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165E&SUBSYS_865d1028
%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV5%         = OEM1_DEV5_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165E&SUBSYS_20031028
%OEM1_DEV6%         = OEM1_DEV6_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_1653&SUBSYS_86531028


%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c&REV_00
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_0a0c103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_3095103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_3098103C
%BCM5750A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_167D&SUBSYS_3099103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_3095103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_3098103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_3099103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_309F103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30ac103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30ad103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30a3103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30a2103C
%BCM5751A1%         =  BCM5750A1M_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_16FD&SUBSYS_30b1103C
%BCM5750A1%         =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1600&SUBSYS_3014103c
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c&REV_00
%BCM5750%           =  BCM5750_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c&REV_00
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169C&SUBSYS_099c103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_308b103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_308e103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3095103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3098103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3099103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_30aa103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_30a1103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_30b0103c
%BCM5788%           =  BCM5788_LHinst.NTamd64.6.1,                  PCI\VEN_14e4&DEV_169c&SUBSYS_3021103c
%OEM2_DEV1%         =  BCM5705M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165d&SUBSYS_00580E11
%OEM2_DEV1%         =  BCM5705M_LHinst.NTamd64.6.1,                 PCI\VEN_14e4&DEV_165d&SUBSYS_005A0E11
%OEM3_DEV1%         =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165e&SUBSYS_0890103c
%OEM3_DEV1%         =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165e&SUBSYS_0a0c103c
%OEM3_DEV2%         =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165e&SUBSYS_0894103c
%OEM3_DEV3%         =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165e&SUBSYS_088c103c
%OEM3_DEV4%         =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165e&SUBSYS_08bc103c
%OEM3_DEV4%         =  BCM5705MA2_LHinst.NTamd64.6.1,               PCI\VEN_14e4&DEV_165e&SUBSYS_099c103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1600&SUBSYS_3013103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1600&SUBSYS_3015103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_12f2103c
%OEM3_DEV6A1%       =  BCM5750A1_LHinst.NTamd64.6.1,                PCI\VEN_14e4&DEV_1677&SUBSYS_3008103c
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.1,   PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.1,   PCI\VEN_14e4&DEV_1677&SUBSYS_3002103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.1,   PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c&REV_00
%OEM3_DEV6%         =  BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.1,   PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c&REV_00


;;------ MSI support ------
[BCM5750_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750X_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1X_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1G_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1HALe_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5714_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5714G_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5780X_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5714S_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5714SHAL_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5714SHAL_LHinst.NTamd64_i.6.1.hw]
AddReg = MsiSupportStd

[BCM5714SWol_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1STSP_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5789_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5789F1_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5789F1N_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750B0MHAL_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750B0MFHAL_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750B0M_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1SPECIAL_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1M_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5754A1_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd


[BCM5754A1MCLNAHKD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1DRSS_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1Estar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1EstarG_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1EstarGX_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1HALeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1HALe_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1F3E_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1F3M_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1F3MNeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1Me_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787MHALe_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787MDisableGig_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750MHALe_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1MBDFS_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1F_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750FHAL_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1CLNAHKD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1CLDeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1F3E_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1F3Ne_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1F3Me_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1F3MNe_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5901_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5788_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5788F1_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5788F1N_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906MHAL_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906F3M_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906Star_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906Mstar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906Mstar_LHinst_CQ39100.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906MD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1EStarAuto_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1EStarLowest_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1MeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1eStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5754A1eStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5754A1MeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5754A1HEStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1MeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5755A1CLNAHKD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1eStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5787A1MeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906eStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5750A1FeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5906MeStar_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5761_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5761_LHinst_CQ35234.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5761_LHinst_CQ47248.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5761_Jumbo.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5761S_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5764MX_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst_CQ35234.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst_P.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5764M_LHinst_P_Lowest.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5764MCLNAHKD.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM5761MCLNAHKD_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM57760_LHinst.NTamd64.6.1.hw]
AddReg = MsiSupportStd

[BCM57765_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM57766_LHinst_EAV.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM57766_LHinst_DMAr.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM57766_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5762_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5762_LHinst_MRRS.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5762RSS4_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5717_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5717C0_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5718_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5718_LHinst_OEM1.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5718_LHinst_OEM2.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5718S_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5718S_LHinst_OEM1.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5718S_LHinst_OEM2.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst_OEMC.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst_OEMD.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719C_LHinst_OEM1.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719S_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719S_LHinst_OEMD.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719A0_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719A0C_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5719A0S_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5720_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5720C_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5720C_LHinst_OEM1.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5720C_LHinst_OEMD.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5720S_LHinst.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

[BCM5720S_LHinst_OEMD.NTamd64.6.1.hw]
AddReg = MsiXSupportStd

;;------ end of MSI support ----

[BCM5703G_LHinst.NTamd64.6.1]
DelReg          = DelReg_Generic, DelReg.ParamsC, DelReg.Jumbo
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5703G_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5704G_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.ParamsC, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOLNS, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704G_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750X_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed, ParamsTuning, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750X_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1X_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsTuning, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1X_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1G_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWOL, ParamsWireSpeed, ParamsTuning, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1G_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1eStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1eStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5751A0_No_WireSpeed_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1HALe_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1HALe_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LgSnd, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL, ParamsTuning, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714G_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LgSnd, DelReg.Wol, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL, ParamsTuning, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714G_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5780X_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5780X_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5714SWol_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsWOLTbi, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714SWol_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5714SHAL_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo , ParamsWOLTbi, ParamsDropVlan, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714SHAL_LHinst.NTamd64_i.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo , ParamsWOLTbi, ParamsDropVlan, ParamsTuning
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5714SHAL_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5714SHAL_LHinst.NTamd64_i.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1STSP_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsTuning, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1STSP_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5789_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5789_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5789F1_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5789F1_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5789F1N_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo , DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5789F1N_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750B0MHAL_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750B0MHAL_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750B0MFHAL_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750B0MFHAL_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog




[BCM5750B0M_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750B0M_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1SPECIAL_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xSPECIAL, ParamsCSPECIAL, ParamsWOLeStar, ParamsWireSpeedSPECIAL, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1SPECIAL_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5750A1M_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1M_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1MeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1MeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5754A1_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5754A1_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5754A1eStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5754A1eStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5754A1CLNAHKD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, ParamsM, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5787MA1CLNAHKD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog






[BCM5754A1MCLNAHKD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, ParamsM, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5754A1MCLNAHKD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, ParamsM, 5755vsta.Params, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5755A1MCLNAHKD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1CLNAHKD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5754vsta.Params, 5755vsta.Params, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5755A1CLNAHKD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5754A1MeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4


[BCM5754A1MeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1DRSS_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSSDisabled
[BCM5755A1DRSS_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1Estar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1Estar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5754A1HEStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4

[BCM5754A1HEStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1EstarG_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWOLeStar, ParamsWireSpeed, ParamsTuning, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1EstarG_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1EstarGX_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsC
AddReg          = LH_AddReg, Intr_coal, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC1G, ParamsWOLeStar, ParamsWireSpeed, ParamsTuning, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5755A1EstarGX_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1EstarAuto_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSSDisabled

[BCM5755A1EstarAuto_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5755A1EstarLowest_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSSDisabled

[BCM5755A1EstarLowest_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1MeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS


[BCM5755A1MeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5755A1HALeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS


[BCM5755A1HALeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5761_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS
;AddReg = ParamsIpsecv4
;AddReg = ParamsIpsecv2

[BCM5761_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761_LHinst_CQ35234.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsCQ35234
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS

[BCM5761_LHinst_CQ35234.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761_LHinst_CQ47248.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsCQ47248
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS
;AddReg = ParamsIpsecv4
;AddReg = ParamsIpsecv2

[BCM5761_LHinst_CQ47248.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761_Jumbo.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSndJumboCombo_5761, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5761_Jumbo.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5761S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsIpsecv4, DelReg.ParamsIpsecv2
AddReg          = LH_AddReg, Intr_coal, BCM5761S_chip.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv6, ParamsGSOv4
AddReg = ParamsRSS
;AddReg = ParamsIpsecv4
AddReg = ParamsIpsecv2

[BCM5761S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5717_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5717.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5717_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5717C0_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5717C0.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5717C0_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5718_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5717.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718_LHinst_OEM1.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5717_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSizeEnabled
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718_LHinst_OEM1.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718_LHinst_OEM2.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5717_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718_LHinst_OEM2.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5718S.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718S_LHinst_OEM1.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5718S_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718S_LHinst_OEM1.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5718S_LHinst_OEM2.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5718S_OEM2.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5718S_LHinst_OEM2.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5719_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsRssQueues, ParamsEEE_CO, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst_OEMC.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL_OEMC, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst_OEMC.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst_OEMD.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst_OEMD.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719C_LHinst_OEM1.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5719_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSizeEnabled
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719C_LHinst_OEM1.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719S_LHinst_OEMD.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5719S_LHinst_OEMD.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719A0_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsRssQueues, ParamsEEE_CO, ParamsTuning
AddReg          = ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5719A0_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719A0C_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5719A0C_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5719A0S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5719.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsRSS

[BCM5719A0S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsRssQueues, ParamsEEE_CO, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720C_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsVAUX1G
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720C_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720C_LHinst_OEM1.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.ParamsTuning
AddReg          = LH_AddReg, Intr_coal, BCM5720_OEM1.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSizeEnabled
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720C_LHinst_OEM1.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720C_LHinst_OEMD.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsEEE, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720C_LHinst_OEMD.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5720S_LHinst_OEMD.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5720.Params, ParamsTuning25,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsRssQueues, ParamsWOLTbi_None, ParamsTuning, ParamsRssBaseProcNumber
AddReg          = ParamsJumbo, ParamsVmq, ParamsPM, ParamsRingSize, bcmPnpInstallReg
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
Port1FunctionNumber = 0
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5720S_LHinst_OEMD.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5764M_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5764M.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5764M_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5764MX_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5764MR.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsTuning, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5764MX_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764M_LHinst_CQ35234.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5764M.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsCQ35234, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5764M_LHinst_CQ35234.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764M_LHinst_P.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSSDisabled

[BCM5764M_LHinst_P.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764M_LHinst_P_Lowest.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.ParamsRSS
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSSDisabled

[BCM5764M_LHinst_P_Lowest.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5764MCLNAHKD.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg,  BCM5764M.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5764vsta.Params, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5764MCLNAHKD.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57760_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57760.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM57760_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM57765_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57765.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsJumbo, ParamsEEE
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS
AddReg = ParamsTbt

[BCM57765_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5762_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsJumbo, ParamsEEE, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5762_LHinst_MRRS.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsJumbo, ParamsEEE, ParamsRingSize, ParamsMRRS
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762_LHinst_MRRS.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsJumbo, ParamsEEE, ParamsRingSize, ParamsMRRS, ParamsJIRA26220
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762_LHinst_MRRS_JIRA26220.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5762RSS4_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM5762.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueuesDef4, ParamsPM, ParamsJumbo, ParamsEEE, ParamsRingSize
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM5762RSS4_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM57766_LHinst_EAV.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57766_EAV.Params, ParamsTuning55,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsRssQueues, ParamsPM, ParamsJumbo, ParamsEEE, ParamsEAV
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS

[BCM57766_LHinst_EAV.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57766_LHinst_DMAr.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57766.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsJumbo, ParamsEEE, ParamsDMAr
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS
AddReg = ParamsTbt

[BCM57766_LHinst_DMAr.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM57766_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = LH_AddReg, Intr_coal, BCM57766.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsRssQueues, ParamsPM, ParamsJumbo, ParamsEEE
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6TxRx
AddReg = ParamsGSOv4, ParamsGSOv6
AddReg = ParamsRSS
AddReg = ParamsTbt

[BCM57766_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1eStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1eStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1HALe_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1HALe_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1F3E_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3E_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1F3M_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3M_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsCQ29902_0, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3MNCQ29902_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1F3MNeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1F3MNeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx

[BCM5787A1F3MNeStar_LHinst_NoLSO.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1MeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1MeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1Me_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1Me_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsCQ39100, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1Me_LHinst_CQ39100.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787A1MBDFS_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787A1MBDFS_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787MHALe_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787MHALe_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5787MDisableGig_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsWOLLink, ParamsPM, ParamsDisableGig
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3
AddReg = ParamsNtv6Tx, ParamsGSOv4

[BCM5787MDisableGig_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750MHALe_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750MHALe_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5750A1FeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1FeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsCQ39100, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1Fe_LHinst_CQ39100.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750FHAL_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsWOLLink, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750FHAL_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1CLNAHKD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg_CLNAHKD_1, DelReg.Jumbo, DelReg.TaskOffload, DelReg.LAA
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1CLNAHKD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1CLDeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg_CLNAHKD_1, DelReg.Jumbo, DelReg.Wol, DelReg.TaskOffload, DelReg.LAA
AddReg          = LH_AddReg, BCM5750.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1CLDeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3E_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3E_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3Ne_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3Ne_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3Me_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
DelReg          = DelReg_Generic
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3Me_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5750A1F3MNe_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5750.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLogOptions, ParamsM, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5750A1F3MNe_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705M_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705M.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705M_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705F_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705F.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705F_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705A2_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705A2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705A2_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705MA2_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705MA2_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5705MA2F2_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705MA2F2_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5705MA2F2N_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5705MA2.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5705MA2F2N_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5901_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LgSnd
AddReg          = LH_AddReg, Intr_coal, BCM5901.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5901_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5788_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5788_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5788F1_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5788F1_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5788F1N_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5788F1N_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5703S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5703S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5703SW_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5703.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5703SW_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5704S_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704S_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5704SW_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704SW_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5704SW_LHinst.NTamd64_d.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.RequestedMediaType, DelReg.Wol, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5704.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi, ParamsDropVlan
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5704SW_LHinst.NTamd64_d.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[3C998T_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[3C998T_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[3C998SX_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[3C998SX_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[3C999T_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5701.Params, ParamsTuning, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[3C999T_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[OEM1_DEV4_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, ParamsTuning, OEM1_DEV4.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[OEM1_DEV4_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[OEM1_DEV5_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, ParamsTuning, OEM1_DEV5.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[OEM1_DEV5_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[OEM1_DEV6_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5702.Params, ParamsTuning, OEM1_DEV6.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[OEM1_DEV6_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906eStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906eStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906MeStar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906MeStar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906MD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol, DelReg.LAA, DelReg.TaskOffload, DelReg_CLNAHKD
AddReg          = LH_AddReg, BCM5788.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, 5906Mvsta.Params, eStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906MD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog



[BCM5906MHAL_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.Wol
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906MHAL_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5906F3M_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo, DelReg.LsoV1IPv4
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906F3M_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906Mstar_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906Mstar_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906Mstar_LHinst_CQ39100.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM, ParamsCQ39100
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906Mstar_LHinst_CQ39100.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


[BCM5906Star_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg.Jumbo
AddReg          = LH_AddReg, Intr_coal, BCM5788.Params, ParamsTuning,  ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5906Star_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog

[BCM5761MCLNAHKD_LHinst.NTamd64.6.1]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg_Generic, DelReg_CLNAHKD, DelReg.Jumbo, DelReg_CLNAHKD_1, DelReg.TaskOffload, DelReg.LAA, DelReg.Wol
AddReg          = LH_AddReg, BCM5761_chip.Params, ParamsTuning,  ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, ClnahkdXP.Params, 5761vsta.Params, eStar, ParamsPM
CopyFiles       = CopyFile_Binary
BusType         = 5
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14  ; NdisPhysicalMedium802_3

[BCM5761MCLNAHKD_LHinst.NTamd64.6.1.Services]
AddService = b57nd60a, 2, BRCM_LH_Service, LH_EventLog


;*******************************************************************************
; 32-bit Windows Longhorn common sections.
;*******************************************************************************

[LH_AddReg]
HKR, Ndi,            Service,    0, "b57nd60a"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Intr_coal]
HKR, Ndi\Params\*InterruptModeration,        ParamDesc, , %ParamDesc_InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,        default,   , "1"
HKR, Ndi\Params\*InterruptModeration,        type,      , "enum"
HKR, Ndi\Params\*InterruptModeration\enum,   0,         , %GenDisable%
HKR, Ndi\Params\*InterruptModeration\enum,   1,         , %GenEnable%

[MsiSupportStd]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1

[MsiXSupportStd]
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 0x03

[LH_EventLog]
AddReg = LH_AddEventLogReg

[LH_AddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57nd60a.sys"
HKR, , TypesSupported  , 0x00010001, 7


[BRCM_LH_Service]
DisplayName    = %SvcDispName%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57nd60a.sys
LoadOrderGroup = NDIS
Addreg         = bcmPnpInstallReg


[bcmPnpInstallReg]
HKR,,product_version,0,"19.0.0"

;*******************************************************************************
; Registry parameters.
;*******************************************************************************

[BCM5701.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5702.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5703.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5704.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705M.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705F.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705A2.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705MA2.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , MaxTxQueueLen,            0, "20000"

[BCM5750R.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5761_chip.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , DisableGig,               0, "0"
HKR, , UserTaskOffloadCapDisable, 0, "62914560"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5761S_chip.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , DisableGig,               0, "0"
;HKR, , UserTaskOffloadCapDisable, 0, "62914560"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5717.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , GphyGreenMode,            0, "4"
HKR, , TSS,                      0, "0"
HKR, , MaxTxQueueLen,            0, "20000"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5717_OEM1.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , GphyGreenMode,            0, "4"
HKR, , TSS,                      0, "0"
HKR, , MaxTxQueueLen,            0, "20000"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5717C0.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , TSS,                      0, "1"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5718S.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , TxAltCoalescingTicks,     0, "100"
HKR, , RxAltCoalescingTicks,     0, "100"
HKR, , TSS,                      0, "0"
HKR, , MaxTxQueueLen,            0, "20000"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5718S_OEM1.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , TSS,                      0, "0"
HKR, , MaxTxQueueLen,            0, "20000"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5718S_OEM2.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , TxAltCoalescingTicks,     0, "100"
HKR, , RxAltCoalescingTicks,     0, "100"
HKR, , TSS,                      0, "0"
HKR, , MaxTxQueueLen,            0, "20000"
HKR, , RegDmpBufSize,            0, "32768"
HKR, , EnableRecovery,           0, "1"
HKR, , CQ72222,                  0, "1"

[BCM5719.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , TSS,                      0, "1"
HKR, , Limit4kBd,                0, "1"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5719_OEM1.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , TSS,                      0, "1"
HKR, , Limit4kBd,                0, "1"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5720.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , TSS,                      0, "1"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5720_OEM1.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , TSS,                      0, "1"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5764M.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , RegDmpBufSize,            0, "32768"

[BCM5764MR.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , RegDmpBufSize,            0, "32768"

[BCM57760.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , GphyGreenMode,            0, "4"
HKR, , RegDmpBufSize,            0, "32768"

[BCM57765.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , GphyGreenMode,            0, "4"
HKR, , RegDmpBufSize,            0, "32768"

[BCM57766.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , RegDmpBufSize,            0, "32768"

[BCM57766_EAV.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "50"
HKR, , TxAltMaxCoalescedFrames,  0, "50"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , RegDmpBufSize,            0, "32768"

HKR, , EavTxCoalescingTicks,        0, "30"
HKR, , EavTxMaxCoalescedFrames,     0, "16"
HKR, , EavTxMaxCoalescedFramesDuringInt, 0, "16"

[BCM5762.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , RegDmpBufSize,            0, "32768"
HKR, , HeartbeatInterval,        0, "3000"

[BCM5901.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5788.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[OEM1_DEV4.Params]
HKR, , AdminSettingsLevel,               0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "0"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV5.Params]
HKR, , AdminSettingsLevel,               0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "1"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV6.Params]
HKR, , AdminSettingsLevel,               0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "1"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[ClnahkdXP.Params]
HKR, , AdminSettingsLevel,               0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *LsoV1IPv4,               0, "1"
HKR, , RxMtu,                    0, "1514"
HKR, , WireSpeed,                0, "1"
HKR, , *InterruptModeration,     0, "1"

[ParamsGSOv4]
HKR, Ndi\Params\*LsoV2IPv4,        ParamDesc, , %ParamDesc_GSOv4%
HKR, Ndi\Params\*LsoV2IPv4,        default,   , "1"
HKR, Ndi\Params\*LsoV2IPv4,        type,      , "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*LsoV2IPv4\enum,   "1",       , %GenEnable%

[ParamsGSOv6]
HKR, Ndi\Params\*LsoV2IPv6,        ParamDesc, , %ParamDesc_GSOv6%
HKR, Ndi\Params\*LsoV2IPv6,        default,   , "1"
HKR, Ndi\Params\*LsoV2IPv6,        type,      , "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*LsoV2IPv6\enum,   "1",       , %GenEnable%

[ParamsRSS]
HKR, Ndi\Params\*RSS,        ParamDesc, , %ParamDesc_RSS%
HKR, Ndi\Params\*RSS,        default,   , "1"
HKR, Ndi\Params\*RSS,        type,      , "enum"
HKR, Ndi\Params\*RSS\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*RSS\enum,   "1",       , %GenEnable%

[ParamsRSSDisabled]
HKR, Ndi\Params\*RSS,        ParamDesc, , %ParamDesc_RSS%
HKR, Ndi\Params\*RSS,        default,   , "0"
HKR, Ndi\Params\*RSS,        type,      , "enum"
HKR, Ndi\Params\*RSS\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*RSS\enum,   "1",       , %GenEnable%

[ParamsRssQueues]
HKR, Ndi\Params\*NumRssQueues,        ParamDesc, , %ParamDesc_RSS_Queues%
HKR, Ndi\Params\*NumRssQueues,        default,   , "4"
HKR, Ndi\Params\*NumRssQueues,        type,      , "long"
hkr, Ndi\Params\*NumRssQueues,        min,       , "1"
hkr, Ndi\Params\*NumRssQueues,        max,       , "4"

[ParamsRssQueuesDef4]
HKR, Ndi\Params\*NumRssQueues,        ParamDesc, , %ParamDesc_RSS_Queues%
HKR, Ndi\Params\*NumRssQueues,        default,   , "4"
HKR, Ndi\Params\*NumRssQueues,        type,      , "long"
hkr, Ndi\Params\*NumRssQueues,        min,       , "1"
hkr, Ndi\Params\*NumRssQueues,        max,       , "4"

[ParamsRssBaseProcNumber]
hkr, Ndi\Params\*RssBaseProcNumber, ParamDesc, , %ParamDesc_RssBaseProcNumber%
hkr, Ndi\Params\*RssBaseProcNumber, default,   , "0"
hkr, Ndi\Params\*RssBaseProcNumber, type,      , "int"
hkr, Ndi\Params\*RssBaseProcNumber, min,       , "0"
hkr, Ndi\Params\*RssBaseProcNumber, max,       , "63"
hkr, Ndi\Params\*RssBaseProcNumber, step,      , "1"
hkr, Ndi\Params\*RssBaseProcNumber, base,      , "10"

[5906Mvsta.Params]
HKR, , AdminSettingsLevel,               0, "2"
HKR, , *TCPUDPChecksumOffloadIPv4,0, "1"
HKR, , *InterruptModeration,     0, "1"

[5754vsta.Params]
HKR, , *TCPUDPChecksumOffloadIPv6,      0, "1"
HKR, , *LsoV2IPv4,                      0, "1"

[5755vsta.Params]
HKR, , *RSS,                            0, "1"

[5761vsta.Params]
HKR, , *TCPUDPChecksumOffloadIPv6,      0, "1"
HKR, , *LsoV2IPv4,                      0, "1"
HKR, , *LsoV2IPv6,                      0, "1"

[5764vsta.Params]
HKR, , *TCPUDPChecksumOffloadIPv6,      0, "1"
HKR, , *LsoV2IPv4,                      0, "1"
HKR, , *LsoV2IPv6,                      0, "1"

[ParamsNt]
HKR, , AdminSettingsLevel,               0, "2"

HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4,        ParamDesc, , %ParamDesc_TCPUDPChecksumOffloadIPv4%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4,        default,   , "3"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4,        type,      , "enum"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "1",       , %GenTxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "2",       , %GenRxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4\enum,   "3",       , %GenTxRxEnable%

[ParamsNtv6Tx]
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        ParamDesc, , %ParamDesc_TCPUDPChecksumOffloadIPv6%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        default,   , "1"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        type,      , "enum"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "1",       , %GenTxEnable%

[ParamsNtv6TxRx]
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        ParamDesc, , %ParamDesc_TCPUDPChecksumOffloadIPv6%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        default,   , "3"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6,        type,      , "enum"
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "1",       , %GenTxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "2",       , %GenRxEnable%
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6\enum,   "3",       , %GenTxRxEnable%

[ParamsNT8021p]
HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , %PriandVlan%
HKR, Ndi\Params\*PriorityVLANTag,      default,, "3"
HKR, Ndi\Params\*PriorityVLANTag,      type,   , "enum"
HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , %PriVlanDisabled%
HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , %PriEnabled%
HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , %VlanEnabled%
HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , %PriVlanEnabled%

HKR, Ndi\params\VlanID,     ParamDesc,       0, %VlanID%
HKR, Ndi\params\VlanID,     default,         0, "0"
HKR, Ndi\params\VlanID,     type,            0, "long"
HKR, Ndi\params\VlanID,     min,             0, "0"
HKR, Ndi\params\VlanID,     max,             0, "4094"
HKR, Ndi\params\VlanID,     step,            0, "1"
HKR, Ndi\params\VlanID,     base,            0, "10"

[ParamsNtW9x]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "0"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 4,          , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsNtW9xFJ]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "0"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 4,          , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsNtW9xMOBILE]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "0"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 4,          , %FlowControl_Auto%

[ParamsNtW9xSPECIAL]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "0"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsJumbo]
HKR, Ndi\Params\*JumboPacket, ParamDesc, , %JumboMtu%
HKR, Ndi\Params\*JumboPacket, default,   , "1514"
HKR, Ndi\Params\*JumboPacket, type,      , "long"
HKR, Ndi\Params\*JumboPacket, min,       , "1500"
HKR, Ndi\Params\*JumboPacket, max,       , "9014"
;HKR, Ndi\Params\*JumboPacket, step,      , "500"
;HKR, Ndi\Params\*JumboPacket, base,      , "10"
HKR, , JumboPacketMode, 0, "1"

[ParamsWireSpeed]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsWireSpeed_CO]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed_CO%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsWOLLink]
HKR, Ndi\Params\WakeOnLink,        ParamDesc, , %WakeOnLink%
HKR, Ndi\Params\WakeOnLink,        default,   , "0"
HKR, Ndi\Params\WakeOnLink,        type,      , "enum"
HKR, Ndi\Params\WakeOnLink\enum,   0,         , %WakeOnLink_Disable%
HKR, Ndi\Params\WakeOnLink\enum,   1,         , %WakeOnLink_Enable%



[ParamsWireSpeedSPECIAL]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsLogOptions]
HKR, Ndi\Params\LogLevelInfo,        ParamDesc, , %LogLevelInfo%
HKR, Ndi\Params\LogLevelInfo,        default,   , "0"
HKR, Ndi\Params\LogLevelInfo,        type,      , "enum"
HKR, Ndi\Params\LogLevelInfo\enum,   0,         , %LogLevelInfo_Disable%
HKR, Ndi\Params\LogLevelInfo\enum,   1,         , %LogLevelInfo_Enable%
HKR, Ndi\Params\LogLevelWarn,        ParamDesc, , %LogLevelWarn%
HKR, Ndi\Params\LogLevelWarn,        default,   , "0"
HKR, Ndi\Params\LogLevelWarn,        type,      , "enum"
HKR, Ndi\Params\LogLevelWarn\enum,   0,         , %LogLevelWarn_Disable%
HKR, Ndi\Params\LogLevelWarn\enum,   1,         , %LogLevelWarn_Enable%


[ParamsC]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 1,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 2,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\*SpeedDuplex\enum, 3,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 4,         , %Speed_Duplex_100Mb_Fd%

[ParamsC_CO]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 1,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 2,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\*SpeedDuplex\enum, 3,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 4,         , %Speed_Duplex_100Mb_Fd%

[ParamsC1G]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 1,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 2,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\*SpeedDuplex\enum, 3,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 4,         , %Speed_Duplex_100Mb_Fd%
HKR, Ndi\Params\*SpeedDuplex\enum, 6,         , %Speed_Duplex_1000Mb_Fd%


[ParamsCSPECIAL]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%

[ParamsC100]
HKR, Ndi\Params\*SpeedDuplex,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\*SpeedDuplex,      default,   , "0"
HKR, Ndi\Params\*SpeedDuplex,      type,      , "enum"
HKR, Ndi\Params\*SpeedDuplex\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\*SpeedDuplex\enum, 1,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 2,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\*SpeedDuplex\enum, 3,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\*SpeedDuplex\enum, 4,         , %Speed_Duplex_100Mb_Fd%


[ParamsWOL]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %GenEnable%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%

[ParamsWOLeStar]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %GenEnable%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "256"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%

[ParamsWOL_OEMC]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%
HKR, , WolSpeed, 0, "3"

[ParamsWOLeStar_CO]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %GenEnable%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed_CO%
HKR, Ndi\Params\WolSpeed,       default,   , "256"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%

[ParamsWOLeStarAuto]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %GenEnable%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%

[eStar]
HKR, , WolSpeed, 0, "256"

[ParamsM]
HKR, , ClockControl,          0, "1"

[ParamsCQ29902_0]
HKR, , CQ29902Errata,         0, "0"

[ParamsCQ35234]
HKR, , CQ35234,               0, "0"

[ParamsCQ39100]
HKR, , CQ39100,               0, "1"

[ParamsCQ47248]
HKR, , CQ47248,               0, "0"

[ParamsWOLTbi]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%
HKR, , TbiWol,                   0, "1"

[ParamsWOLTbi_None]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "0"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%
HKR, , TbiWol,                   0, "1"

[ParamsWOLNS]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %GenEnable%

[ParamsFlow]
HKR, Ndi\Params\*FlowControl,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\*FlowControl,      default,    , "0"
HKR, Ndi\Params\*FlowControl,      type,       , "enum"
HKR, Ndi\Params\*FlowControl\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\*FlowControl\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\*FlowControl\enum, 4,          , %FlowControl_Auto%

[ParamsLgSndJumboCombo]
HKR, , *LsoV1IPv4,                   0, "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    ParamDesc, , %TaskOffload_LargeSend_Jumbo%
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    default,   , "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 0,        , %TaskOffload_LargeSend_Disable_Both%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 1,        , %TaskOffload_LargeSend_Enable_JumboDisable%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 2,        , %TaskOffload_LargeSend_Disable_JumboEnable3000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 3,        , %TaskOffload_LargeSend_Disable_JumboEnable4500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 4,        , %TaskOffload_LargeSend_Disable_JumboEnable6000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 5,        , %TaskOffload_LargeSend_Disable_JumboEnable7500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 6,        , %TaskOffload_LargeSend_Disable_JumboEnable9000%

[ParamsLgSndJumboCombo_5761]
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    ParamDesc, , %TaskOffload_LargeSend_Jumbo%
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    default,   , "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 0,        , %TaskOffload_LargeSend_Disable_Both%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 1,        , %TaskOffload_LargeSend_Enable_JumboDisable%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 2,        , %TaskOffload_LargeSend_Disable_JumboEnable3000%

[ParamsWOLMagic]
HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %GenDisable%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %GenEnable%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%

[ParamsIpsecv2]
HKR, Ndi\Params\*IPsecOffloadV2,       ParamDesc, , %ParamDesc_IPsecOffloadV2%
HKR, Ndi\Params\*IPsecOffloadV2,       default,   , "3"
HKR, Ndi\Params\*IPsecOffloadV2,       type,      , "enum"
HKR, Ndi\Params\*IPsecOffloadV2\enum,  0,         , %GenDisable%
HKR, Ndi\Params\*IPsecOffloadV2\enum,  1,         , %IpsecAu%
HKR, Ndi\Params\*IPsecOffloadV2\enum,  2,         , %IpsecEsp%
HKR, Ndi\Params\*IPsecOffloadV2\enum,  3,         , %IpsecAuEsp%

[ParamsDropVlan]
HKR, , DropVlanPkt,          0, "1"

[ParamsTuning]
HKR, Ndi\Params\*ReceiveBuffers,      ParamDesc,          0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,      type,               0, "dword"
HKR, Ndi\Params\*ReceiveBuffers,      Default,            0, "200"
HKR, Ndi\Params\*ReceiveBuffers ,     min,                0, "64"
HKR, Ndi\Params\*ReceiveBuffers ,     max,                0, "511"

HKR, Ndi\Params\*TransmitBuffers ,   ParamDesc,          0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers ,   type,               0, "dword"
HKR, Ndi\Params\*TransmitBuffers ,   default,            0, "200"
HKR, Ndi\Params\*TransmitBuffers ,   min,                0, "100"
HKR, Ndi\Params\*TransmitBuffers ,   max,                0, "600"

[ParamsTuning25]
HKR, Ndi\Params\*ReceiveBuffers,      ParamDesc,          0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,      type,               0, "dword"
HKR, Ndi\Params\*ReceiveBuffers,      Default,            0, "200"
HKR, Ndi\Params\*ReceiveBuffers ,     min,                0, "64"
HKR, Ndi\Params\*ReceiveBuffers ,     max,                0, "511"

HKR, Ndi\Params\*TransmitBuffers ,   ParamDesc,          0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers ,   type,               0, "dword"
HKR, Ndi\Params\*TransmitBuffers ,   default,            0, "500"
HKR, Ndi\Params\*TransmitBuffers ,   min,                0, "100"
HKR, Ndi\Params\*TransmitBuffers ,   max,                0, "600"

[ParamsTuning55]
HKR, Ndi\Params\*ReceiveBuffers,      ParamDesc,          0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,      type,               0, "dword"
HKR, Ndi\Params\*ReceiveBuffers,      Default,            0, "500"
HKR, Ndi\Params\*ReceiveBuffers ,     min,                0, "64"
HKR, Ndi\Params\*ReceiveBuffers ,     max,                0, "511"

HKR, Ndi\Params\*TransmitBuffers ,   ParamDesc,          0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers ,   type,               0, "dword"
HKR, Ndi\Params\*TransmitBuffers ,   default,            0, "500"
HKR, Ndi\Params\*TransmitBuffers ,   min,                0, "100"
HKR, Ndi\Params\*TransmitBuffers ,   max,                0, "600"

[ParamsPM]
HKR, Ndi\Params\*PMARPOffload,        ParamDesc, , %ParamDesc_PmArp%
HKR, Ndi\Params\*PMARPOffload,        default,   , "1"
HKR, Ndi\Params\*PMARPOffload,        type,      , "enum"
HKR, Ndi\Params\*PMARPOffload\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*PMARPOffload\enum,   "1",       , %GenEnable%

HKR, Ndi\Params\*PMNSOffload,        ParamDesc, , %ParamDesc_PmNs%
HKR, Ndi\Params\*PMNSOffload,        default,   , "1"
HKR, Ndi\Params\*PMNSOffload,        type,      , "enum"
HKR, Ndi\Params\*PMNSOffload\enum,   "0",       , %GenDisable%
HKR, Ndi\Params\*PMNSOffload\enum,   "1",       , %GenEnable%

[ParamsVmq]

HKR, Ndi\Params\*VMQ,                       ParamDesc, , %VMQ%
HKR, Ndi\Params\*VMQ,                       default,   , "1"
HKR, Ndi\Params\*VMQ,                       type,      , "enum"
HKR, Ndi\Params\*VMQ\enum,                  0,         , %VMQ_Disable%
HKR, Ndi\Params\*VMQ\enum,                  1,         , %VMQ_Enable%
HKR, , *VMQ,        0, "0"

HKR, Ndi\Params\*VMQVlanFiltering,          ParamDesc, , %VMQ_Vlan%
HKR, Ndi\Params\*VMQVlanFiltering,          default,   , "1"
HKR, Ndi\Params\*VMQVlanFiltering,          type,      , "enum"
HKR, Ndi\Params\*VMQVlanFiltering\enum,     0,         , %VMQ_Vlan_Disable%
HKR, Ndi\Params\*VMQVlanFiltering\enum,     1,         , %VMQ_Vlan_Enable%

;HKR, Ndi\Params\*VMQLookaheadSplit,        ParamDesc, , %VMQ_HDS%
;HKR, Ndi\Params\*VMQLookaheadSplit,        default,   , "0"
;HKR, Ndi\Params\*VMQLookaheadSplit,        type,      , "enum"
;HKR, Ndi\Params\*VMQLookaheadSplit\enum,   0,         , %VMQ_HDS_Disable%
;HKR, Ndi\Params\*VMQLookaheadSplit\enum,   1,         , %VMQ_HDS_Enable%

HKR, Ndi\Params\*MaxRssProcessors,        	ParamDesc, , %ParamDesc_MaxRssProcs%
HKR, Ndi\Params\*MaxRssProcessors,        	default,   , "4"
HKR, Ndi\Params\*MaxRssProcessors,        	type,      , "long"
HKR, Ndi\Params\*MaxRssProcessors,        	min,       , "1"
HKR, Ndi\Params\*MaxRssProcessors,        	max,       , "4"

[ParamsRingSize]
HKR, , LargeSizeRxRing,               0, "0"

[ParamsMRRS]
HKR, , MRRS,                     0,  "1"

[ParamsJIRA26220]
HKR, , JIRA26220,                0,  "1"

[ParamsRingSizeEnabled]
HKR, , LargeSizeRxRing,               0, "1"

[ParamsEEE]
HKR, Ndi\Params\*EEE,               ParamDesc, , %EEE%
HKR, Ndi\Params\*EEE,               default,   , "0"
HKR, Ndi\Params\*EEE,               type,      , "enum"
HKR, Ndi\Params\*EEE\enum,          0,         , %EEE_Disable%
HKR, Ndi\Params\*EEE\enum,          1,         , %EEE_Enable%

HKR, Ndi\Params\EeeCtrlMode,        ParamDesc, , %EEE_Control%
HKR, Ndi\Params\EeeCtrlMode,        default,   , "1"
HKR, Ndi\Params\EeeCtrlMode,        type,      , "enum"
HKR, Ndi\Params\EeeCtrlMode\enum,   0,         , %EEE_MaxPowerSave%
HKR, Ndi\Params\EeeCtrlMode\enum,   1,         , %EEE_Balance%
HKR, Ndi\Params\EeeCtrlMode\enum,   2,         , %EEE_MaxPerformance%

[ParamsEAV]
HKR, Ndi\Params\EAV,               ParamDesc, , %EAV%
HKR, Ndi\Params\EAV,               default,   , "1"
HKR, Ndi\Params\EAV,               type,      , "enum"
HKR, Ndi\Params\EAV\enum,          0,         , %EAV_Disable%
HKR, Ndi\Params\EAV\enum,          1,         , %EAV_Enable%
HKR, , EAV, 0, "1"

[ParamsDMAr]
HKR, Parameters, DmaRemappingCompatible, 0x00010001, 2

;1 = opt-in, 2 = opt-in only for external devices

[ParamsEEE_CO]
HKR, Ndi\Params\*EEE,               ParamDesc, , %EEE_CO%
HKR, Ndi\Params\*EEE,               default,   , "0"
HKR, Ndi\Params\*EEE,               type,      , "enum"
HKR, Ndi\Params\*EEE\enum,          0,         , %EEE_Disable%
HKR, Ndi\Params\*EEE\enum,          1,         , %EEE_Enable%

HKR, Ndi\Params\EeeCtrlMode,        ParamDesc, , %EEE_Control_CO%
HKR, Ndi\Params\EeeCtrlMode,        default,   , "1"
HKR, Ndi\Params\EeeCtrlMode,        type,      , "enum"
HKR, Ndi\Params\EeeCtrlMode\enum,   0,         , %EEE_MaxPowerSave%
HKR, Ndi\Params\EeeCtrlMode\enum,   1,         , %EEE_Balance%
HKR, Ndi\Params\EeeCtrlMode\enum,   2,         , %EEE_MaxPerformance%

[ParamsDisableGig]
HKR, , DisableGig,               0, "1"

[ParamsTbt]
HKR, , TBT,               	0, "1"

[ParamsVAUX1G]
HKR, , VAUX1G,                0,  "1"

;*******************************************************************************
; DriverInfo section.
;*******************************************************************************

[DriverInfo]


;*******************************************************************************
; Keys to remove.
;*******************************************************************************

[DelReg_Generic]
;; Vista
HKR, , UserTaskOffloadCapDisable
HKR, ,          LargeSendOffload
HKR, Ndi\Params\LargeSendOffload

HKR, ,          InterruptModeration
HKR, Ndi\Params\InterruptModeration

HKR, ,          AdminSettingsLevel
HKR, Ndi\Params\AdminSettingsLevel

HKR, ,          RSS
HKR, Ndi\Params\RSS

HKR, ,          TaskOffloadCap
HKR, Ndi\Params\TaskOffloadCap

HKR, ,          *TCPChksumOffv4
HKR, Ndi\Params\*TCPChksumOffv4
HKR, ,          *UDPChksumOffv4
HKR, Ndi\Params\*UDPChksumOffv4
HKR, ,          *IPChksumOffv4
HKR, Ndi\Params\*IPChksumOffv4

HKR, ,          *TCPChksumOffv6
HKR, Ndi\Params\*TCPChksumOffv6
HKR, ,          *UDPChksumOffv6
HKR, Ndi\Params\*UDPChksumOffv6

HKR, ,          *TCPChecksumOffloadIPv4
HKR, Ndi\Params\*TCPChecksumOffloadIPv4
HKR, ,          *UDPChecksumOffloadIPv4
HKR, Ndi\Params\*UDPChecksumOffloadIPv4
HKR, ,          *IPChecksumOffloadIPv4
HKR, Ndi\Params\*IPChecksumOffloadIPv4

HKR, ,          *TCPChecksumOffloadIPv6
HKR, Ndi\Params\*TCPChecksumOffloadIPv6
HKR, ,          *UDPChecksumOffloadIPv6
HKR, Ndi\Params\*UDPChecksumOffloadIPv6

HKR, ,          *LSOv4
HKR, Ndi\Params\*LSOv4
HKR, ,          *GSOv4
HKR, Ndi\Params\*GSOv4
HKR, ,          *GSOv6
HKR, Ndi\Params\*GSOv6

HKR, ,          *LsoV1IPv4
HKR, Ndi\Params\*LsoV1IPv4

HKR, ,          FlowControlCap
HKR, Ndi\Params\FlowControlCap
HKR, Ndi\Params\RequestedMediaType
HKR, Ndi\Params\*SpeedDuplex
HKR, Ndi\Params\Enable8021p
HKR, NDI\params\*NetworkAddress

HKR, ,          WakeUpModeCap
HKR, Ndi\Params\WakeUpModeCap

HKR, ,          *VMQLookaheadSplit
HKR, Ndi\Params\*VMQLookaheadSplit

HKR, ,          ClockControl

HKR, ,          LargeSizeRxRing
HKR, Ndi\Params\LargeSizeRxRing

[DelReg_CLNAHKD]
HKR, ,          *InterruptModeration
HKR, Ndi\Params\*InterruptModeration
HKR, ,          WakeOnLink
HKR, Ndi\Params\WakeOnLink
HKR, ,          LogLevelInfo
HKR, Ndi\Params\LogLevelInfo
HKR, ,          *RSS
HKR, Ndi\Params\*RSS

[DelReg_CLNAHKD_1]
HKR, ,          *LsoV1IPv4
HKR, Ndi\Params\*LsoV1IPv4
HKR, ,          *TCPUDPChecksumOffloadIPv6
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv6
HKR, ,          *TCPUDPChecksumOffloadIPv4
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4
HKR, ,          *GSOv4
HKR, Ndi\Params\*GSOv4
HKR, ,          *GSOv6
HKR, Ndi\Params\*GSOv6

[DelReg.RequestedMediaType]
HKR, Ndi\Params\RequestedMediaType
HKR, Ndi\Params\*SpeedDuplex
HKR, Ndi\Params\Enable8021p

[DelReg.Wol]
HKR, Ndi\Params\WakeUpModeCap

[DelReg.Jumbo]
HKR, Ndi\Params\RxMtu
HKR, ,         \RxMtu
HKR, Ndi\Params\JumboPacketMode
HKR, ,          JumboPacketMode

[DelReg.GphyGreenMode]
HKR, Ndi\Params\GphyGreenMode

[DelReg.LgSnd]
HKR, Ndi\Params\LargeSendOffload

[DelReg.LsoV1IPv4]
HKR, Ndi\Params\*LsoV1IPv4
HKR, ,          *LsoV1IPv4


[DelReg.LAA]
HKR, Ndi\params\*NetworkAddress
HKR, , *NetworkAddress
HKR, Ndi\params\NetworkAddress
HKR, , NetworkAddress

[DelReg.TaskOffload]
HKR, Ndi\Params\*TCPUDPChecksumOffloadIPv4
HKR, ,*TCPUDPChecksumOffloadIPv4

[DelReg.ParamsRSS]
HKR, Ndi\Params\*RSS
HKR, ,*RSS

[DelReg.ParamsC]
HKR, Ndi\Params\*SpeedDuplex

[DelReg.ParamsIpsecv4]
HKR, Ndi\Params\*IPsecOffloadV2IPv4

[DelReg.ParamsIpsecv2]
HKR, Ndi\Params\*IPsecOffloadV2

[DelReg.ParamsTuning]
HKR, Ndi\Params\*ReceiveBuffers
HKR, ,         \*ReceiveBuffers
HKR, Ndi\Params\*TransmitBuffers
HKR, ,         \*TransmitBuffers

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 11
CopyFile_Binary = 12

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
b57nd60a.sys = 1

[CopyFile_Binary]
b57nd60a.sys,,,1


;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
BRCM                = "Broadcom"
SvcDispName         = "Broadcom NetXtreme Gigabit Ethernet - NDIS 6.0"
DISK_DESC           = "Broadcom NetXtreme Installation Media"

BCM5700             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5701             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5702             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705F            = "Broadcom 570x 10/100 Integrated Controller"
BCM5750             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1F          = "Broadcom NetXtreme Fast Ethernet"
BCM5751A1           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5714             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5714S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5714SW           = "Broadcom NetXtreme Gigabit Ethernet"

BCM5786             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787F            = "Broadcom NetLink (TM) Fast Ethernet"
BCM5787M            = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787MKDMNUN      = "Broadcom NetLink (TM) Ethernet"
BCM5755             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5754             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5764M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM57760            = "Broadcom NetXtreme Gigabit Ethernet"
BCM57765            = "Broadcom NetXtreme Gigabit Ethernet"
BCM57766            = "Broadcom NetXtreme Gigabit Ethernet"
BCM57766_OEM1       = "Echo Streamware NIC-1"
BCM5717             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5718S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5719             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5719L            = "Broadcom 5719 1GbE RJ45 4-port OCP Ethernet Adapter"
BCM5719T            = "HPE Ethernet 1Gb 4-port 331T OCP3 Adapter"
BCM5719I            = "HPE Ethernet 1Gb 2-port 331i Adapter"
BCM5719_BRCM        = "Broadcom NetXtreme 5719 Quad Port Gigabit PCIe Adapter"
BCM5719C_OEMC       = "Gigabit BCM5719 Network Adapter"
BCM5719S_OEMC       = "Gigabit BCM5719 Fiber Network Adapter"
BCM5720             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5720L1           = "Broadcom 5720 1GbE RJ45 2-Port PCIe Ethernet LOM"
BCM5720L2           = "Broadcom 5720 1GbE 2-port OCP Ethernet Adapter"
BCM5720_BRCM        = "Broadcom NetXtreme 5720 Dual Port Gigabit PCIe Adapter"
BCM5720L            = "Supermicro Gigabit Ethernet Controller"
BCM5720_SMC         = "Supermicro SIOM Gigabit Ethernet Controller"
BCM5720_Kura        = "Kura_LOM_1GbE"
BCM5762             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5761_OEM1        = "Broadcom NetXtreme Gigabit Ethernet Plus"

BCM5750A1STSP       = "Embedded Broadcom NetXtreme 5721 PCI-E Gigabit NIC"

BCM5750B0           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750B0F          = "Broadcom NetXtreme Fast Ethernet"

BCM5901             = "Broadcom NetXtreme Fast Ethernet"
BCM5782             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5788             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5789             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5700FB           = "Broadcom NetXtreme Gigabit Fiber"
BCM5700FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5703S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5703SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5704SW           = "Broadcom NetXtreme Gigabit Ethernet"

BCM5718_OEM1        = "D-Link\DGE-560SX (Fiber mode only)"

3C998T              = "3Com Dual Port 10/100/1000 PCI-X Server NIC"
3C998SX             = "3Com Dual Port 1000-SX PCI-X Server NIC"
3C999T              = "3Com Quad Port 10/100/1000 PCI-X Server NIC"

OEM1_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV4           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV5           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"
OEM2_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV4           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV5           = "Broadcom 570x 10/100 Integrated Controller"
OEM3_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV6A1         = "Broadcom NetXtreme Gigabit Ethernet"

BCM5750A1DSF        = "Broadcom NetXtreme 5751 Gigabit Controller"
BCM5750A1DSSF       = "Broadcom NetXtreme 5721 Gigabit Controller"
BCM5750A1DDT        = "Broadcom NetXtreme 57xx Gigabit Controller"
BCM5750A1CLNAHKD    = "Broadcom NetXtreme 57xx Gigabit Controller"

BCM5906             = "Broadcom NetLink (TM) Fast Ethernet"
BCM5906MH           = "Broadcom 590x 10/100 Ethernet"
BCM5906M            = "Broadcom NetLink (TM) Fast Ethernet"

OEM1_DEV7           = "Broadcom 570x Gigabit Integrated Controller"

BCM5705FHA          = "Broadcom NetXtreme FE-A"
BCM5705FHB          = "Broadcom NetXtreme FE-B"

BCM5906_ID4_FEA     = "Broadcom NetLink (TM) FE-A"
BCM5906_ID4_FEB     = "Broadcom NetLink (TM) FE-B"

JumboMtu = "Jumbo Mtu"

FlowControl             = "Flow Control"
FlowControl_Disable     = "Disabled"
FlowControl_Rx_Pause    = "Tx Enabled"
FlowControl_Tx_Pause    = "Rx Enabled"
FlowControl_Rx_Tx_Pause = "Rx & Tx Enabled"
FlowControl_Auto        = "Auto Negotiation"

Speed_Duplex          = "Speed & Duplex"
Speed_Duplex_CO       = "Speed & Duplex (Copper Only)"
Speed_Duplex_Auto     = "Auto Negotiation"
Speed_Duplex_10Mb_Hd  = "10 Mbps Half Duplex"
Speed_Duplex_10Mb_Fd  = "10 Mbps Full Duplex"
Speed_Duplex_100Mb_Hd = "100 Mbps Half Duplex"
Speed_Duplex_100Mb_Fd = "100 Mbps Full Duplex"
Speed_Duplex_1000Mb_Fd = "1000 Mb Full Duplex"

QOS_8021p         = "802.1p QOS"
QOS_8021p_Disable = "Disable"
QOS_8021p_Enable  = "Enable"

WireSpeed         = "Ethernet@WireSpeed"
WireSpeed_CO      = "Ethernet@WireSpeed (Copper Only)"
WireSpeed_Disable = "Disable"
WireSpeed_Enable  = "Enable"

WakeOnLink         = "Wake On Link"
WakeOnLink_Disable = "Disable"
WakeOnLink_Enable  = "Enable"

;; Vista
ParamDesc_RSS = "Receive Side Scaling"
ParamDesc_RSS_Queues = "Maximum Number of RSS Queues"
ParamDesc_RssBaseProcNumber = "RSS Base Processor Number"
ParamDesc_MaxRssProcs = "Maximum Number of RSS Processors"
ParamDesc_InterruptModeration = "Interrupt Moderation"
ParamDesc_IPChksumOffv4  = "IPv4 Checksum Offload"
ParamDesc_TCPChksumOffv4 = "TCP Checksum Offload (IPv4)"
ParamDesc_UDPChksumOffv4 = "UDP Checksum Offload (IPv4)"
ParamDesc_TCPChksumOffv6 = "TCP Checksum Offload (IPv6)"
ParamDesc_UDPChksumOffv6 = "UDP Checksum Offload (IPv6)"
ParamDesc_TCPUDPChecksumOffloadIPv4 = "TCP/UDP Checksum Offload (IPv4)"
ParamDesc_TCPUDPChecksumOffloadIPv6 = "TCP/UDP Checksum Offload (IPv6)"
ParamDesc_LSOv4          = "Large Send Offload (IPv4)"
ParamDesc_GSOv4          = "Large Send Offload V2 (IPv4)"
ParamDesc_GSOv6          = "Large Send Offload V2 (IPv6)"
ParamDesc_DMATEST        = "DMA Loopback test"

GenTxEnable = "Tx Enabled"
GenRxEnable = "Rx Enabled"
GenTxRxEnable = "Rx & Tx Enabled"
GenEnable="Enabled"
GenDisable="Disabled"


TaskOffload              = "Checksum Offload"
TaskOffload_None         = "None"
TaskOffload_Rx_Chksum    = "Rx TCP/IP Checksum"
TaskOffload_Tx_Chksum    = "Tx TCP/IP Checksum"
TaskOffload_Rx_Tx_Chksum = "Tx/Rx TCP/IP Checksum"


TaskOffload_LargeSend           = "Large Send Offload"
TaskOffload_LargeSend_Disable   = "Disable"
TaskOffload_LargeSend_Enable    = "Enable"

TaskOffload_LargeSend_Jumbo                           = "LSO & Jumbo Frames"
TaskOffload_LargeSend_Disable_Both                = "Both Disabled"
TaskOffload_LargeSend_Enable_JumboDisable   = "LSO Enabled,Jumbo Off"
TaskOffload_LargeSend_Disable_JumboEnable3000   = "LSO Off,Jumbo 3000"
TaskOffload_LargeSend_Disable_JumboEnable4500   = "LSO Off,Jumbo 4500"
TaskOffload_LargeSend_Disable_JumboEnable6000   = "LSO Off,Jumbo 6000"
TaskOffload_LargeSend_Disable_JumboEnable7500   = "LSO Off,Jumbo 7500"
TaskOffload_LargeSend_Disable_JumboEnable9000   = "LSO Off,Jumbo 9000"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"

WolSpeed       = "WOL Speed"
WolSpeed_CO    = "WOL Speed (Copper Only)"
WolSpeed_Auto  = "Auto"
WolSpeed_10mb  = "10 Mb"
WolSpeed_100mb = "100 Mb"
WolSpeed_1000mb = "1000 Mb"
WolSpeed_LowestAvail = "Lowest Speed Advertised"

NetworkAddress           = "Network Address"


LogLevelInfo    = "Log Information Messages"
LogLevelWarn  = "Log Warning Messages"
LogLevelInfo_Disable  =  "Disable"
LogLevelInfo_Enable  =  "Enable"
LogLevelWarn_Disable  =  "Disable"
LogLevelWarn_Enable  =  "Enable"

GenIgnore  = "Ignore"
GenRecover = "Recover"
GenBreak   = "Break"

VlanID = "VLAN ID"

ipsecv4_IPsecOffloadV2IPv4 = "IPSec Offload (IPv4 only)"
ParamDesc_IpsecOffloadV2 = "IPsec Offload"
IpsecAu = "Auth Header Enabled"
IpsecEsp = "ESP Enabled"
IpsecAuEsp ="Auth Header & ESP Enabled"
ParamDesc_DELAYHC = "Delay HC"
ParamDesc_PartComp = "Partial Completion"

PriandVlan      =       "Priority & VLAN"
PriVlanDisabled =       "Priority & VLAN Disabled"
PriEnabled      =       "Priority Enabled"
VlanEnabled     =       "VLAN Enabled"
PriVlanEnabled  =       "Priority & VLAN Enabled"

ReceiveBuffers    =       "Receive Buffers"
TransmitBuffers   =       "Transmit Buffers"

Default   =  "Default"
Minimum   =  "Minimum"
Maximum   =  "Maximum"

ParamDesc_PmArp ="ARP Offload"
ParamDesc_PmNs  ="NS Offload"

VMQ                 =       "Virtual Machine Queues"
VMQ_Disable         =       "Disabled"
VMQ_Enable          =       "Enabled"

VMQ_Vlan            =       "VMQ VLAN Filtering"
VMQ_Vlan_Disable    =       "Disable"
VMQ_Vlan_Enable     =       "Enable"

VMQ_HDS             =       "VMQ Lookahead Split"
VMQ_HDS_Disable     =       "Disable"
VMQ_HDS_Enable      =       "Enable"

EEE                     = "802.3az EEE"
EEE_CO                  = "802.3az EEE (Copper Only)"
EEE_Disable             = "Disable"
EEE_Enable              = "Enable"

EEE_Control             = "EEE Control Policies"
EEE_Control_CO          = "EEE Control Policies (Copper Only)"
EEE_MaxPowerSave        = "Maximum Power Saving"
EEE_Balance             = "Optimal Power and Performance"
EEE_MaxPerformance      = "Maximum Performance"

EAV                     = "EAV"
EAV_Disable             = "Disable"
EAV_Enable              = "Enable"
