; Copyright (C) 2009 Intel Corporation
; **********************************************************************************************
; **********************************************************************************************
; **    Filename:  iaStorB.inf
; **    Abstract:  Windows* INF File for AHCI Intel(R) Virtual RAID on CPU Driver
; **               Installs: Intel(R) VROC AHCI RAID Controller Miniport (without RST Filter Driver)
; **               Only for Windows 8 releases
; **********************************************************************************************
;
[Version]
Signature="$Windows NT$"
Provider=%INTEL%
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Class=SCSIAdapter
CatalogFile=iaStorB.cat
DriverVer = 10/04/2023,8.5.0.1592
PnPlockdown=1
;
[SourceDisksNames]
1 = %DiskId1%,,,""
;
[DestinationDirs]
DefaultDestDir = 12
;
[ControlFlags]
ExcludeFromSelect = *
;
[Manufacturer]
%INTEL% = INTEL, NTamd64.6.3, NTamd64.10.0, NTamd64.10.0...14393
[iaStorB_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\iaStorB.sys
LoadOrderGroup = SCSI miniport
AddReg         = pnpsafe_pci_addreg
;
[iaStorB_EventLog_Inst]
AddReg = iaStorB_EventLog_AddReg
;
[iaStorB_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorB.sys"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7
;
;********************************************************
;*
;* 64-BIT X86 ARCHITECTURE
;*
;* This section specifies the 64-bit architecture specific INF file entries
;* required to install a driver as a 64-bit compatible driver.
;*
;******************************************************************************
[SourceDisksFiles.amd64]
iaStorB.sys = 1,,,
;
[INTEL.ntamd64.10.0...14393]
;windows 10_64_14393 and later
%PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_2827&CC_0104
;
[INTEL.ntamd64.10.0]
;windows_10_64-bit to windows 10_64_14393
%PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_2827&CC_0104
;
[INTEL.ntamd64.6.3]
;windows_8.1_64-bit
%PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_2827&CC_0104
;
[iaStorB_inst.ntamd64]
CopyFiles=@iaStorB.sys
;
[iaStorB_inst.ntamd64.HW]
AddReg = msi_addreg
AddReg = storport_addreg
AddReg = sgpio_addreg
AddReg = led_addreg
;
[iaStorB_inst.ntamd64.Services]
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst
;
[pnpsafe_pci_addreg]
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x00000008
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8)
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001
;
[Strings]
; Localizable Strings
;
diskId1 = "Intel(R) VROC Installation Disk"
;server
PCI\VEN_8086&DEV_2827&CC_0104.DeviceDesc = "Intel(R) VROC sSATA Controller"
;
INTEL = "Intel Corporation"
;
; Non-Localizable Strings
;
SPSVCINST_ASSOCSERVICE = 0x00000002
REG_MULTI_SZ           = 0x00010000
REG_EXPAND_SZ          = 0x00020000
REG_TYPE_DWORD         = 0x00010001
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
;
; MSI enables.
;
[msi_addreg]
HKR, Interrupt Management, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   1
;
[storport_addreg]
;;; Enables/Disables Idle Power Management for StorPort
HKR, "StorPort", "EnableIdlePowerManagement", %REG_TYPE_DWORD%, 0x00000001
;
[sgpio_addreg]
;;; Enable/disable SGPIO support
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LED_Supported, %REG_TYPE_DWORD%, 0x00000001
;

[led_addreg]
;;; Custimizable LED management
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LedLocateTimeout, %REG_TYPE_DWORD%, 0x0000000C
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LedFaultOnEmptyPortBehavior, %REG_TYPE_DWORD%, 0x00000000
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LedBehaviorForInitializing, %REG_TYPE_DWORD%, 0x00000001
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LedBehaviorForRebuilding, %REG_TYPE_DWORD%, 0x00000000
HKLM, System\CurrentControlSet\Services\iaStorB\Parameters\Device, LedBehaviorForMigrating, %REG_TYPE_DWORD%, 0x00000001
;
