;******************************************************************************
;**                                                                          **
;**  Copyright 2007-2018 Intel Corporation All Rights Reserved.              **
;**                                                                          **
;**  The material contained or described herein and all documents related    **
;**  to such material ("Material") is owned by Intel Corporation or its      **
;**  suppliers or licensors, and title to such Material remains with Intel   **
;**  Corporation or its suppliers or licensors. The Material contains        **
;**  proprietary information of Intel or its suppliers and licensors. The    **
;**  Material is protected by worldwide copyright laws and treaty            **
;**  provisions. No part of the Material may be used, copied, reproduced,    **
;**  modified, published, uploaded, posted, transmitted, distributed or      **
;**  disclosed in any way without Intel's prior express written permission.  **
;**  No license under any patent, copyright or other intellectual property   **
;**  rights in the Material is granted to or conferred upon you, either      **
;**  expressly, by implication, inducement, estoppel or otherwise. Any       **
;**  license under such intellectual property rights must be express and     **
;**  approved by Intel in writing.                                           **
;**                                                                          **
;**  Unless otherwise agreed by Intel in writing, you may not remove or      **
;**  alter this notice or any other notice embedded in Materials by Intel    **
;**  or Intel’s suppliers or licensors in any way.                           **
;******************************************************************************
;
;******************************************************************************

; e1s68x64.INF (Intel 64 bit extension Platform Only,
; Windows 10 64 bit extension)

;
; Intel(R) Gigabit Adapters
;******************************************************************************
;

[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Intel%
CatalogFile = e1s68x64.cat
DriverVer = 11/19/2020,12.15.184.4

[Manufacturer]
%Intel%     = Intel, NTamd64.10.0, NTamd64.10.0.1

[ControlFlags]
ExcludeFromSelect = * 

[Intel]

[Intel.NTamd64.10.0.1]
; DisplayName                   Section                DeviceID
; -----------                   -------                --------
%E1F40NC.DeviceDesc%            = E1F40.10.0.1,         PCI\VEN_8086&DEV_1F40 
%E1F41NC.DeviceDesc%            = E1F41.10.0.1,         PCI\VEN_8086&DEV_1F41 
%E1F45NC.DeviceDesc%            = E1F40.10.0.1,         PCI\VEN_8086&DEV_1F45 

[Intel.NTamd64.10.0]
; DisplayName                   Section                DeviceID
; -----------                   -------                --------
%E1F40NC.DeviceDesc%            = E1F40,               PCI\VEN_8086&DEV_1F40 
%E1F41NC.DeviceDesc%            = E1F41,               PCI\VEN_8086&DEV_1F41 
%E1F45NC.DeviceDesc%            = E1F40,               PCI\VEN_8086&DEV_1F45 

;===============================================================================
;

;              WINDOWS 10 for 64-bit EXTENDED PLATFORMS

;
;===============================================================================

;------------------------------------------------------------------------------
; Intel(R) Ethernet Connection I354 1.0/2.5 GbE Backplane
;------------------------------------------------------------------------------
[E1F40.10.0.1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1s.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = LLI.reg
AddReg             = RSS.reg, RSS8Q.reg
AddReg             = DMACoalescing.reg
AddReg             = ProtocolOffload.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKSQuadLOM.reg
CopyFiles          = win10.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1F40.10.0.1.Services]
AddService = e1sexpress, 2, win10.Service, win10.EventLog

[E1F40.10.0.1.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired
AddReg             = MSIX10.reg

;------------------------------------------------------------------------------
; Intel(R) Ethernet Connection I354
;------------------------------------------------------------------------------
[E1F41.10.0.1]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1s.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Copper.reg, Copper1000.reg
AddReg             = EEE.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = LLI.reg
AddReg             = RSS.reg, RSS8Q.reg
AddReg             = DMACoalescing.reg
AddReg             = ProtocolOffload.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKSQuadLOM.reg
CopyFiles          = win10.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1F41.10.0.1.Services]
AddService = e1sexpress, 2, win10.Service, win10.EventLog

[E1F41.10.0.1.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired
AddReg             = MSIX10.reg

;===============================================================================
;

;
;===============================================================================

;-------------------------------------------------------------------------------
; Intel(R) Ethernet Connection I354 1.0/2.5 GbE Backplane
;-------------------------------------------------------------------------------
[E1F40]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1s.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = LLI.reg, VMQ.reg, VlanId.reg
AddReg             = RSS.reg, RSS8Q.reg, RSSAdvanced.reg
AddReg             = DMACoalescing.reg
AddReg             = ProtocolOffload.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKSQuadLOM.reg
CopyFiles          = win10.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1F40.Services]
AddService = e1sexpress, 2, win10.Service, win10.EventLog

[E1F40.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired
AddReg             = MSIX10.reg

;-------------------------------------------------------------------------------
; Intel(R) Ethernet Connection I354
;-------------------------------------------------------------------------------
[E1F41]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1s.reg, TcpSeg.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Copper.reg, Copper1000.reg
AddReg             = EEE.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = LLI.reg, VMQ.reg, VlanId.reg
AddReg             = RSS.reg, RSS8Q.reg, RSSAdvanced.reg
AddReg             = DMACoalescing.reg
AddReg             = ProtocolOffload.reg
AddReg             = UninstallW2.reg
AddReg             = CoInKSQuadLOM.reg
CopyFiles          = win10.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1F41.Services]
AddService = e1sexpress, 2, win10.Service, win10.EventLog

[E1F41.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired
AddReg             = MSIX10.reg

;-------------------------------------------------------------------------------
; Do-nothing section used to avoid "Unknown hardware" installation prompts.
;
[NO_DRV]
Characteristics    = 0x01
Include            = machine.inf
Needs              = NO_DRV

[NO_DRV.Services]
Include            = machine.inf
Needs              = NO_DRV.Services

;-------------------------------------------------------------------------------
; Registry Settings (decimal)
;
[e1s.reg]
HKR, Ndi\Interfaces,                                    UpperRange,             0, "ndis5"
HKR, Ndi\Interfaces,                                    LowerRange,             0, "ethernet"
HKR, Ndi,                                               Service,                0, "e1sexpress"
HKR, Ndi\Params\*FlowControl,                           ParamDesc,              0, %FlowControl%
HKR, Ndi\Params\*FlowControl,                           default,                0, "3"
HKR, Ndi\Params\*FlowControl\Enum,                      "0",                    0, %Disabled%
HKR, Ndi\Params\*FlowControl\Enum,                      "1",                    0, %FlowControl_TxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "2",                    0, %FlowControl_RxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "3",                    0, %FlowControl_Full%
HKR, Ndi\Params\*FlowControl,                           type,                   0, "enum"

; *TransmitBuffers
HKR, Ndi\params\*TransmitBuffers,                       ParamDesc,              0, %TransmitBuffers%
HKR, Ndi\params\*TransmitBuffers,                       default,                0, "512"
HKR, Ndi\params\*TransmitBuffers,                       min,                    0, "80"
HKR, Ndi\params\*TransmitBuffers,                       max,                    0, "2048"
HKR, Ndi\params\*TransmitBuffers,                       step,                   0, "8"
HKR, Ndi\params\*TransmitBuffers,                       Base,                   0, "10"
HKR, Ndi\params\*TransmitBuffers,                       type,                   0, "int"

; *ReceiveBuffers
HKR, Ndi\params\*ReceiveBuffers,                        ParamDesc,              0, %ReceiveBuffers%
HKR, Ndi\params\*ReceiveBuffers,                        default,                0, "256"
HKR, Ndi\params\*ReceiveBuffers,                        min,                    0, "80"
HKR, Ndi\params\*ReceiveBuffers,                        max,                    0, "2048"
HKR, Ndi\params\*ReceiveBuffers,                        step,                   0, "8"
HKR, Ndi\params\*ReceiveBuffers,                        Base,                   0, "10"
HKR, Ndi\params\*ReceiveBuffers,                        type,                   0, "int"

; *TCPChecksumOffloadIPv4
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                ParamDesc,              0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                type,                   0, "enum"

; *TCPChecksumOffloadIPv6
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                ParamDesc,              0, %TCPChksumOffv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                default,                0, "3"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,                type,                   0, "enum"

; *UDPChecksumOffloadIPv4
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                ParamDesc,              0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                type,                   0, "enum"

; *UDPChecksumOffloadIPv6
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                ParamDesc,              0, %UDPChksumOffv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                default,                0, "3"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,                type,                   0, "enum"

; *IPChecksumOffloadIPv4
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 ParamDesc,              0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 default,                0, "3"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "0",                    0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 type,                   0, "enum"

; Network Address
HKR, Ndi\params\NetworkAddress,                         ParamDesc,              0, %LAA%
HKR, Ndi\params\NetworkAddress,                         Default,                0, ""
HKR, Ndi\params\NetworkAddress,                         type,                   0, "edit"
HKR, NDI\params\NetworkAddress,                         LimitText,              0, "12"
HKR, NDI\params\NetworkAddress,                         UpperCase,              0, "1"
HKR, NDI\params\NetworkAddress,                         optional,               0, "1"

;Log Link State Event
HKR,Ndi\Params\LogLinkStateEvent,                       ParamDesc,              0, %LogLinkState%
HKR,Ndi\Params\LogLinkStateEvent,                       Type,                   0, "enum"
HKR,Ndi\Params\LogLinkStateEvent,                       Default,                0, "51"
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "51",                   0, %Enabled%
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "16",                   0, %Disabled%
HKR,,                                                   LogLinkStateEvent,      0, "51"

; Wait for Link
HKR, Ndi\Params\WaitAutoNegComplete,                    ParamDesc,              0, %WaitAutoNegComplete%
HKR, Ndi\Params\WaitAutoNegComplete,                    default,                0, "2"
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "0",                    0, %Off%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "1",                    0, %On%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "2",                    0, %AutoDetect%
HKR, Ndi\Params\WaitAutoNegComplete,                    type,                   0, "enum"

;  Interrupt Throttle Rate
HKR, Ndi\Params\ITR,                                    ParamDesc,              0, %InterruptThrottleRate%
HKR, Ndi\Params\ITR,                                    default,                0, "65535"
HKR, Ndi\Params\ITR\Enum,                               "65535",                0, %Adaptive%
HKR, Ndi\Params\ITR\Enum,                               "3600",                 0, %Extreme%
HKR, Ndi\Params\ITR\Enum,                               "2000",                 0, %High%
HKR, Ndi\Params\ITR\Enum,                               "950",                  0, %Medium%
HKR, Ndi\Params\ITR\Enum,                               "400",                  0, %Low%
HKR, Ndi\Params\ITR\Enum,                               "200",                  0, %Minimal%
HKR, Ndi\Params\ITR\Enum,                               "0",                    0, %Off%
HKR, Ndi\Params\ITR,                                    type,                   0, "enum"
HKR,,                                                   ITR,                    0, "65535"

; *InterruptModeration
HKR, Ndi\Params\*InterruptModeration,                   ParamDesc,              0, %InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,                   default,                0, "1"
HKR, Ndi\Params\*InterruptModeration\Enum,              "0",                    0, %Disabled%
HKR, Ndi\Params\*InterruptModeration\Enum,              "1",                    0, %Enabled%
HKR, Ndi\Params\*InterruptModeration,                   type,                   0, "enum"

; *PriorityVLANTag
HKR, Ndi\Params\*PriorityVLANTag,                       ParamDesc,              0, %PriorityVLANTag2%
HKR, Ndi\Params\*PriorityVLANTag,                       default,                0, "3"
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "0",                    0, %PriorityVlanDisabled2%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "1",                    0, %PriorityEnabled2%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "2",                    0, %VlanEnabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "3",                    0, %PriorityVlanEnabled2%
HKR, Ndi\Params\*PriorityVLANTag,                       type,                   0, "enum"

; EnablePME
HKR,Ndi\Params\EnablePME,                               ParamDesc,              0, %Enable_PME%
HKR,Ndi\Params\EnablePME,                               Type,                   0, "enum"
HKR,Ndi\Params\EnablePME,                               Default,                0, "0"
HKR,Ndi\Params\EnablePME\Enum,                          "1",                    0, %Enabled%
HKR,Ndi\Params\EnablePME\Enum,                          "0",                    0, %Disabled%

; Hardwired defaults
HKR,,                                                   PciScanMethod,          0, "3"
HKR,,                                                   TxIntDelay,             0, "28"
HKR,,                                                   MulticastFilterType,    0, "0"
HKR,,                                                   VlanFiltering,          0, "0"
HKR,,                                                   UniversalInstall,       0x00010001, 1

; Advanced Power Consumption Features

[TcpSeg.reg]
; *LsoV2IPv4 / *LsoV2IPv6
HKR, Ndi\Params\*LsoV2IPv4,                             ParamDesc,              0, %LsoV2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,                             default,                0, "1"
HKR, Ndi\Params\*LsoV2IPv4\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\*LsoV2IPv4\Enum,                        "1",                    0, %Enabled%
HKR, Ndi\Params\*LsoV2IPv4,                             type,                   0, "enum"
HKR, Ndi\Params\*LsoV2IPv6,                             ParamDesc,              0, %LsoV2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,                             default,                0, "1"
HKR, Ndi\Params\*LsoV2IPv6\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\*LsoV2IPv6\Enum,                        "1",                    0, %Enabled%
HKR, Ndi\Params\*LsoV2IPv6,                             type,                   0, "enum"
HKR,,                                                   *LsoV1IPv4,             0, "0"

[Copper.reg]
HKR, Ndi\params\*SpeedDuplex,                           ParamDesc,              0, %SpeedDuplex%
HKR, Ndi\params\*SpeedDuplex,                           default,                0, "0"
HKR, Ndi\params\*SpeedDuplex,                           type,                   0, "enum"
HKR, Ndi\params\*SpeedDuplex\enum,                      "0",                    0, %AutoNegotiation%
HKR, Ndi\params\*SpeedDuplex\enum,                      "1",                    0, %10Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "2",                    0, %10Mb_Full_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "3",                    0, %100Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "4",                    0, %100Mb_Full_Duplex%
HKR, PROSetNdi\NdiExt\Params\*SpeedDuplex,              ExposeLevel,            0, "3"

[Copper1000.reg]
HKR, Ndi\params\*SpeedDuplex\enum,                      "6",                    0, %1000Mb_Full_Duplex%
; Gigabit Master Slave Mode
HKR,Ndi\Params\MasterSlave,                             ParamDesc,              0, %MasterSlaveMode%
HKR,Ndi\Params\MasterSlave,                             Type,                   0, "enum"
HKR,Ndi\Params\MasterSlave,                             Default,                0, "0"
HKR,Ndi\Params\MasterSlave\Enum,                        "0",                    0, %AutoDetect%
HKR,Ndi\Params\MasterSlave\Enum,                        "1",                    0, %GigabitMasterMode%
HKR,Ndi\Params\MasterSlave\Enum,                        "2",                    0, %GigabitSlaveMode%

;-------------------------------------------------------------------------------
; Packet specifics
;

; *JumboPacket
[JumboPacket.reg]
HKR, Ndi\Params\*JumboPacket,                           ParamDesc,              0, %JumboPacket%
HKR, Ndi\Params\*JumboPacket,                           default,                0, "1514"
HKR, Ndi\Params\*JumboPacket\Enum,                      "1514",                 0, %Disabled%
HKR, Ndi\Params\*JumboPacket\Enum,                      "4088",                 0, %Bytes4088%
HKR, Ndi\Params\*JumboPacket\Enum,                      "9014",                 0, %Bytes9014%
HKR, Ndi\Params\*JumboPacket,                           type,                   0, "enum"

[Powermgmt.reg]
HKR, Ndi\Params\*WakeOnPattern,                         ParamDesc,              0, %WakeOnPattern%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "0",                    0, %Disabled%
HKR, Ndi\Params\*WakeOnPattern\Enum,                    "1",                    0, %Enabled%
HKR, Ndi\Params\*WakeOnPattern,                         type,                   0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                         default,                0, "1"
HKR, Ndi\Params\*WakeOnMagicPacket,                     ParamDesc,              0, %WakeOnMagicPacket%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "0",                    0, %Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,                "1",                    0, %Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket,                     type,                   0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,                     default,                0, "1"

[EEE.reg]
HKR, Ndi\Params\EEELinkAdvertisement,                   ParamDesc,              0, %EEELinkAdvertisement%
HKR, Ndi\Params\EEELinkAdvertisement\Enum,              "0",                    0, %EEE_Disabled%
HKR, Ndi\Params\EEELinkAdvertisement\Enum,              "1",                    0, %EEE_Enabled_AWAKE%
HKR, Ndi\Params\EEELinkAdvertisement,                   type,                   0, "enum"
HKR, Ndi\Params\EEELinkAdvertisement,                   default,                0, "1"

[DMACoalescing.reg]
HKR, Ndi\Params\DMACoalescing,                          ParamDesc,              0, %EnableDMACoalescing%
HKR, Ndi\Params\DMACoalescing\Enum,                     "0",                    0, %Disabled%
HKR, Ndi\Params\DMACoalescing\Enum,                     "250",                  0, %250usec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "500",                  0, %500usec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "1000",                 0, %1msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "2000",                 0, %2msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "3000",                 0, %3msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "4000",                 0, %4msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "5000",                 0, %5msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "6000",                 0, %6msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "7000",                 0, %7msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "8000",                 0, %8msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "9000",                 0, %9msec%
HKR, Ndi\Params\DMACoalescing\Enum,                     "10000",                0, %10msec%
HKR, Ndi\Params\DMACoalescing,                          type,                   0, "enum"
HKR, Ndi\Params\DMACoalescing,                          default,                0, "0"

[ProtocolOffload.reg]
HKR, Ndi\Params\*PMARPOffload,                          ParamDesc,              0, %ARPOffload%
HKR, Ndi\Params\*PMARPOffload\Enum,                     "0",                    0, %Disabled%
HKR, Ndi\Params\*PMARPOffload\Enum,                     "1",                    0, %Enabled%
HKR, Ndi\Params\*PMARPOffload,                          type,                   0, "enum"
HKR, Ndi\Params\*PMARPOffload,                          default,                0, "1"
HKR, Ndi\Params\*PMNSOffload,                           ParamDesc,              0, %NSOffload%
HKR, Ndi\Params\*PMNSOffload\Enum,                      "0",                    0, %Disabled%
HKR, Ndi\Params\*PMNSOffload\Enum,                      "1",                    0, %Enabled%
HKR, Ndi\Params\*PMNSOffload,                           type,                   0, "enum"
HKR, Ndi\Params\*PMNSOffload,                           default,                0, "1"

[WakeOnLink.reg]
HKR, Ndi\Params\WakeOnLink,                             ParamDesc,              0, %WakeOnLinkSettings%
HKR, Ndi\Params\WakeOnLink\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\WakeOnLink\Enum,                        "2",                    0, %Forced%
HKR, Ndi\Params\WakeOnLink,                             type,                   0, "enum"
HKR, Ndi\Params\WakeOnLink,                             default,                0, "0"

[VMQ.reg]
; *VMQ
HKR, Ndi\Params\*VMQ,                                   ParamDesc,              0, %VMQ%
HKR, Ndi\Params\*VMQ,                                   default,                0, "1"
HKR, Ndi\Params\*VMQ,                                   type,                   0, "enum"
HKR, Ndi\Params\*VMQ\Enum,                              "0",                    0, %Disabled%
HKR, Ndi\Params\*VMQ\Enum,                              "1",                    0, %Enabled%
HKR,,                                                   VMQSupported,           0, "1"

[RSS.reg]
; *RSS
HKR, Ndi\Params\*RSS,                                   ParamDesc,              0, %RSS%
HKR, Ndi\Params\*RSS,                                   default,                0, "1"
HKR, Ndi\Params\*RSS,                                   type,                   0, "enum"
HKR, Ndi\Params\*RSS\Enum,                              "0",                    0, %Disabled%
HKR, Ndi\Params\*RSS\Enum,                              "1",                    0, %Enabled%

[RSSAdvanced.reg]
; *MaxRssProcessors
HKR, Ndi\Params\*MaxRssProcessors,                      ParamDesc,              0, %MaxRssProcessors%
HKR, Ndi\Params\*MaxRssProcessors,                      default,                0, "8"
HKR, Ndi\Params\*MaxRssProcessors,                      type,                   0, "enum"
HKR, Ndi\Params\*MaxRssProcessors\Enum,                 "1",                    0, "1"
HKR, Ndi\Params\*MaxRssProcessors\Enum,                 "2",                    0, "2"
HKR, Ndi\Params\*MaxRssProcessors\Enum,                 "4",                    0, "4"
HKR, Ndi\Params\*MaxRssProcessors\Enum,                 "8",                    0, "8"

; *RssBaseProcNumber
HKR, Ndi\params\*RssBaseProcNumber,                     ParamDesc,              0, %RssBaseProcNumber%
HKR, Ndi\params\*RssBaseProcNumber,                     default,                0, "0"
HKR, Ndi\params\*RssBaseProcNumber,                     min,                    0, "0"
HKR, Ndi\params\*RssBaseProcNumber,                     max,                    0, "63"
HKR, Ndi\params\*RssBaseProcNumber,                     step,                   0, "1"
HKR, Ndi\params\*RssBaseProcNumber,                     Optional,               0, "0"
HKR, Ndi\params\*RssBaseProcNumber,                     type,                   0, "int"

; *NumaNodeId
HKR, Ndi\params\*NumaNodeId,                            ParamDesc,              0, %NumaNodeId%
HKR, Ndi\params\*NumaNodeId,                            default,                0, "65535"
HKR, Ndi\params\*NumaNodeId,                            type,                   0, "dword"
HKR, Ndi\params\*NumaNodeId,                            min,                    0, "0"
HKR, Ndi\params\*NumaNodeId,                            max,                    0, "65535"
HKR, Ndi\params\*NumaNodeId,                            step,                   0, "1"

; *RSSProfile
HKR, Ndi\Params\*RSSProfile,                            ParamDesc,              0, %RSSProfile%
HKR, Ndi\Params\*RSSProfile,                            default,                0, "1"
HKR, Ndi\Params\*RSSProfile,                            type,                   0, "enum"
HKR, Ndi\Params\*RSSProfile\Enum,                       "1",                    0, %Closest_Processor%
HKR, Ndi\Params\*RSSProfile\Enum,                       "2",                    0, %Closest_Processor_Static%
HKR, Ndi\Params\*RSSProfile\Enum,                       "3",                    0, %NUMA_Scaling%
HKR, Ndi\Params\*RSSProfile\Enum,                       "4",                    0, %NUMA_Scaling_Static%
HKR, Ndi\Params\*RSSProfile\Enum,                       "5",                    0, %Conservative_Scaling%
HKR,,                                                   *RSSProfile,            0, "1"

[RSS8Q.reg]
; NumRssQueues
HKR, Ndi\Params\*NumRssQueues,                           ParamDesc,              0, %NumRssQueues2%
HKR, Ndi\Params\*NumRssQueues,                           default,                0, "2"
HKR, Ndi\Params\*NumRssQueues,                           type,                   0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,                      "1",                    0, %1queue%
HKR, Ndi\Params\*NumRssQueues\Enum,                      "2",                    0, %2queues%
HKR, Ndi\Params\*NumRssQueues\Enum,                      "4",                    0, %4queues%
HKR, Ndi\Params\*NumRssQueues\Enum,                      "8",                    0, %8queues%

[LLI.reg]
HKR, PROSetNdi\Params\EnableLLI,                        ParamDesc,              0, %EnableLLI%
HKR, PROSetNdi\Params\EnableLLI,                        default,                0, "0"
HKR, PROSetNdi\Params\EnableLLI,                        type,                   0, "enum"
HKR, PROSetNdi\Params\EnableLLI\Enum,                   "0",                    0, %Disabled%
HKR, PROSetNdi\Params\EnableLLI\Enum,                   "1",                    0, %LLIPortBased%
HKR, PROSetNdi\Params\EnableLLI\Enum,                   "2",                    0, %LLIPSHBased%
HKR,,                                                   EnableLLI,              2, "0"
HKR, PROSetNdi\Params\LLIPorts,                         ParamDesc,              0, %LLIPorts%
HKR, PROSetNdi\Params\LLIPorts,                         default,                0, ""
HKR, PROSetNdi\Params\LLIPorts,                         type,                   0, "edit"
HKR, PROSetNdi\Params\LLIPorts,                         UpperCase,              0, "1"
HKR, PROSetNdi\Params\LLIPorts,                         optional,               0, "1"
HKR, PROSetNdi\Params\LLIPorts,                         multi_string,           0, "1"
HKR,,                                                   LLIPorts,               0x00010002, ""

;-------------------------------------------------------------------------------
[WakeOnSlot.reg]
HKR,,                                                   WakeOnSlot,             0, 0

[VlanId.reg]
; VlanId
HKR, Ndi\params\VlanId,                                 ParamDesc,              0, %VlanID%
HKR, Ndi\params\VlanId,                                 default,                0, "0"
HKR, Ndi\params\VlanId,                                 type,                   0, "DWORD"
HKR, Ndi\params\VlanId,                                 min,                    0, "0"
HKR, Ndi\params\VlanId,                                 max,                    0, "4094"
HKR, Ndi\params\VlanId,                                 step,                   0, "1"
HKR, Ndi\params\VlanId,                                 base,                   0, "10"

[MSIX10.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 10

[EnableWakeOnManagmentOnTCO.reg]
HKR,,                                                   EnableWakeOnManagmentOnTCO, 0, "0"

;-------------------------------------------------------------------------------
; Uninstallation

[UninstallW2.reg]
HKR,Prounstl\SupportedDevices\8086, 1F40, 0, "1F40"
HKR,Prounstl\SupportedDevices\8086, 1F41, 0, "1F41"
HKR,Prounstl\SupportedDevices\8086, 1F45, 0, "1F45"
HKR,Prounstl\Dins, e1s68x64.din, 0, "8254x.Uninstall"
HKR,Prounstl\Services, e1sexpress, 0, "e1s68x64.sys"

[UninstallProg.CopyFiles]
e1s68x64.din,,,2

;-------------------------------------------------------------------------------
; WinVista copy files
;
[win10.CopyFiles]
e1s68x64.sys,,,2
e1smsg.dll

[win10.Service]
DisplayName     = %E1SExpress.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e1s68x64.sys
LoadOrderGroup  = NDIS
AddReg             = Service_AddReg

[Service_AddReg]
HKR,, BootFlags, 0x00010001, 0x1

;-------------------------------------------------------------------------------
; Common base for all drivers for Eventlog and TextModeFlags
;

[win10.EventLog]
AddReg             = win10.AddEventLog.reg

[win10.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %EventLogMessageDllPath%
HKR, , TypesSupported,   0x00010001, 7

[CoInKSQuadLOM.reg]
HKR,,                                          CoInstallFlag,      0x00010001, 0x80281051

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir                = 11
win10.CopyFiles          = 12
UninstallProg.CopyFiles          = 11

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>,subdir]]
;
1 = %DISKNAME%,,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
e1s68x64.din = 1,,
e1smsg.dll = 1,,
e1s68x64.sys = 1,, ; on distribution disk 1

;-------------------------------------------------------------------------------
; Legacy
[Advanced.DelReg]
HKR, Ndi\Params
HKR, PROSetNdi\Params
HKR, PROSetNdi\NdiExt
HKR,, LinkNegotiationProcess

;-----------------------------------------------------------------------------
; Localizable Strings

[Strings]
AutoDetect                      = "Auto Detect"
AutoNegotiation                 = "Auto Negotiation"
SpeedDuplex                     = "Speed & Duplex"
10Mb_Half_Duplex                = "10 Mbps Half Duplex"
10Mb_Full_Duplex                = "10 Mbps Full Duplex"
100Mb_Half_Duplex               = "100 Mbps Half Duplex"
100Mb_Full_Duplex               = "100 Mbps Full Duplex"
1000Mb_Full_Duplex              = "1.0 Gbps Full Duplex"
IPChksumOffv4                   = "IPv4 Checksum Offload"
TCPChksumOffv4                  = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4                  = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6                  = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6                  = "UDP Checksum Offload (IPv6)"
LsoV2IPv4                       = "Large Send Offload V2 (IPv4)"
LsoV2IPv6                       = "Large Send Offload V2 (IPv6)"
ChksumOffTxRx                   = "Rx & Tx Enabled"
ChksumOffTx                     = "Tx Enabled"
ChksumOffRx                     = "Rx Enabled"
FlowControl                     = "Flow Control"
FlowControl_TxOnly              = "Tx Enabled"
FlowControl_RxOnly              = "Rx Enabled"
FlowControl_Full                = "Rx & Tx Enabled"
PriorityVlanDisabled2           = "Packet Priority & VLAN Disabled"
PriorityEnabled2                = "Packet Priority Enabled"
VlanEnabled                     = "VLAN Enabled"
PriorityVlanEnabled2            = "Packet Priority & VLAN Enabled"
TransmitBuffers                 = "Transmit Buffers"
ReceiveBuffers                  = "Receive Buffers"
PriorityVLANTag2                = "Packet Priority & VLAN"
VMQ                             = "Virtual Machine Queues"
RSS                             = "Receive Side Scaling"
NumRssQueues2                   = "Maximum Number of RSS Queues"
RSSProfile                      = "RSS load balancing profile"
Closest_Processor               = "ClosestProcessor"
Closest_Processor_Static        = "ClosestProcessorStatic"
NUMA_Scaling                    = "NUMAScaling"
NUMA_Scaling_Static             = "NUMAScalingStatic"
Conservative_Scaling            = "ConservativeScaling"
RssBaseProcNumber               = "RSS Base Processor Number"
NumaNodeId                      = "Preferred NUMA node"
MaxRssProcessors                = "Maximum number of RSS Processors"
1queue                          = "1 Queue"
2queues                         = "2 Queues"
4queues                         = "4 Queues"
8queues                         = "8 Queues"
On                              = "On"
Off                             = "Off"
Enabled                         = "Enabled"
Disabled                        = "Disabled"
Bytes4088                       = "4088 Bytes"
Bytes9014                       = "9014 Bytes"
LAA                             = "Locally Administered Address"
JumboPacket                     = "Jumbo Packet"
WakeOnMagicPacket               = "Wake on Magic Packet"
Enable_PME                      = "Enable PME"
Forced                          = "Forced"
WakeOnLinkSettings              = "Wake on Link Settings"
WakeOnPattern                   = "Wake on Pattern Match"
LogLinkState                    = "Log Link State Event"
InterruptModeration             = "Interrupt Moderation"
InterruptThrottleRate           = "Interrupt Moderation Rate"
Adaptive                        = "Adaptive"
Extreme                         = "Extreme"
Minimal                         = "Minimal"
High                            = "High"
Medium                          = "Medium"
Low                             = "Low"
GigabitMasterMode               = "Force Master Mode"
GigabitSlaveMode                = "Force Slave Mode"
MasterSlaveMode                 = "Gigabit Master Slave Mode"
WaitAutoNegComplete             = "Wait for Link"
EnableLLI                       = "Low Latency Interrupts"
LLIPorts                        = "Low Latency Interrupt Ports"
LLIPortBased                    = "Port-Based"
LLIPSHBased                     = "PSH Flag-Based"
EEELinkAdvertisement            = "Energy Efficient Ethernet"
EEE_Disabled                    = "Off"
EEE_Enabled_AWAKE               = "On if system is awake"
EnableDMACoalescing             = "DMA Coalescing"
250usec                         = "250 usec"
500usec                         = "500 usec"
1msec                           = "1 msec"
2msec                           = "2 msec"
3msec                           = "3 msec"
4msec                           = "4 msec"
5msec                           = "5 msec"
6msec                           = "6 msec"
7msec                           = "7 msec"
8msec                           = "8 msec"
9msec                           = "9 msec"
10msec                          = "10 msec"
ARPOffload                      = "ARP Offload"
NSOffload                       = "NS Offload"
VlanID                          = "VLAN ID"
Intel                           = "Intel"
EventLogMessageDllPath          = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\drivers\e1s68x64.sys"
E1SExpress.Service.DispName     = "Intel(R) PCI Express Network Connection Driver S"
DISKNAME                        = "Intel(R) Driver Disk"

;; Brandnames.str
;------------------------------------------------------------------------------
E1F40NC.DeviceDesc              = "Intel(R) Ethernet Connection I354 1.0 GbE Backplane"
E1F41NC.DeviceDesc              = "Intel(R) Ethernet Connection I354"
E1F45NC.DeviceDesc              = "Intel(R) Ethernet Connection I354 2.5 GbE Backplane"

;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------

